gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 4-28-2016  18:02:17
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Mar  1 2016 15:13:08) (MSVC)
                                           ; This file was generated Thu Apr 28 16:19:21 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.radix dec
                                           	.include "KF8S1022.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1022 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2                .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           T2CCR             .EQU                0x54
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P12               .EQU                2
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x12 T2CTL Bits----------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT1SE             .EQU                6
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS6               .EQU                6
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           _ANS6              .EQU                6
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x4c0
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern STK12
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Mar  1 2016 15:13:08) (MSVC)
                                           ; This file was generated Thu Apr 28 16:19:21 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../debug_touch.c"
                                           	.radix dec
                                           	.include "KF8S1022.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1022 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2                .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           T2CCR             .EQU                0x54
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P12               .EQU                2
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x12 T2CTL Bits----------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT1SE             .EQU                6
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS6               .EQU                6
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           _ANS6              .EQU                6
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_init_mcu
                                           	.extern	__KF8S_Get_Ver_General_
                                           	.extern	__KF8S_Lib_Set_General_Parameter
                                           	.extern	__KF8S_Init_Touch_General_
                                           	.extern	__KF8S_Touch_Process_General_
                                           	.extern	__KF8S_Touch_TEST_General_
                                           	.extern	_delay_ms
                                           	.extern	_delay_us
                                           	.extern	__R2PCL
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CMCTL1_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_T3L_bits
                                           	.extern	_CTCTL_bits
                                           	.extern	_OSCLDOCAL_bits
                                           	.extern	__KF8_LIBi_channel_flag_
                                           	.extern	__KF8_LIBc_channel_
                                           	.extern	__KF8_LIBc_channel_Buf
                                           	.extern	__KF8_LIBi_Date_Change_
                                           	.extern	__KF8_LIBc_baseline_count_
                                           	.extern	__KF8_LIBi_buff_hit_
                                           	.extern	__KF8_LIBi_buff_baseline_
                                           	.extern	__KF8_LIBc_touch_count_
                                           	.extern	_CHS_AMOUNT
                                           	.extern	_TCS_AMOUNT
                                           	.extern	__KF8_Disturb_Protect_Circle_
                                           	.extern	__KF8_DoubleKey_Compages_Limitable_Circle_
                                           	.extern	__KF8_Key_Max_Pressed_Limitable_Circle_
                                           	.extern	__KF8_BaseLine_Update_Circle_Count_For_UP_
                                           	.extern	__KF8_BaseLine_Update_Circle_Count_For_Down_
                                           	.extern	__KF8_Define_Disturb_Channels_Amount_
                                           	.extern	__KF8_BasicLine_UP_Noise_Threshold_
                                           	.extern	__KF8_BasicLine_Down_Noise_Threshold_
                                           	.extern	__KF8_Data_Steady_Threshold_Set_
                                           	.extern	__KF8_Inside_Reference_Channel_Disturb_Threshold_Set_
                                           	.extern	__KF8_Inside_Reference_Channel_Declare_
                                           	.extern	__KF8_Config_Finger_Threshold
                                           	.extern	__KF8_TOUCH_CH_EN
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2
                                           	.extern	_T2CTL
                                           	.extern	_PWMCTL
                                           	.extern	_CMCTL1
                                           	.extern	_VRECAL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_OPTR
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_TR3
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T3L
                                           	.extern	_CTCTL
                                           	.extern	_T2CCR
                                           	.extern	_OSCLDOCAL
                                           	.extern	_T1U
                                           
                                           	.extern STK12
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_TOUCH_DEBUG_SEND_OUT
                                           	.global	_TOUCH_DEBUG_TRS_DEAL
                                           	.global	_TOUCH_CH_TRS_EN
                                           	.global	_T_buf
                                           	.global	_i_T_D
                                           	.global	_sentbuf1
                                           	.global	_sentbuf2
                                           	.global	_sentbuf3
                                           	.global	_sentbuf4
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_debug_touch_0	.udata
                                           _T_buf	.res	1
                                           
                                           UD_debug_touch_1	.udata
                                           _i_T_D	.res	1
                                           
                                           UD_debug_touch_2	.udata
                                           _sentbuf1	.res	1
                                           
                                           UD_debug_touch_3	.udata
                                           _sentbuf2	.res	1
                                           
                                           UD_debug_touch_4	.udata
                                           _sentbuf3	.res	1
                                           
                                           UD_debug_touch_5	.udata
                                           _sentbuf4	.res	1
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_debug_touch_0	.udata
                                           r0x1008	.res	1
                                           UDL_debug_touch_1	.udata
                                           r0x1009	.res	1
                                           UDL_debug_touch_2	.udata
                                           r0x1006	.res	1
                                           UDL_debug_touch_3	.udata
                                           r0x1007	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           
                                           ID_debug_touch_0	.idata
                                           _TOUCH_CH_TRS_EN
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           	.db	0x00
                                           
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           
                                           func._TOUCH_DEBUG_SEND_OUT	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _TOUCH_DEBUG_SEND_OUT	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;3 compiler assigned registers:
                                           ;   STK00
                                           ;   r0x1006
                                           ;   r0x1007
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _TOUCH_DEBUG_SEND_OUT	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	322; "../debug_touch.c"	CLK_SET_IN;
                                           	SET	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	323; "../debug_touch.c"	DAT_SET_IN;
                                           	SET	_TR0_bits, 0
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	324; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	328; "../debug_touch.c"	if(CLK_GET_STATE)
                                           	JB	_P0_bits, 1
                                           	JMP	_00078_DS_
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	330; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	331; "../debug_touch.c"	if(!CLK_GET_STATE)
                                           	JNB	_P0_bits, 1
                                           	JMP	_00079_DS_
                                           ;	op : RETURN
                                           ;	.line	332; "../debug_touch.c"	return;
                                           	JMP	_00116_DS_
                                           ;	op : LABEL
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           _00078_DS_
                                           ;	.line	334; "../debug_touch.c"	else if(!CLK_GET_STATE)
                                           	JNB	_P0_bits, 1
                                           	JMP	_00075_DS_
                                           ;	op : RETURN
                                           ;	.line	336; "../debug_touch.c"	return;
                                           	JMP	_00116_DS_
                                           ;	op : LABEL
                                           ;	op : RETURN
                                           _00075_DS_
                                           ;	.line	339; "../debug_touch.c"	return;
                                           	JMP	_00116_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00079_DS_
                                           ;	.line	341; "../debug_touch.c"	CLK_SET_OUT;
                                           	CLR	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	343; "../debug_touch.c"	CLK_SET_LOW;
                                           	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	344; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	346; "../debug_touch.c"	CLK_SET_HIGH;		//ÉÏÉýÑØ
                                           	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	348; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           ;	.line	350; "../debug_touch.c"	if(!DAT_GET_STATE)
                                           	PAGESEL	$
                                           ;	.line	352; "../debug_touch.c"	return;
                                           	JB	_P0_bits, 0
                                           ;	.line	355; "../debug_touch.c"	CLK_SET_LOW;			//ÏÂ½µÑØ
                                           	JMP	_00116_DS_
                                           	CLR	_P0_bits, 1
                                           ;	.line	358; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	360; "../debug_touch.c"	DAT_SET_OUT;
                                           	CLR	_TR0_bits, 0
                                           ;	op : =
                                           ;	.line	363; "../debug_touch.c"	j=5;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	365; "../debug_touch.c"	for(step=0;step<5;step++)
                                           	BANKSEL	r0x1007
                                           	CLR	r0x1007
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x5=5), size=1
                                           _00108_DS_
                                           	MOV	R0,# 0x05
                                           	BANKSEL	r0x1007
                                           	SUB	R0, r0x1007
                                           ;comparing bytes at offset 0
                                           	JNB	PSW, 0
                                           	JMP	_00111_DS_
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;unsigned compare: left >= lit(0x5=5), size=1
                                           ;	.line	368; "../debug_touch.c"	switch(step)
                                           	MOV	R0,# 0x05
                                           	BANKSEL	r0x1007
                                           	SUB	R0, r0x1007
                                           ;comparing bytes at offset 0
                                           	JNB	PSW, 0
                                           	JMP	_00087_DS_
                                           ;	op : JUMPTABLE
                                           	MOV	R0,#high _00138_DS_
                                           	MOV	PCH, R0
                                           	MOV	R0,#_00138_DS_
                                           	BANKSEL	r0x1007
                                           	ADD	R0, r0x1007
                                           	JNB	PSW, 0
                                           	INC	PCH
                                           	MOV	PCL, R0
                                           _00138_DS_
                                           	JMP	_00082_DS_
                                           	JMP	_00083_DS_
                                           	JMP	_00084_DS_
                                           	JMP	_00085_DS_
                                           	JMP	_00086_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00082_DS_
                                           ;	.line	372; "../debug_touch.c"	j=5;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	373; "../debug_touch.c"	T_buf=0x04;
                                           	MOV	R0,# 0x04
                                           	BANKSEL	_T_buf
                                           	MOV	_T_buf, R0
                                           ;	op : GOTO
                                           ;	.line	374; "../debug_touch.c"	}break;
                                           	JMP	_00087_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00083_DS_
                                           ;	.line	378; "../debug_touch.c"	j=8;
                                           	MOV	R0,# 0x08
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	380; "../debug_touch.c"	T_buf=sentbuf1;
                                           	BANKSEL	_sentbuf1
                                           	MOVZ	R0, _sentbuf1
                                           	BANKSEL	_T_buf
                                           	MOV	_T_buf, R0
                                           ;	op : GOTO
                                           ;	.line	382; "../debug_touch.c"	}break;
                                           	JMP	_00087_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00084_DS_
                                           ;	.line	386; "../debug_touch.c"	j=8;
                                           	MOV	R0,# 0x08
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	387; "../debug_touch.c"	T_buf=sentbuf2;
                                           	BANKSEL	_sentbuf2
                                           	MOVZ	R0, _sentbuf2
                                           	BANKSEL	_T_buf
                                           	MOV	_T_buf, R0
                                           ;	op : GOTO
                                           ;	.line	389; "../debug_touch.c"	}break;
                                           	JMP	_00087_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00085_DS_
                                           ;	.line	393; "../debug_touch.c"	j=8;
                                           	MOV	R0,# 0x08
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	394; "../debug_touch.c"	T_buf=sentbuf3;
                                           	BANKSEL	_sentbuf3
                                           	MOVZ	R0, _sentbuf3
                                           	BANKSEL	_T_buf
                                           	MOV	_T_buf, R0
                                           ;	op : GOTO
                                           ;	.line	395; "../debug_touch.c"	}break;
                                           	JMP	_00087_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00086_DS_
                                           ;	.line	399; "../debug_touch.c"	j=8;
                                           	MOV	R0,# 0x08
                                           	BANKSEL	r0x1006
                                           	MOV	r0x1006, R0
                                           ;	op : =
                                           ;	.line	400; "../debug_touch.c"	T_buf=sentbuf4;
                                           	BANKSEL	_sentbuf4
                                           	MOVZ	R0, _sentbuf4
                                           	BANKSEL	_T_buf
                                           	MOV	_T_buf, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00087_DS_
                                           ;	.line	404; "../debug_touch.c"	for(i_T_D=0;i_T_D<j;i_T_D++)
                                           	BANKSEL	_i_T_D
                                           	CLR	_i_T_D
                                           ;	op : LABEL
                                           ;	op : <
                                           _00104_DS_
                                           	BANKSEL	r0x1006
                                           	MOVZ	R0, r0x1006
                                           	BANKSEL	_i_T_D
                                           	SUB	R0, _i_T_D
                                           ;comparing bytes at offset 0
                                           	JNB	PSW, 0
                                           	JMP	_00107_DS_
                                           ;	op : BITWISEAND
                                           ;	.line	406; "../debug_touch.c"	if(T_buf&0x01)
                                           	BANKSEL	_T_buf
                                           	JB	_T_buf, 0
                                           	JMP	_00089_DS_
                                           ;	op : =
                                           ;	.line	407; "../debug_touch.c"	DAT_SET_HIGH;
                                           	SET	_P0_bits, 0
                                           ;	op : GOTO
                                           	JMP	_00090_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00089_DS_
                                           ;	.line	409; "../debug_touch.c"	DAT_SET_LOW;
                                           	CLR	_P0_bits, 0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00090_DS_
                                           ;	.line	411; "../debug_touch.c"	CLK_SET_HIGH;
                                           	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	412; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	414; "../debug_touch.c"	CLK_SET_LOW;
                                           	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	415; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : RIGHT_OP
                                           ;	.line	417; "../debug_touch.c"	T_buf=T_buf>>1;
                                           	CLR	PSW, 0
                                           	BANKSEL	_T_buf
                                           	RRC	_T_buf
                                           ;	op : +
                                           ;	.line	404; "../debug_touch.c"	for(i_T_D=0;i_T_D<j;i_T_D++)
                                           	BANKSEL	_i_T_D
                                           	INC	_i_T_D
                                           ;	op : GOTO
                                           	JMP	_00104_DS_
                                           ;	op : LABEL
                                           ;	op : SEND
                                           ;	op : CALL
                                           _00107_DS_
                                           ;	.line	420; "../debug_touch.c"	Touch_Delay2;
                                           	MOV	R0,# 0x6e
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : +
                                           ;	.line	365; "../debug_touch.c"	for(step=0;step<5;step++)
                                           	BANKSEL	r0x1007
                                           	INC	r0x1007
                                           ;	op : GOTO
                                           	JMP	_00108_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00111_DS_
                                           ;	.line	424; "../debug_touch.c"	DAT_SET_IN;
                                           	SET	_TR0_bits, 0
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	425; "../debug_touch.c"	Touch_Delay2;	//±à³ÌÆ÷ÅÐ¶ÏÐèÒªÊ±¼ä
                                           	MOV	R0,# 0x6e
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	427; "../debug_touch.c"	CLK_SET_HIGH;
                                           	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	428; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	429; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	430; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	433; "../debug_touch.c"	if(DAT_GET_STATE)
                                           	JB	_P0_bits, 0
                                           	JMP	_00102_DS_
                                           ;	op : =
                                           ;	.line	435; "../debug_touch.c"	CLK_SET_LOW;
                                           	CLR	_P0_bits, 1
                                           ;	op : =
                                           ;	.line	436; "../debug_touch.c"	T_buf=0;
                                           	BANKSEL	_T_buf
                                           	CLR	_T_buf
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	437; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	438; "../debug_touch.c"	for(i_T_D=0;i_T_D<6;i_T_D++)
                                           	BANKSEL	_i_T_D
                                           	CLR	_i_T_D
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x6=6), size=1
                                           _00112_DS_
                                           	MOV	R0,# 0x06
                                           	BANKSEL	_i_T_D
                                           	SUB	R0, _i_T_D
                                           ;comparing bytes at offset 0
                                           	JNB	PSW, 0
                                           	JMP	_00103_DS_
                                           ;	op : =
                                           ;	.line	440; "../debug_touch.c"	CLK_SET_HIGH;
                                           	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	441; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : EQ_OP
                                           ;	.line	443; "../debug_touch.c"	if(i_T_D!=5)
                                           	BANKSEL	_i_T_D
                                           	MOVZ	R0, _i_T_D
                                           ;	.line	445; "../debug_touch.c"	T_buf=T_buf>>1;
                                           	XOR	R0,# 0x05
                                           	JNB	PSW, 2
                                           	JMP	_00099_DS_
                                           	CLR	PSW, 0
                                           	BANKSEL	_T_buf
                                           	RRC	_T_buf
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	446; "../debug_touch.c"	if(DAT_GET_STATE)
                                           	JB	_P0_bits, 0
                                           	JMP	_00100_DS_
                                           ;	op : |
                                           ;	.line	447; "../debug_touch.c"	T_buf=T_buf|0x10;
                                           	BANKSEL	_T_buf
                                           	SET	_T_buf, 4
                                           ;	op : GOTO
                                           	JMP	_00100_DS_
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00099_DS_
                                           ;	.line	451; "../debug_touch.c"	if(T_buf<16)   //´«Êä´íÎóµÄ£¬·ÀÏÂ·ÇÓ°ÏìÆäËûÊý¾Ý
                                           	MOV	R0,# 0x10
                                           	BANKSEL	_T_buf
                                           	SUB	R0, _T_buf
                                           ;comparing bytes at offset 0
                                           	JNB	PSW, 0
                                           	JMP	_00100_DS_
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	453; "../debug_touch.c"	if(DAT_GET_STATE)
                                           	JB	_P0_bits, 0
                                           	JMP	_00094_DS_
                                           ;	op : INLINEASM
                                           	BANKSEL _T_buf
                                           	MOV R0,_T_buf
                                           	ADD R0,#(_TOUCH_CH_TRS_EN+0)
                                           	MOV R1,#0x01
                                           	BANKSEL _TOUCH_CH_TRS_EN
                                           	ST [R0],R1
                                           	
                                           ;	op : GOTO
                                           	JMP	_00100_DS_
                                           ;	op : LABEL
                                           ;	op : INLINEASM
                                           _00094_DS_
                                           	BANKSEL _T_buf
                                           	MOV R0,_T_buf
                                           	ADD R0,#(_TOUCH_CH_TRS_EN+0)
                                           	MOV R1,#0x00
                                           	BANKSEL _TOUCH_CH_TRS_EN
                                           	ST [R0],R1
                                           	
                                           ;	op : LABEL
                                           ;	op : =
                                           _00100_DS_
                                           ;	.line	479; "../debug_touch.c"	CLK_SET_LOW;
                                           	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	480; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : +
                                           ;	.line	438; "../debug_touch.c"	for(i_T_D=0;i_T_D<6;i_T_D++)
                                           	BANKSEL	_i_T_D
                                           	INC	_i_T_D
                                           ;	op : GOTO
                                           	JMP	_00112_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00102_DS_
                                           ;	.line	485; "../debug_touch.c"	CLK_SET_LOW;
                                           	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	486; "../debug_touch.c"	Touch_Delay1;
                                           	MOV	R0,# 0x05
                                           	BANKSEL	STK00
                                           	MOV	STK00, R0
                                           	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
                                           	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : =
                                           _00103_DS_
                                           ;	.line	489; "../debug_touch.c"	CLK_SET_IN;
                                           	SET	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	490; "../debug_touch.c"	DAT_SET_IN;
                                           	SET	_TR0_bits, 0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00116_DS_
                                           	CRET	
                                           ; exit point of _TOUCH_DEBUG_SEND_OUT
                                           
                                           
                                           
                                           func._TOUCH_DEBUG_TRS_DEAL	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _TOUCH_DEBUG_TRS_DEAL	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;   _delay_us
                                           ;3 compiler assigned registers:
                                           ;   STK00
                                           ;   r0x1008
                                           ;   r0x1009
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _TOUCH_DEBUG_TRS_DEAL	;Function start
                                           ; 2 exit points
                                           ;	op : INLINEASM
0003bc   9906     MOV	R1, #0x6             	MOV R1,#High(__KF8_TOUCH_CH_EN+0)
0003bd   9800     MOV	R0, #0               	MOV R0,#(0)
0003be   80ae     ADD	R0, #0xae            	ADD R0,#Low(__KF8_TOUCH_CH_EN+0)
0003bf   7003     JNB	0x3, 0               	JNB PSW,0
0003c0   ff11     INC	R1                   	INC R1
                                           	PAGESEL __R2PCL
0003c1   d603     CALL	#0x603              	CALL __R2PCL
                                           	PAGESEL $
0003c2   8080     ADD	R0, #0x80            	ADD R0,#(_TOUCH_CH_TRS_EN+0)
0003c3   9901     MOV	R1, #0x1             	MOV R1,#0x01
0003c4   6503     CLR	0x3, 5               	BANKSEL _TOUCH_CH_TRS_EN
0003c5   f748     ST	[R0], R1              	ST [R0],R1
                                           	
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
0003c6   50cd     MOV	R0, 0xcd             	MOV R0,__KF8_LIBc_channel_
0003c7   80ae     ADD	R0, #0xae            	ADD R0,#Low(__KF8_TOUCH_CH_EN+0)
0003c8   9906     MOV	R1, #0x6             	MOV R1,#High(__KF8_TOUCH_CH_EN+0)
0003c9   7003     JNB	0x3, 0               	JNB PSW,0
0003ca   ff11     INC	R1                   	INC R1
                                           	PAGESEL __R2PCL
0003cb   d603     CALL	#0x603              	CALL __R2PCL
                                           	PAGESEL $
0003cc   8080     ADD	R0, #0x80            	ADD R0,#(_TOUCH_CH_TRS_EN+0)
0003cd   6503     CLR	0x3, 5               	BANKSEL _TOUCH_CH_TRS_EN
0003ce   f701     LD	R1, [R0]              	LD R1,[R0]
0003cf   a900     XOR	R1, #0               	XOR R1,#0x00
0003d0   7203     JNB	0x3, 2               	JNB PSW,2
0003d1   c4b3     JMP	#0x4b3               	JMP Label_x_y_z_a
                                           	
                                           ;	op : =
                                           ;	.line	64; "../debug_touch.c"	CLK_SET_IN;
0003d2   6925     SET	0x25, 1              	SET	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	65; "../debug_touch.c"	DAT_SET_IN;
0003d3   6825     SET	0x25, 0              	SET	_TR0_bits, 0
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	66; "../debug_touch.c"	Touch_Delay1;
0003d4   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	STK00
0003d5   519c     MOV	0x9c, R0             	MOV	STK00, R0
0003d6   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0003d7   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	70; "../debug_touch.c"	if(CLK_GET_STATE)
0003d8   7905     JB	0x5, 1                	JB	_P0_bits, 1
0003d9   c3e2     JMP	#0x3e2               	JMP	_00007_DS_
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	72; "../debug_touch.c"	Touch_Delay1;
0003da   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0003db   6503     CLR	0x3, 5               	BANKSEL	STK00
0003dc   519c     MOV	0x9c, R0             	MOV	STK00, R0
0003dd   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0003de   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	73; "../debug_touch.c"	if(!CLK_GET_STATE)
0003df   7105     JNB	0x5, 1               	JNB	_P0_bits, 1
0003e0   c3e6     JMP	#0x3e6               	JMP	_00008_DS_
                                           ;	op : RETURN
                                           ;	.line	74; "../debug_touch.c"	return;
0003e1   c4b3     JMP	#0x4b3               	JMP	_00045_DS_
                                           ;	op : LABEL
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           _00007_DS_
                                           ;	.line	76; "../debug_touch.c"	else if(!CLK_GET_STATE)
0003e2   7105     JNB	0x5, 1               	JNB	_P0_bits, 1
0003e3   c3e5     JMP	#0x3e5               	JMP	_00004_DS_
                                           ;	op : RETURN
                                           ;	.line	78; "../debug_touch.c"	return;
0003e4   c4b3     JMP	#0x4b3               	JMP	_00045_DS_
                                           ;	op : LABEL
                                           ;	op : RETURN
                                           _00004_DS_
                                           ;	.line	81; "../debug_touch.c"	return;
0003e5   c4b3     JMP	#0x4b3               	JMP	_00045_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00008_DS_
                                           ;	.line	83; "../debug_touch.c"	CLK_SET_OUT;
0003e6   6125     CLR	0x25, 1              	CLR	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	85; "../debug_touch.c"	CLK_SET_LOW;
0003e7   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	86; "../debug_touch.c"	Touch_Delay1;
0003e8   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0003e9   6503     CLR	0x3, 5               	BANKSEL	STK00
0003ea   519c     MOV	0x9c, R0             	MOV	STK00, R0
0003eb   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0003ec   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	88; "../debug_touch.c"	CLK_SET_HIGH;		//ÉÏÉýÑØ
0003ed   6905     SET	0x5, 1               	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	90; "../debug_touch.c"	Touch_Delay1;
0003ee   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0003ef   6503     CLR	0x3, 5               	BANKSEL	STK00
0003f0   519c     MOV	0x9c, R0             	MOV	STK00, R0
0003f1   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0003f2   d69c     CALL	#0x69c              	CALL	_delay_us
                                           ;	.line	92; "../debug_touch.c"	if(!DAT_GET_STATE)
                                           	PAGESEL	$
                                           ;	.line	94; "../debug_touch.c"	return;
0003f3   7805     JB	0x5, 0                	JB	_P0_bits, 0
                                           ;	.line	97; "../debug_touch.c"	CLK_SET_LOW;			//ÏÂ½µÑØ
0003f4   c4b3     JMP	#0x4b3               	JMP	_00045_DS_
0003f5   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	.line	101; "../debug_touch.c"	Touch_Delay1;
0003f6   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0003f7   6503     CLR	0x3, 5               	BANKSEL	STK00
0003f8   519c     MOV	0x9c, R0             	MOV	STK00, R0
0003f9   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0003fa   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	102; "../debug_touch.c"	DAT_SET_OUT;
0003fb   6025     CLR	0x25, 0              	CLR	_TR0_bits, 0
                                           ;	op : =
                                           ;	.line	104; "../debug_touch.c"	j=5;
0003fc   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0003fd   6503     CLR	0x3, 5               	BANKSEL	r0x1008
0003fe   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : =
                                           ;	.line	106; "../debug_touch.c"	for(step=0;step<5;step++)
                                           	BANKSEL	r0x1009
0003ff   03cc     CLR	0xcc                 	CLR	r0x1009
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x5=5), size=1
                                           _00037_DS_
000400   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	r0x1009
000401   38cc     SUB	R0, 0xcc             	SUB	R0, r0x1009
                                           ;comparing bytes at offset 0
000402   7003     JNB	0x3, 0               	JNB	PSW, 0
000403   c460     JMP	#0x460               	JMP	_00040_DS_
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;unsigned compare: left >= lit(0x5=5), size=1
                                           ;	.line	109; "../debug_touch.c"	switch(step)
000404   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	r0x1009
000405   38cc     SUB	R0, 0xcc             	SUB	R0, r0x1009
                                           ;comparing bytes at offset 0
000406   7003     JNB	0x3, 0               	JNB	PSW, 0
000407   c43f     JMP	#0x43f               	JMP	_00016_DS_
                                           ;	op : JUMPTABLE
000408   9804     MOV	R0, #0x4             	MOV	R0,#high _00067_DS_
000409   510a     MOV	0xa, R0              	MOV	PCH, R0
00040a   980f     MOV	R0, #0xf             	MOV	R0,#_00067_DS_
                                           	BANKSEL	r0x1009
00040b   20cc     ADD	R0, 0xcc             	ADD	R0, r0x1009
00040c   7003     JNB	0x3, 0               	JNB	PSW, 0
00040d   0b0a     INC	0xa                  	INC	PCH
00040e   5102     MOV	0x2, R0              	MOV	PCL, R0
                                           _00067_DS_
00040f   c414     JMP	#0x414               	JMP	_00011_DS_
000410   c420     JMP	#0x420               	JMP	_00012_DS_
000411   c428     JMP	#0x428               	JMP	_00013_DS_
000412   c430     JMP	#0x430               	JMP	_00014_DS_
000413   c438     JMP	#0x438               	JMP	_00015_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00011_DS_
                                           ;	.line	113; "../debug_touch.c"	j=5;
000414   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	r0x1008
000415   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
000416   50cd     MOV	R0, 0xcd             	MOV R0, __KF8_LIBc_channel_
000417   80ae     ADD	R0, #0xae            	ADD R0,#Low(__KF8_TOUCH_CH_EN+0)
000418   9906     MOV	R1, #0x6             	MOV R1,#High(__KF8_TOUCH_CH_EN+0)
000419   7003     JNB	0x3, 0               	JNB PSW,0
00041a   ff11     INC	R1                   	INC R1
00041b   530a     MOV	0xa, R1              	MOV PCH,R1
                                           	PAGESEL __R2PCL
00041c   d603     CALL	#0x603              	CALL __R2PCL
                                           	PAGESEL $
00041d   6503     CLR	0x3, 5               	BANKSEL _T_buf
00041e   51c9     MOV	0xc9, R0             	MOV _T_buf,R0
                                           	
                                           ;	op : GOTO
                                           ;	.line	132; "../debug_touch.c"	}break;
00041f   c43f     JMP	#0x43f               	JMP	_00016_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00012_DS_
                                           ;	.line	136; "../debug_touch.c"	j=8;
000420   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	r0x1008
000421   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
000422   6003     CLR	0x3, 0               	CLR PSW,0
000423   12cd     RLCR	0xcd                	RLCR __KF8_LIBc_channel_
                                           	BANKSEL __KF8_LIBi_buff_baseline_
000424   80a5     ADD	R0, #0xa5            	ADD R0,#(__KF8_LIBi_buff_baseline_+0)
000425   f701     LD	R1, [R0]              	LD R1,[R0]
                                           	BANKSEL _T_buf
000426   53c9     MOV	0xc9, R1             	MOV _T_buf,R1
                                           	
                                           ;	op : GOTO
                                           ;	.line	151; "../debug_touch.c"	}break;
000427   c43f     JMP	#0x43f               	JMP	_00016_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00013_DS_
                                           ;	.line	155; "../debug_touch.c"	j=8;
000428   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	r0x1008
000429   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
00042a   6003     CLR	0x3, 0               	CLR PSW,0
00042b   12cd     RLCR	0xcd                	RLCR __KF8_LIBc_channel_
                                           	BANKSEL __KF8_LIBi_buff_baseline_
00042c   80a6     ADD	R0, #0xa6            	ADD R0,#(__KF8_LIBi_buff_baseline_+1)
00042d   f701     LD	R1, [R0]              	LD R1,[R0]
                                           	BANKSEL _T_buf
00042e   53c9     MOV	0xc9, R1             	MOV _T_buf,R1
                                           	
                                           ;	op : GOTO
                                           ;	.line	172; "../debug_touch.c"	}break;
00042f   c43f     JMP	#0x43f               	JMP	_00016_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00014_DS_
                                           ;	.line	176; "../debug_touch.c"	j=8;
000430   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	r0x1008
000431   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
000432   6003     CLR	0x3, 0               	CLR PSW,0
000433   12cd     RLCR	0xcd                	RLCR __KF8_LIBc_channel_
                                           	BANKSEL __KF8_LIBi_buff_hit_
000434   809d     ADD	R0, #0x9d            	ADD R0,#(__KF8_LIBi_buff_hit_+0)
000435   f701     LD	R1, [R0]              	LD R1,[R0]
                                           	BANKSEL _T_buf
000436   53c9     MOV	0xc9, R1             	MOV _T_buf,R1
                                           	
                                           ;	op : GOTO
                                           ;	.line	192; "../debug_touch.c"	}break;
000437   c43f     JMP	#0x43f               	JMP	_00016_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00015_DS_
                                           ;	.line	196; "../debug_touch.c"	j=8;
000438   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	r0x1008
000439   51cb     MOV	0xcb, R0             	MOV	r0x1008, R0
                                           ;	op : INLINEASM
                                           	BANKSEL __KF8_LIBc_channel_
00043a   6003     CLR	0x3, 0               	CLR PSW,0
00043b   12cd     RLCR	0xcd                	RLCR __KF8_LIBc_channel_
                                           	BANKSEL __KF8_LIBi_buff_hit_
00043c   809e     ADD	R0, #0x9e            	ADD R0,#(__KF8_LIBi_buff_hit_+1)
00043d   f701     LD	R1, [R0]              	LD R1,[R0]
                                           	BANKSEL _T_buf
00043e   53c9     MOV	0xc9, R1             	MOV _T_buf,R1
                                           	
                                           ;	op : LABEL
                                           ;	op : =
                                           _00016_DS_
                                           ;	.line	214; "../debug_touch.c"	for(i_T_D=0;i_T_D<j;i_T_D++)
                                           	BANKSEL	_i_T_D
00043f   03ca     CLR	0xca                 	CLR	_i_T_D
                                           ;	op : LABEL
                                           ;	op : <
                                           _00033_DS_
                                           	BANKSEL	r0x1008
000440   0ecb     MOVZ	R0, 0xcb            	MOVZ	R0, r0x1008
                                           	BANKSEL	_i_T_D
000441   38ca     SUB	R0, 0xca             	SUB	R0, _i_T_D
                                           ;comparing bytes at offset 0
000442   7003     JNB	0x3, 0               	JNB	PSW, 0
000443   c459     JMP	#0x459               	JMP	_00036_DS_
                                           ;	op : BITWISEAND
                                           ;	.line	216; "../debug_touch.c"	if(T_buf&0x01)
                                           	BANKSEL	_T_buf
000444   78c9     JB	0xc9, 0               	JB	_T_buf, 0
000445   c448     JMP	#0x448               	JMP	_00018_DS_
                                           ;	op : =
                                           ;	.line	217; "../debug_touch.c"	DAT_SET_HIGH;
000446   6805     SET	0x5, 0               	SET	_P0_bits, 0
                                           ;	op : GOTO
000447   c449     JMP	#0x449               	JMP	_00019_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00018_DS_
                                           ;	.line	219; "../debug_touch.c"	DAT_SET_LOW;
000448   6005     CLR	0x5, 0               	CLR	_P0_bits, 0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00019_DS_
                                           ;	.line	221; "../debug_touch.c"	CLK_SET_HIGH;
000449   6905     SET	0x5, 1               	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	222; "../debug_touch.c"	Touch_Delay1;
00044a   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	STK00
00044b   519c     MOV	0x9c, R0             	MOV	STK00, R0
00044c   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
00044d   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	224; "../debug_touch.c"	CLK_SET_LOW;
00044e   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	225; "../debug_touch.c"	Touch_Delay1;
00044f   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
000450   6503     CLR	0x3, 5               	BANKSEL	STK00
000451   519c     MOV	0x9c, R0             	MOV	STK00, R0
000452   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
000453   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : RIGHT_OP
                                           ;	.line	227; "../debug_touch.c"	T_buf=T_buf>>1;
000454   6003     CLR	0x3, 0               	CLR	PSW, 0
000455   6503     CLR	0x3, 5               	BANKSEL	_T_buf
000456   11c9     RRC	0xc9                 	RRC	_T_buf
                                           ;	op : +
                                           ;	.line	214; "../debug_touch.c"	for(i_T_D=0;i_T_D<j;i_T_D++)
                                           	BANKSEL	_i_T_D
000457   0bca     INC	0xca                 	INC	_i_T_D
                                           ;	op : GOTO
000458   c440     JMP	#0x440               	JMP	_00033_DS_
                                           ;	op : LABEL
                                           ;	op : SEND
                                           ;	op : CALL
                                           _00036_DS_
                                           ;	.line	230; "../debug_touch.c"	Touch_Delay2;
000459   986e     MOV	R0, #0x6e            	MOV	R0,# 0x6e
                                           	BANKSEL	STK00
00045a   519c     MOV	0x9c, R0             	MOV	STK00, R0
00045b   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
00045c   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : +
                                           ;	.line	106; "../debug_touch.c"	for(step=0;step<5;step++)
00045d   6503     CLR	0x3, 5               	BANKSEL	r0x1009
00045e   0bcc     INC	0xcc                 	INC	r0x1009
                                           ;	op : GOTO
00045f   c400     JMP	#0x400               	JMP	_00037_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00040_DS_
                                           ;	.line	234; "../debug_touch.c"	DAT_SET_IN;
000460   6825     SET	0x25, 0              	SET	_TR0_bits, 0
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	235; "../debug_touch.c"	Touch_Delay2;	//±à³ÌÆ÷ÅÐ¶ÏÐèÒªÊ±¼ä
000461   986e     MOV	R0, #0x6e            	MOV	R0,# 0x6e
                                           	BANKSEL	STK00
000462   519c     MOV	0x9c, R0             	MOV	STK00, R0
000463   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
000464   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	237; "../debug_touch.c"	CLK_SET_HIGH;
000465   6905     SET	0x5, 1               	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	238; "../debug_touch.c"	Touch_Delay1;
000466   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
000467   6503     CLR	0x3, 5               	BANKSEL	STK00
000468   519c     MOV	0x9c, R0             	MOV	STK00, R0
000469   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
00046a   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	239; "../debug_touch.c"	Touch_Delay1;
00046b   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
00046c   6503     CLR	0x3, 5               	BANKSEL	STK00
00046d   519c     MOV	0x9c, R0             	MOV	STK00, R0
00046e   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
00046f   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	240; "../debug_touch.c"	Touch_Delay1;
000470   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
000471   6503     CLR	0x3, 5               	BANKSEL	STK00
000472   519c     MOV	0x9c, R0             	MOV	STK00, R0
000473   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
000474   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	243; "../debug_touch.c"	if(DAT_GET_STATE)
000475   7805     JB	0x5, 0                	JB	_P0_bits, 0
000476   c4ab     JMP	#0x4ab               	JMP	_00031_DS_
                                           ;	op : =
                                           ;	.line	245; "../debug_touch.c"	CLK_SET_LOW;
000477   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	op : =
                                           ;	.line	246; "../debug_touch.c"	T_buf=0;
000478   6503     CLR	0x3, 5               	BANKSEL	_T_buf
000479   03c9     CLR	0xc9                 	CLR	_T_buf
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	247; "../debug_touch.c"	Touch_Delay1;
00047a   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	STK00
00047b   519c     MOV	0x9c, R0             	MOV	STK00, R0
00047c   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
00047d   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	248; "../debug_touch.c"	for(i_T_D=0;i_T_D<6;i_T_D++)
00047e   6503     CLR	0x3, 5               	BANKSEL	_i_T_D
00047f   03ca     CLR	0xca                 	CLR	_i_T_D
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x6=6), size=1
                                           _00041_DS_
000480   9806     MOV	R0, #0x6             	MOV	R0,# 0x06
                                           	BANKSEL	_i_T_D
000481   38ca     SUB	R0, 0xca             	SUB	R0, _i_T_D
                                           ;comparing bytes at offset 0
000482   7003     JNB	0x3, 0               	JNB	PSW, 0
000483   c4b1     JMP	#0x4b1               	JMP	_00032_DS_
                                           ;	op : =
                                           ;	.line	250; "../debug_touch.c"	CLK_SET_HIGH;
000484   6905     SET	0x5, 1               	SET	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	251; "../debug_touch.c"	Touch_Delay1;
000485   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	STK00
000486   519c     MOV	0x9c, R0             	MOV	STK00, R0
000487   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
000488   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : EQ_OP
                                           ;	.line	253; "../debug_touch.c"	if(i_T_D!=5)
000489   6503     CLR	0x3, 5               	BANKSEL	_i_T_D
00048a   0eca     MOVZ	R0, 0xca            	MOVZ	R0, _i_T_D
                                           ;	.line	255; "../debug_touch.c"	T_buf=T_buf>>1;
00048b   a805     XOR	R0, #0x5             	XOR	R0,# 0x05
00048c   7203     JNB	0x3, 2               	JNB	PSW, 2
00048d   c494     JMP	#0x494               	JMP	_00028_DS_
00048e   6003     CLR	0x3, 0               	CLR	PSW, 0
                                           	BANKSEL	_T_buf
00048f   11c9     RRC	0xc9                 	RRC	_T_buf
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	256; "../debug_touch.c"	if(DAT_GET_STATE)
000490   7805     JB	0x5, 0                	JB	_P0_bits, 0
000491   c4a3     JMP	#0x4a3               	JMP	_00029_DS_
                                           ;	op : |
                                           ;	.line	257; "../debug_touch.c"	T_buf=T_buf|0x10;
                                           	BANKSEL	_T_buf
000492   6cc9     SET	0xc9, 4              	SET	_T_buf, 4
                                           ;	op : GOTO
000493   c4a3     JMP	#0x4a3               	JMP	_00029_DS_
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00028_DS_
                                           ;	.line	261; "../debug_touch.c"	if(T_buf<16)   //´«Êä´íÎóµÄ£¬·ÀÏÂ·ÇÓ°ÏìÆäËûÊý¾Ý
000494   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	_T_buf
000495   38c9     SUB	R0, 0xc9             	SUB	R0, _T_buf
                                           ;comparing bytes at offset 0
000496   7003     JNB	0x3, 0               	JNB	PSW, 0
000497   c4a3     JMP	#0x4a3               	JMP	_00029_DS_
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	263; "../debug_touch.c"	if(DAT_GET_STATE)
000498   7805     JB	0x5, 0                	JB	_P0_bits, 0
000499   c49f     JMP	#0x49f               	JMP	_00023_DS_
                                           ;	op : INLINEASM
                                           	BANKSEL _T_buf
00049a   50c9     MOV	R0, 0xc9             	MOV R0,_T_buf
00049b   8080     ADD	R0, #0x80            	ADD R0,#(_TOUCH_CH_TRS_EN+0)
00049c   9901     MOV	R1, #0x1             	MOV R1,#0x01
                                           	BANKSEL _TOUCH_CH_TRS_EN
00049d   f748     ST	[R0], R1              	ST [R0],R1
                                           	
                                           ;	op : GOTO
00049e   c4a3     JMP	#0x4a3               	JMP	_00029_DS_
                                           ;	op : LABEL
                                           ;	op : INLINEASM
                                           _00023_DS_
                                           	BANKSEL _T_buf
00049f   50c9     MOV	R0, 0xc9             	MOV R0,_T_buf
0004a0   8080     ADD	R0, #0x80            	ADD R0,#(_TOUCH_CH_TRS_EN+0)
0004a1   9900     MOV	R1, #0               	MOV R1,#0x00
                                           	BANKSEL _TOUCH_CH_TRS_EN
0004a2   f748     ST	[R0], R1              	ST [R0],R1
                                           	
                                           ;	op : LABEL
                                           ;	op : =
                                           _00029_DS_
                                           ;	.line	289; "../debug_touch.c"	CLK_SET_LOW;
0004a3   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	290; "../debug_touch.c"	Touch_Delay1;
0004a4   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
                                           	BANKSEL	STK00
0004a5   519c     MOV	0x9c, R0             	MOV	STK00, R0
0004a6   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0004a7   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : +
                                           ;	.line	248; "../debug_touch.c"	for(i_T_D=0;i_T_D<6;i_T_D++)
0004a8   6503     CLR	0x3, 5               	BANKSEL	_i_T_D
0004a9   0bca     INC	0xca                 	INC	_i_T_D
                                           ;	op : GOTO
0004aa   c480     JMP	#0x480               	JMP	_00041_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00031_DS_
                                           ;	.line	295; "../debug_touch.c"	CLK_SET_LOW;
0004ab   6105     CLR	0x5, 1               	CLR	_P0_bits, 1
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	296; "../debug_touch.c"	Touch_Delay1;
0004ac   9805     MOV	R0, #0x5             	MOV	R0,# 0x05
0004ad   6503     CLR	0x3, 5               	BANKSEL	STK00
0004ae   519c     MOV	0x9c, R0             	MOV	STK00, R0
0004af   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_delay_us
0004b0   d69c     CALL	#0x69c              	CALL	_delay_us
                                           	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : =
                                           _00032_DS_
                                           ;	.line	299; "../debug_touch.c"	CLK_SET_IN;
0004b1   6925     SET	0x25, 1              	SET	_TR0_bits, 1
                                           ;	op : =
                                           ;	.line	300; "../debug_touch.c"	DAT_SET_IN;
0004b2   6825     SET	0x25, 0              	SET	_TR0_bits, 0
                                           ;	op : INLINEASM
                                           Label_x_y_z_a:
                                           	
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00045_DS_
0004b3   0008     CRET                     	CRET	
                                           ; exit point of _TOUCH_DEBUG_TRS_DEAL
                                           
                                           
                                           ;	code size estimation:
                                           ;	  420+   91 =   511 instructions ( 1204 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Mar  1 2016 15:13:08) (MSVC)
                                           ; This file was generated Thu Apr 28 16:35:45 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../init_mcu.c"
                                           	.radix dec
                                           	.include "KF8S1022.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1022 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2                .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           T2CCR             .EQU                0x54
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P12               .EQU                2
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x12 T2CTL Bits----------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT1SE             .EQU                6
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS6               .EQU                6
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           _ANS6              .EQU                6
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CMCTL1_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_T3L_bits
                                           	.extern	_CTCTL_bits
                                           	.extern	_OSCLDOCAL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2
                                           	.extern	_T2CTL
                                           	.extern	_PWMCTL
                                           	.extern	_CMCTL1
                                           	.extern	_VRECAL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_OPTR
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_TR3
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T3L
                                           	.extern	_CTCTL
                                           	.extern	_T2CCR
                                           	.extern	_OSCLDOCAL
                                           	.extern	_T1U
                                           
                                           	.extern STK12
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_init_mcu
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	17; "../init_mcu.c"	OSCCTL = 0x60;           //8M
000678   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
000679   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	20; "../init_mcu.c"	TR0 = 0XFF;              //1111 1111		£¡£¡¡¶¡¶×¢Òâµã:TR0.7ÕâÒ»Î»±ØÐëÉèÖÃÎª1£¬ÊäÈëÌ¬¡·¡·£¡£¡
00067a   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
00067b   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	21; "../init_mcu.c"	TR1 = 0XFF;              //1111 1111		P16,P17´¥ÃþÍ¨µÀ2,3  ÉèÖÃIO¿ÚÎªÊäÈë
00067c   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
00067d   5127     MOV	0x27, R0             	MOV	_TR1, R0
                                           ;	op : =
                                           ;	.line	22; "../init_mcu.c"	TR2 = 0XFF;              //1111 1111		P20,P21´¥ÃþÍ¨µÀ4,5  ÉèÖÃIO¿ÚÎªÊäÈë
00067e   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
00067f   5126     MOV	0x26, R0             	MOV	_TR2, R0
                                           ;	op : =
                                           ;	.line	24; "../init_mcu.c"	P0 = 0X00;               //0000 0000
000680   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	25; "../init_mcu.c"	P1 = 0X00;               //0000 0000
000681   0307     CLR	0x7                  	CLR	_P1
                                           ;	op : =
                                           ;	.line	26; "../init_mcu.c"	P2 = 0x00;               //0000 0000
000682   0306     CLR	0x6                  	CLR	_P2
                                           ;	op : |
                                           ;	.line	28; "../init_mcu.c"	ANSEL |= 1<<6;			 //ÉèÖÃAN6ÎªÄ£Äâ¿Ú,Íâ¹ÒµçÈÝ½ÅÉèÖÃÎªÄ£Äâ¿Ú
000683   6e31     SET	0x31, 6              	SET	_ANSEL, 6
                                           ;	op : =
                                           ;	.line	31; "../init_mcu.c"	T1CTL = 0X00;    		 //1£º1·ÖÆµ£¬²»¿ªÆô¼ÆÊýÆ÷T1
000684   0310     CLR	0x10                 	CLR	_T1CTL
                                           ;	op : =
                                           ;	.line	32; "../init_mcu.c"	T1L = 0;
000685   030e     CLR	0xe                  	CLR	_T1L
                                           ;	op : =
                                           ;	.line	33; "../init_mcu.c"	T1H = 0;
000686   030f     CLR	0xf                  	CLR	_T1H
                                           ;	op : =
                                           ;	.line	34; "../init_mcu.c"	T1IF = 0;
000687   600c     CLR	0xc, 0               	CLR	_EIF1_bits, 0
                                           ;	op : =
                                           ;	.line	35; "../init_mcu.c"	AIE = 0;
000688   670b     CLR	0xb, 7               	CLR	_INTCTL_bits, 7
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000689   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           ;	code size estimation:
                                           ;	   18+    0 =    18 instructions (   36 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Mar  1 2016 15:13:08) (MSVC)
                                           ; This file was generated Thu Apr 28 16:20:54 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../kf8s_touch_g.c"
                                           	.radix dec
                                           	.include "KF8S1022.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1022 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2                .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           T2CCR             .EQU                0x54
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P12               .EQU                2
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x12 T2CTL Bits----------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT1SE             .EQU                6
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS6               .EQU                6
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           _ANS6              .EQU                6
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_init_mcu
                                           	.extern	__KF8S_Get_Ver_General_
                                           	.extern	__KF8S_Lib_Set_General_Parameter
                                           	.extern	__KF8S_Init_Touch_General_
                                           	.extern	__KF8S_Touch_Process_General_
                                           	.extern	__KF8S_Touch_TEST_General_
                                           	.extern	__R2PCL
                                           	.extern	_TOUCH_DEBUG_TRS_DEAL
                                           	.extern	_TOUCH_DEBUG_SEND_OUT
                                           	.extern	_delay_ms
                                           	.extern	_delay_us
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CMCTL1_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_T3L_bits
                                           	.extern	_CTCTL_bits
                                           	.extern	_OSCLDOCAL_bits
                                           	.extern	__KF8_LIBc_channel_Buf
                                           	.extern	_sentbuf1
                                           	.extern	_sentbuf2
                                           	.extern	_sentbuf3
                                           	.extern	_sentbuf4
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2
                                           	.extern	_T2CTL
                                           	.extern	_PWMCTL
                                           	.extern	_CMCTL1
                                           	.extern	_VRECAL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_OPTR
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_TR3
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T3L
                                           	.extern	_CTCTL
                                           	.extern	_T2CCR
                                           	.extern	_OSCLDOCAL
                                           	.extern	_T1U
                                           
                                           	.extern STK12
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	__KF8_LIBc_baseline_count_
                                           	.global	__KF8_LIBi_buff_hit_
                                           	.global	__KF8_LIBi_buff_baseline_
                                           	.global	__KF8_LIBc_touch_count_
                                           	.global	__KF8_LIBi_Date_Change_
                                           	.global	__KF8_LIBc_channel_
                                           	.global	__KF8_LIBi_channel_flag_
                                           	.global	_CHS_AMOUNT
                                           	.global	_TCS_AMOUNT
                                           	.global	__KF8_Disturb_Protect_Circle_
                                           	.global	__KF8_DoubleKey_Compages_Limitable_Circle_
                                           	.global	__KF8_Key_Max_Pressed_Limitable_Circle_
                                           	.global	__KF8_BaseLine_Update_Circle_Count_For_UP_
                                           	.global	__KF8_BaseLine_Update_Circle_Count_For_Down_
                                           	.global	__KF8_Define_Disturb_Channels_Amount_
                                           	.global	__KF8_BasicLine_UP_Noise_Threshold_
                                           	.global	__KF8_BasicLine_Down_Noise_Threshold_
                                           	.global	__KF8_Data_Steady_Threshold_Set_
                                           	.global	__KF8_Inside_Reference_Channel_Disturb_Threshold_Set_
                                           	.global	__KF8_TOUCH_CH_EN
                                           	.global	__KF8_Inside_Reference_Channel_Declare_
                                           	.global	__KF8_Config_Finger_Threshold
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_kf8s_touch_g_0	.udata
                                           __KF8_LIBc_baseline_count_	.res	4
                                           
                                           UD_kf8s_touch_g_1	.udata
                                           __KF8_LIBi_buff_hit_	.res	8
                                           
                                           UD_kf8s_touch_g_2	.udata
                                           __KF8_LIBi_buff_baseline_	.res	8
                                           
                                           UD_kf8s_touch_g_3	.udata
                                           __KF8_LIBc_touch_count_	.res	4
                                           
                                           UD_kf8s_touch_g_4	.udata
                                           __KF8_LIBi_Date_Change_	.res	4
                                           
                                           UD_kf8s_touch_g_5	.udata
                                           __KF8_LIBc_channel_	.res	1
                                           
                                           UD_kf8s_touch_g_6	.udata
                                           __KF8_LIBi_channel_flag_	.res	2
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           
                                           ID_kf8s_touch_g_0	.code
                                           _CHS_AMOUNT
0006c0   b004     RRET	R0, #0x4            	RRET R0, #0x04
                                           
                                           
                                           ID_kf8s_touch_g_1	.code
                                           _TCS_AMOUNT
0006c1   b005     RRET	R0, #0x5            	RRET R0, #0x05
                                           
                                           
                                           ID_kf8s_touch_g_2	.code
                                           __KF8_Disturb_Protect_Circle_
0006c2   b064     RRET	R0, #0x64           	RRET R0, #0x64
                                           
                                           
                                           ID_kf8s_touch_g_3	.code
                                           __KF8_DoubleKey_Compages_Limitable_Circle_
000002   b02c     RRET	R0, #0x2c           	RRET R0, #0x2c
000003   b001     RRET	R0, #0x1            	RRET R0, #0x01
                                           
                                           
                                           ID_kf8s_touch_g_4	.code
                                           __KF8_Key_Max_Pressed_Limitable_Circle_
0006bc   b040     RRET	R0, #0x40           	RRET R0, #0x40
0006bd   b01f     RRET	R0, #0x1f           	RRET R0, #0x1f
                                           
                                           
                                           ID_kf8s_touch_g_5	.code
                                           __KF8_BaseLine_Update_Circle_Count_For_UP_
0006c3   b040     RRET	R0, #0x40           	RRET R0, #0x40
                                           
                                           
                                           ID_kf8s_touch_g_6	.code
                                           __KF8_BaseLine_Update_Circle_Count_For_Down_
0006c4   b0c0     RRET	R0, #0xc0           	RRET R0, #0xc0
                                           
                                           
                                           ID_kf8s_touch_g_7	.code
                                           __KF8_Define_Disturb_Channels_Amount_
0006c5   b003     RRET	R0, #0x3            	RRET R0, #0x03
                                           
                                           
                                           ID_kf8s_touch_g_8	.code
                                           __KF8_BasicLine_UP_Noise_Threshold_
0006c6   b0dd     RRET	R0, #0xdd           	RRET R0, #0xdd
                                           
                                           
                                           ID_kf8s_touch_g_9	.code
                                           __KF8_BasicLine_Down_Noise_Threshold_
0006c7   b023     RRET	R0, #0x23           	RRET R0, #0x23
                                           
                                           
                                           ID_kf8s_touch_g_10	.code
                                           __KF8_Data_Steady_Threshold_Set_
0006c8   b014     RRET	R0, #0x14           	RRET R0, #0x14
                                           
                                           
                                           ID_kf8s_touch_g_11	.code
                                           __KF8_Inside_Reference_Channel_Disturb_Threshold_Set_
0006c9   b00f     RRET	R0, #0xf            	RRET R0, #0x0f
                                           
                                           
                                           ID_kf8s_touch_g_12	.code
                                           __KF8_TOUCH_CH_EN
0006ae   b002     RRET	R0, #0x2            	RRET R0, #0x02
0006af   b003     RRET	R0, #0x3            	RRET R0, #0x03
0006b0   b004     RRET	R0, #0x4            	RRET R0, #0x04
0006b1   b005     RRET	R0, #0x5            	RRET R0, #0x05
                                           
                                           
                                           ID_kf8s_touch_g_13	.code
                                           __KF8_Inside_Reference_Channel_Declare_
0006ca   b014     RRET	R0, #0x14           	RRET R0, #0x14
                                           
                                           
                                           ID_kf8s_touch_g_14	.code
                                           __KF8_Config_Finger_Threshold
0006b2   b032     RRET	R0, #0x32           	RRET R0, #0x32
0006b3   b032     RRET	R0, #0x32           	RRET R0, #0x32
0006b4   b032     RRET	R0, #0x32           	RRET R0, #0x32
0006b5   b032     RRET	R0, #0x32           	RRET R0, #0x32
                                           
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Mar  1 2016 15:13:08) (MSVC)
                                           ; This file was generated Thu Apr 28 18:02:17 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.radix dec
                                           	.include "KF8S1022.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1022 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2                .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           T2CCR             .EQU                0x54
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P12               .EQU                2
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x12 T2CTL Bits----------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT1SE             .EQU                6
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS6               .EQU                6
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           _ANS6              .EQU                6
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_init_mcu
                                           	.extern	__KF8S_Get_Ver_General_
                                           	.extern	__KF8S_Lib_Set_General_Parameter
                                           	.extern	__KF8S_Init_Touch_General_
                                           	.extern	__KF8S_Touch_Process_General_
                                           	.extern	__KF8S_Touch_TEST_General_
                                           	.extern	__R2PCL
                                           	.extern	_TOUCH_DEBUG_TRS_DEAL
                                           	.extern	_TOUCH_DEBUG_SEND_OUT
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CMCTL1_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_T3L_bits
                                           	.extern	_CTCTL_bits
                                           	.extern	_OSCLDOCAL_bits
                                           	.extern	__KF8_LIBi_channel_flag_
                                           	.extern	__KF8_LIBc_channel_
                                           	.extern	__KF8_LIBc_channel_Buf
                                           	.extern	__KF8_LIBi_Date_Change_
                                           	.extern	__KF8_LIBc_baseline_count_
                                           	.extern	__KF8_LIBi_buff_hit_
                                           	.extern	__KF8_LIBi_buff_baseline_
                                           	.extern	__KF8_LIBc_touch_count_
                                           	.extern	_sentbuf1
                                           	.extern	_sentbuf2
                                           	.extern	_sentbuf3
                                           	.extern	_sentbuf4
                                           	.extern	_CHS_AMOUNT
                                           	.extern	_TCS_AMOUNT
                                           	.extern	__KF8_Disturb_Protect_Circle_
                                           	.extern	__KF8_DoubleKey_Compages_Limitable_Circle_
                                           	.extern	__KF8_Key_Max_Pressed_Limitable_Circle_
                                           	.extern	__KF8_BaseLine_Update_Circle_Count_For_UP_
                                           	.extern	__KF8_BaseLine_Update_Circle_Count_For_Down_
                                           	.extern	__KF8_Define_Disturb_Channels_Amount_
                                           	.extern	__KF8_BasicLine_UP_Noise_Threshold_
                                           	.extern	__KF8_BasicLine_Down_Noise_Threshold_
                                           	.extern	__KF8_Data_Steady_Threshold_Set_
                                           	.extern	__KF8_Inside_Reference_Channel_Disturb_Threshold_Set_
                                           	.extern	__KF8_Inside_Reference_Channel_Declare_
                                           	.extern	__KF8_Config_Finger_Threshold
                                           	.extern	__KF8_TOUCH_CH_EN
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2
                                           	.extern	_T2CTL
                                           	.extern	_PWMCTL
                                           	.extern	_CMCTL1
                                           	.extern	_VRECAL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_OPTR
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_TR3
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T3L
                                           	.extern	_CTCTL
                                           	.extern	_T2CCR
                                           	.extern	_OSCLDOCAL
                                           	.extern	_T1U
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_delay_us
                                           	.global	_delay_ms
                                           	.global	_display
                                           	.global	_INT_FUN
                                           	.global	_main
                                           	.global	_Touch_Watch
                                           	.global	_flag
                                           
                                           	.global STK12
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata
                                           STK12	.res 1
                                           	.type STK12, 108
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_main_0	.udata
                                           _Touch_Watch	.res	2
                                           
                                           UD_main_1	.udata
                                           _flag	.res	1
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1004	.res	1
                                           UDL_main_1	.udata
                                           r0x1003	.res	1
                                           UDL_main_2	.udata
                                           r0x1005	.res	1
                                           UDL_main_3	.udata
                                           r0x1006	.res	1
                                           UDL_main_4	.udata
                                           r0x1007	.res	1
                                           UDL_main_5	.udata
                                           r0x1008	.res	1
                                           UDL_main_6	.udata
                                           r0x100E	.res	1
                                           UDL_main_7	.udata
                                           r0x100D	.res	1
                                           UDL_main_8	.udata
                                           r0x100F	.res	1
                                           UDL_main_9	.udata
                                           r0x1010	.res	1
                                           UDL_main_10	.udata
                                           r0x1009	.res	1
                                           UDL_main_11	.udata
                                           r0x100A	.res	1
                                           UDL_main_12	.udata
                                           r0x100B	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
                                           	PAGESEL	init_imp
000001   c6b6     JMP	#0x6b6               	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
                                           	PAGESEL	_startup
0006b6   d605     CALL	#0x605              	CALL	_startup
                                           	PAGESEL	__sdcc_gsinit_startup
0006b7   d6be     CALL	#0x6be              	CALL	__sdcc_gsinit_startup
                                           	PAGESEL	_main
0006b8   c598     JMP	#0x598               	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           c_interrupt	.code	0x4
000004   f8c3     MOV	R3, R0               	MOV		R3,R0
000005   5803     MOV	R4, 0x3              	MOV		R4,PSW
000006   5a0a     MOV	R5, 0xa              	MOV		R5,PCH
000007   f8ca     MOV	R2, R1               	MOV		R2,R1
                                           	PAGESEL	__sdcc_interrupt
000008   c68a     JMP	#0x68a               	JMP		__sdcc_interrupt
                                           
                                           
                                           
                                           func._INT_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _INT_FUN	;Function start
                                           ; 0 exit points
                                           ;functions called:
                                           ;   _TOUCH_DEBUG_TRS_DEAL
                                           ;   __KF8S_Touch_Process_General_
                                           ;   _TOUCH_DEBUG_TRS_DEAL
                                           ;   __KF8S_Touch_Process_General_
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _INT_FUN	;Function start
                                           ; 0 exit points
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           __sdcc_interrupt
                                           ;	.line	128; "../main.c"	if(T1IF||CTIF)
00068a   700c     JNB	0xc, 0               	JNB	_EIF1_bits, 0
00068b   c68e     JMP	#0x68e               	JMP	_00023_DS_
                                           ;	op : GET_VALUE_AT_ADDRESS
00068c   7f0c     JB	0xc, 7                	JB	_EIF1_bits, 7
00068d   c697     JMP	#0x697               	JMP	_00026_DS_
                                           ;	op : LABEL
                                           ;	op : =
                                           _00023_DS_
                                           ;	.line	130; "../main.c"	T1IF=0;
00068e   600c     CLR	0xc, 0               	CLR	_EIF1_bits, 0
                                           ;	op : =
                                           ;	.line	131; "../main.c"	CTIF=0;
00068f   670c     CLR	0xc, 7               	CLR	_EIF1_bits, 7
                                           ;	op : =
                                           ;	.line	132; "../main.c"	Touch_Watch=0;
000690   6503     CLR	0x3, 5               	BANKSEL	_Touch_Watch
000691   03bb     CLR	0xbb                 	CLR	_Touch_Watch
                                           	BANKSEL	_Touch_Watch
000692   03bc     CLR	0xbc                 	CLR	(_Touch_Watch + 1)
                                           ;	op : =
                                           ;	.line	133; "../main.c"	flag = 1;
000693   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_flag
000694   51ce     MOV	0xce, R0             	MOV	_flag, R0
                                           ;	op : CALL
                                           ;	.line	135; "../main.c"	TOUCH_DEBUG_TRS_DEAL();		// µ÷ÊÔÇúÏßÊä³ö
                                           	PAGESEL	_TOUCH_DEBUG_TRS_DEAL
000695   d3bc     CALL	#0x3bc              	CALL	_TOUCH_DEBUG_TRS_DEAL
                                           	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	136; "../main.c"	_KF8S_Touch_Process_General_(); //¸üÐÂ°´¼ü±êÖ¾
                                           	PAGESEL	__KF8S_Touch_Process_General_
000696   d4b4     CALL	#0x4b4              	CALL	__KF8S_Touch_Process_General_
                                           	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00026_DS_
000697   f8d1     MOV	R1, R2               	MOV	R1, R2
000698   5b0a     MOV	0xa, R5              	MOV	PCH, R5
000699   5903     MOV	0x3, R4              	MOV	PSW, R4
00069a   f8d8     MOV	R0, R3               	MOV	R0, R3
00069b   0009     IRET                     	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _delay_ms
                                           ;   __KF8S_Init_Touch_General_
                                           ;   _display
                                           ;   __KF8S_Init_Touch_General_
                                           ;   _init_mcu
                                           ;   _delay_ms
                                           ;   __KF8S_Init_Touch_General_
                                           ;   _display
                                           ;   __KF8S_Init_Touch_General_
                                           ;5 compiler assigned registers:
                                           ;   STK00
                                           ;   r0x1009
                                           ;   r0x100A
                                           ;   r0x100B
                                           ;   r0x100C
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	150; "../main.c"	init_mcu();						//³õÊ¼»¯MCU¼Ä´æÆ÷
                                           	PAGESEL	_init_mcu
000598   d678     CALL	#0x678              	CALL	_init_mcu
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	151; "../main.c"	delay_ms(500);					//ÑÓÊ±Ò»»á£¬·ÀÖ¹ÉÏµçÎó´¥·¢´¥ÃþÍ¨µÀ
000599   98f4     MOV	R0, #0xf4            	MOV	R0,# 0xf4
00059a   6503     CLR	0x3, 5               	BANKSEL	STK00
00059b   519c     MOV	0x9c, R0             	MOV	STK00, R0
00059c   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	PAGESEL	_delay_ms
00059d   d616     CALL	#0x616              	CALL	_delay_ms
                                           	PAGESEL	$
                                           ;	op : =
                                           ;	.line	152; "../main.c"	CMCTL1 = 0x90;    //ÉèÖÃ´¥Ãþ·ÖÆµºÍ»ù×¼µçÑ¹
00059e   9890     MOV	R0, #0x90            	MOV	R0,# 0x90
00059f   511a     MOV	0x1a, R0             	MOV	_CMCTL1, R0
                                           ;	op : INLINEASM
0005a0   0064     CWDT                     	CWDT 
                                           ;	op : CALL
                                           ;	.line	156; "../main.c"	_KF8S_Init_Touch_General_();		//µ÷ÓÃµçÈÝ´¥Ãþ¿âº¯ÊýµÄ³õÊ¼»¯
                                           	PAGESEL	__KF8S_Init_Touch_General_
0005a1   d5c5     CALL	#0x5c5              	CALL	__KF8S_Init_Touch_General_
                                           	PAGESEL	$
                                           ;	op : INLINEASM
0005a2   0064     CWDT                     	CWDT 
                                           ;	op : LABEL
                                           ;	op : INLINEASM
                                           _00032_DS_
0005a3   0064     CWDT                     	CWDT 
                                           ;	op : CALL
                                           ;	.line	163; "../main.c"	display();					//ÏÔÊ¾LEDµÆ
                                           	PAGESEL	_display
0005a4   d6cb     CALL	#0x6cb              	CALL	_display
                                           	PAGESEL	$
                                           ;	op : +
                                           ;	.line	176; "../main.c"	Touch_Watch++;
0005a5   6503     CLR	0x3, 5               	BANKSEL	_Touch_Watch
0005a6   0bbb     INC	0xbb                 	INC	_Touch_Watch
0005a7   7a03     JB	0x3, 2                	JB	PSW, 2
0005a8   c5aa     JMP	#0x5aa               	JMP	_00039_DS_
                                           	BANKSEL	_Touch_Watch
0005a9   0bbc     INC	0xbc                 	INC	(_Touch_Watch + 1)
                                           ;	op : CAST
                                           _00039_DS_
                                           ;	.line	177; "../main.c"	if(Touch_Watch>50000)
                                           	BANKSEL	_Touch_Watch
0005aa   0ebb     MOVZ	R0, 0xbb            	MOVZ	R0, _Touch_Watch
                                           	BANKSEL	r0x1009
0005ab   51d9     MOV	0xd9, R0             	MOV	r0x1009, R0
                                           	BANKSEL	_Touch_Watch
0005ac   0ebc     MOVZ	R0, 0xbc            	MOVZ	R0, (_Touch_Watch + 1)
                                           	BANKSEL	r0x100A
0005ad   51da     MOV	0xda, R0             	MOV	r0x100A, R0
                                           	BANKSEL	r0x100B
0005ae   03db     CLR	0xdb                 	CLR	r0x100B
                                           ;;1	CLR	r0x100C
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;signed compare: left >= lit(0xC351=50001), size=4, mask=ffffffff
0005af   9800     MOV	R0, #0               	MOV	R0,# 0x00
0005b0   8080     ADD	R0, #0x80            	ADD	R0,# 0x80
0005b1   8080     ADD	R0, #0x80            	ADD	R0,# 0x80
                                           ;comparing bytes at offset 3
0005b2   7a03     JB	0x3, 2                	JB	PSW, 2
0005b3   c5be     JMP	#0x5be               	JMP	_00038_DS_
0005b4   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x100B
0005b5   38db     SUB	R0, 0xdb             	SUB	R0, r0x100B
0005b6   7a03     JB	0x3, 2                	JB	PSW, 2
0005b7   c5be     JMP	#0x5be               	JMP	_00038_DS_
0005b8   98c3     MOV	R0, #0xc3            	MOV	R0,# 0xc3
                                           	BANKSEL	r0x100A
0005b9   38da     SUB	R0, 0xda             	SUB	R0, r0x100A
0005ba   7a03     JB	0x3, 2                	JB	PSW, 2
0005bb   c5be     JMP	#0x5be               	JMP	_00038_DS_
0005bc   9851     MOV	R0, #0x51            	MOV	R0,# 0x51
                                           	BANKSEL	r0x1009
0005bd   38d9     SUB	R0, 0xd9             	SUB	R0, r0x1009
                                           _00038_DS_
0005be   7803     JB	0x3, 0                	JB	PSW, 0
0005bf   c5a3     JMP	#0x5a3               	JMP	_00032_DS_
                                           ;	op : =
                                           ;	.line	179; "../main.c"	Touch_Watch=0;
                                           	BANKSEL	_Touch_Watch
0005c0   03bb     CLR	0xbb                 	CLR	_Touch_Watch
                                           	BANKSEL	_Touch_Watch
0005c1   03bc     CLR	0xbc                 	CLR	(_Touch_Watch + 1)
                                           ;	op : CALL
                                           ;	.line	180; "../main.c"	_KF8S_Init_Touch_General_();
                                           	PAGESEL	__KF8S_Init_Touch_General_
0005c2   d5c5     CALL	#0x5c5              	CALL	__KF8S_Init_Touch_General_
                                           	PAGESEL	$
                                           ;	op : GOTO
0005c3   c5a3     JMP	#0x5a3               	JMP	_00032_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
0005c4   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._delay_us	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _delay_us	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x100D
                                           ;   STK00
                                           ;   r0x100E
                                           ;   r0x100F
                                           ;   r0x1010
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _delay_us	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	89; "../main.c"	void delay_us(uint us_data)
00069c   6503     CLR	0x3, 5               	BANKSEL	r0x100D
00069d   51d6     MOV	0xd6, R0             	MOV	r0x100D, R0
                                           	BANKSEL	STK00
00069e   0e9c     MOVZ	R0, 0x9c            	MOVZ	R0, STK00
                                           	BANKSEL	r0x100E
00069f   51d5     MOV	0xd5, R0             	MOV	r0x100E, R0
                                           ;	op : =
                                           ;	op : LABEL
                                           ;	op : =
                                           _00016_DS_
                                           ;	.line	91; "../main.c"	while(us_data--);
                                           	BANKSEL	r0x100E
0006a0   0ed5     MOVZ	R0, 0xd5            	MOVZ	R0, r0x100E
                                           	BANKSEL	r0x100F
0006a1   51d7     MOV	0xd7, R0             	MOV	r0x100F, R0
                                           	BANKSEL	r0x100D
0006a2   0ed6     MOVZ	R0, 0xd6            	MOVZ	R0, r0x100D
                                           	BANKSEL	r0x1010
0006a3   51d8     MOV	0xd8, R0             	MOV	r0x1010, R0
                                           ;	op : -
0006a4   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x100E
0006a5   21d5     ADD	0xd5, R0             	ADD	r0x100E, R0
0006a6   7003     JNB	0x3, 0               	JNB	PSW, 0
0006a7   c6a9     JMP	#0x6a9               	JMP	_00040_DS_
                                           	BANKSEL	r0x100D
0006a8   07d6     DEC	0xd6                 	DEC	r0x100D
                                           ;	op : IFX
                                           _00040_DS_
                                           	BANKSEL	r0x100F
0006a9   0ed7     MOVZ	R0, 0xd7            	MOVZ	R0, r0x100F
                                           	BANKSEL	r0x1010
0006aa   30d8     ORL	R0, 0xd8             	ORL	R0, r0x1010
0006ab   7a03     JB	0x3, 2                	JB	PSW, 2
0006ac   c6a0     JMP	#0x6a0               	JMP	_00016_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
0006ad   0008     CRET                     	CRET	
                                           ; exit point of _delay_us
                                           
                                           
                                           
                                           func._delay_ms	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _delay_ms	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;7 compiler assigned registers:
                                           ;   r0x1003
                                           ;   STK00
                                           ;   r0x1004
                                           ;   r0x1005
                                           ;   r0x1006
                                           ;   r0x1007
                                           ;   r0x1008
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _delay_ms	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	69; "../main.c"	void delay_ms(uint ms_data)
000616   6503     CLR	0x3, 5               	BANKSEL	r0x1003
000617   51d0     MOV	0xd0, R0             	MOV	r0x1003, R0
                                           	BANKSEL	STK00
000618   0e9c     MOVZ	R0, 0x9c            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1004
000619   51cf     MOV	0xcf, R0             	MOV	r0x1004, R0
                                           ;	op : =
                                           ;	op : LABEL
                                           ;	op : =
                                           _00006_DS_
                                           ;	.line	72; "../main.c"	while(ms_data--)
                                           	BANKSEL	r0x1004
00061a   0ecf     MOVZ	R0, 0xcf            	MOVZ	R0, r0x1004
                                           	BANKSEL	r0x1005
00061b   51d1     MOV	0xd1, R0             	MOV	r0x1005, R0
                                           	BANKSEL	r0x1003
00061c   0ed0     MOVZ	R0, 0xd0            	MOVZ	R0, r0x1003
                                           	BANKSEL	r0x1006
00061d   51d2     MOV	0xd2, R0             	MOV	r0x1006, R0
                                           ;	op : -
00061e   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x1004
00061f   21cf     ADD	0xcf, R0             	ADD	r0x1004, R0
000620   7003     JNB	0x3, 0               	JNB	PSW, 0
000621   c623     JMP	#0x623               	JMP	_00041_DS_
                                           	BANKSEL	r0x1003
000622   07d0     DEC	0xd0                 	DEC	r0x1003
                                           ;	op : IFX
                                           _00041_DS_
                                           	BANKSEL	r0x1005
000623   0ed1     MOVZ	R0, 0xd1            	MOVZ	R0, r0x1005
                                           	BANKSEL	r0x1006
000624   30d2     ORL	R0, 0xd2             	ORL	R0, r0x1006
000625   7203     JNB	0x3, 2               	JNB	PSW, 2
000626   c63a     JMP	#0x63a               	JMP	_00009_DS_
                                           ;	op : INLINEASM
000627   0064     CWDT                     	CWDT 
                                           ;	op : =
                                           ;	.line	76; "../main.c"	while(j--)
000628   98c8     MOV	R0, #0xc8            	MOV	R0,# 0xc8
                                           	BANKSEL	r0x1005
000629   51d1     MOV	0xd1, R0             	MOV	r0x1005, R0
                                           	BANKSEL	r0x1006
00062a   03d2     CLR	0xd2                 	CLR	r0x1006
                                           ;	op : LABEL
                                           ;	op : =
                                           _00003_DS_
                                           	BANKSEL	r0x1005
00062b   0ed1     MOVZ	R0, 0xd1            	MOVZ	R0, r0x1005
                                           	BANKSEL	r0x1007
00062c   51d3     MOV	0xd3, R0             	MOV	r0x1007, R0
                                           	BANKSEL	r0x1006
00062d   0ed2     MOVZ	R0, 0xd2            	MOVZ	R0, r0x1006
                                           	BANKSEL	r0x1008
00062e   51d4     MOV	0xd4, R0             	MOV	r0x1008, R0
                                           ;	op : -
00062f   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x1005
000630   21d1     ADD	0xd1, R0             	ADD	r0x1005, R0
000631   7003     JNB	0x3, 0               	JNB	PSW, 0
000632   c634     JMP	#0x634               	JMP	_00042_DS_
                                           	BANKSEL	r0x1006
000633   07d2     DEC	0xd2                 	DEC	r0x1006
                                           ;	op : IFX
                                           _00042_DS_
                                           	BANKSEL	r0x1007
000634   0ed3     MOVZ	R0, 0xd3            	MOVZ	R0, r0x1007
                                           	BANKSEL	r0x1008
000635   30d4     ORL	R0, 0xd4             	ORL	R0, r0x1008
000636   7203     JNB	0x3, 2               	JNB	PSW, 2
000637   c61a     JMP	#0x61a               	JMP	_00006_DS_
                                           ;	op : INLINEASM
000638   0064     CWDT                     	CWDT 
                                           ;	op : GOTO
000639   c62b     JMP	#0x62b               	JMP	_00003_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00009_DS_
00063a   0008     CRET                     	CRET	
                                           ; exit point of _delay_ms
                                           
                                           
                                           
                                           func._display	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _display	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _display	;Function start
                                           ; 2 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ;	.line	53; "../main.c"	if(_KF8_LIBi_channel_flag_&0x0020)		//Í¨µÀ5
0006cb   0008     CRET                     	CRET	
                                           ; exit point of _display
                                           
                                           
                                           ;	code size estimation:
                                           ;	  123+   48 =   171 instructions (  438 byte)
                                           
                                           
                                           	.end
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8S1011 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           P4                .EQU                0x09
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           PWMCTL            .EQU                0x15
                                           CMCTL1            .EQU                0x1A
                                           VRECAL            .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           OPTR              .EQU                0x21
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           TR3               .EQU                0x28
                                           TR4               .EQU                0x29
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           BADDRH            .EQU                0x3A
                                           BADDRL            .EQU                0x3B
                                           EECTL1            .EQU                0x3C
                                           EECTL2            .EQU                0x3D
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T3L               .EQU                0x50
                                           CTCTL             .EQU                0x53
                                           RSCTL             .EQU                0x58
                                           TXSDR             .EQU                0x59
                                           RXSDR             .EQU                0x5A
                                           OSCLDOCAL         .EQU                0x5E
                                           T1U               .EQU                0x5F
                                           BRCTL             .EQU                0x77
                                           TSCTL             .EQU                0x78
                                           EUBRGL            .EQU                0x79
                                           EUBRGH            .EQU                0x7A
                                            
                                            
                                           
                                           ;Address:0x03 PSW Bits------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;Address:0x05 P0 Bits-------------------
                                           P07                .EQU                7
                                           P06                .EQU                6
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P07               .EQU                7
                                           _P06               .EQU                6
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;Address:0x06 P2 Bits-------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;Address:0x07 P1 Bits-------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           
                                           ;Address:0x08 P3 Bits-------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;Address:0x09 P4 Bits-------------------
                                           P43                .EQU                3
                                           _P43               .EQU                3
                                           
                                           ;Address:0x0B INTCTL Bits---------------
                                           AIE                .EQU                7
                                           PUIE               .EQU                6
                                           T0IE               .EQU                5
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _PUIE              .EQU                6
                                           _T0IE              .EQU                5
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _P0IF              .EQU                0
                                           
                                           ;Address:0x0C EIF1 Bits-----------------
                                           CTIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _CTIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;Address:0x0D EIF2 Bits-----------------
                                           RXIF               .EQU                5
                                           TXIF               .EQU                4
                                           _RXIF              .EQU                5
                                           _TXIF              .EQU                4
                                           
                                           ;Address:0x10 T1CTL Bits----------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;Address:0x15 PWMCTL Bits---------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           
                                           ;Address:0x1A CMCTL1 Bits---------------
                                           CTCLKSEL1          .EQU                7
                                           CTCLKSEL0          .EQU                6
                                           CTVREFSEL1         .EQU                5
                                           CTVREFSEL0         .EQU                4
                                           _CTCLKSEL1         .EQU                7
                                           _CTCLKSEL0         .EQU                6
                                           _CTVREFSEL1        .EQU                5
                                           _CTVREFSEL0        .EQU                4
                                           
                                           ;Address:0x1D ANSEH Bits----------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           
                                           ;Address:0x1F ADCCTL0 Bits--------------
                                           ADLR               .EQU                7
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;Address:0x21 OPTR Bits-----------------
                                           PUPH               .EQU                7
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;Address:0x25 TR0 Bits------------------
                                           TR07               .EQU                7
                                           TR06               .EQU                6
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR07              .EQU                7
                                           _TR06              .EQU                6
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;Address:0x26 TR2 Bits------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;Address:0x27 TR1 Bits------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           
                                           ;Address:0x28 TR3 Bits------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;Address:0x29 TR4 Bits------------------
                                           TR43               .EQU                3
                                           _TR43              .EQU                3
                                           
                                           ;Address:0x2C EIE1 Bits-----------------
                                           CTIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _CTIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;Address:0x2D EIE2 Bits-----------------
                                           RXIE               .EQU                5
                                           TXIE               .EQU                4
                                           _RXIE              .EQU                5
                                           _TXIE              .EQU                4
                                           
                                           ;Address:0x2E PCTL Bits-----------------
                                           VREEN              .EQU                7
                                           VREOE              .EQU                6
                                           SLVREN             .EQU                4
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _VREEN             .EQU                7
                                           _VREOE             .EQU                6
                                           _SLVREN            .EQU                4
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;Address:0x2F OSCCTL Bits---------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;Address:0x31 ANSEL Bits----------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;Address:0x35 PUR Bits------------------
                                           PUR7               .EQU                7
                                           PUR6               .EQU                6
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR7              .EQU                7
                                           _PUR6              .EQU                6
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;Address:0x36 IOCL Bits-----------------
                                           IOCL7              .EQU                7
                                           IOCL6              .EQU                6
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL7             .EQU                7
                                           _IOCL6             .EQU                6
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;Address:0x3F ADCCTL1 Bits--------------
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           
                                           ;Address:0x50 T3L Bits------------------
                                           T3L7               .EQU                7
                                           T3L6               .EQU                6
                                           T3L5               .EQU                5
                                           T3L4               .EQU                4
                                           T3L3               .EQU                3
                                           T3L2               .EQU                2
                                           T3L1               .EQU                1
                                           T3L0               .EQU                0
                                           _T3L7              .EQU                7
                                           _T3L6              .EQU                6
                                           _T3L5              .EQU                5
                                           _T3L4              .EQU                4
                                           _T3L3              .EQU                3
                                           _T3L2              .EQU                2
                                           _T3L1              .EQU                1
                                           _T3L0              .EQU                0
                                           
                                           ;Address:0x53 CTCTL Bits----------------
                                           CTEN               .EQU                7
                                           CTSTART            .EQU                6
                                           CTCAPS             .EQU                5
                                           CTCMS              .EQU                4
                                           CTCHSEL4           .EQU                4
                                           CTCHSEL3           .EQU                3
                                           CTCHSEL2           .EQU                2
                                           CTCHSEL1           .EQU                1
                                           CTCHSEL0           .EQU                0
                                           _CTEN              .EQU                7
                                           _CTSTART           .EQU                6
                                           _CTCAPS            .EQU                5
                                           _CTCMS             .EQU                4
                                           _CTCHSEL4          .EQU                4
                                           _CTCHSEL3          .EQU                3
                                           _CTCHSEL2          .EQU                2
                                           _CTCHSEL1          .EQU                1
                                           _CTCHSEL0          .EQU                0
                                           
                                           ;Address:0x58 RSCTL Bits----------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;Address:0x5E OSCLDOCAL Bits------------
                                           
                                           ;Address:0x77 BRCTL Bits----------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                4
                                           BRG16              .EQU                3
                                           WUEN               .EQU                1
                                           ADRBEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                4
                                           _BRG16             .EQU                3
                                           _WUEN              .EQU                1
                                           _ADRBEN            .EQU                0
                                           
                                           ;Address:0x78 TSCTL Bits----------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;Address:0x79 EUBRGL Bits---------------
                                           BRG7               .EQU                7
                                           BRG6               .EQU                6
                                           BRG5               .EQU                5
                                           BRG4               .EQU                4
                                           BRG3               .EQU                3
                                           BRG2               .EQU                2
                                           BRG1               .EQU                1
                                           BRG0               .EQU                0
                                           _BRG7              .EQU                7
                                           _BRG6              .EQU                6
                                           _BRG5              .EQU                5
                                           _BRG4              .EQU                4
                                           _BRG3              .EQU                3
                                           _BRG2              .EQU                2
                                           _BRG1              .EQU                1
                                           _BRG0              .EQU                0
                                           
                                           ;Address:0x7A EUBRGH Bits---------------
                                           BRG15              .EQU                7
                                           BRG14              .EQU                6
                                           BRG13              .EQU                5
                                           BRG12              .EQU                4
                                           BRG11              .EQU                3
                                           BRG10              .EQU                2
                                           BRG9               .EQU                1
                                           BRG8               .EQU                0
                                           _BRG15             .EQU                7
                                           _BRG14             .EQU                6
                                           _BRG13             .EQU                5
                                           _BRG12             .EQU                4
                                           _BRG11             .EQU                3
                                           _BRG10             .EQU                2
                                           _BRG9              .EQU                1
                                           _BRG8              .EQU                0
                                            
                                            
                                           .config
002007   04c0     CPLR	0xc0               
002008   ffff     NOPZ                    
                                           .code
0005ef   a800     XOR	R0, #0              
0005f0   7203     JNB	0x3, 2              
0005f1   c5f6     JMP	#0x5f6              
0005f2   a880     XOR	R0, #0x80           
0005f3   7203     JNB	0x3, 2              
0005f4   c5fe     JMP	#0x5fe              
0005f5   c602     JMP	#0x602              
0005f6   6503     CLR	0x3, 5              
0005f7   529b     MOV	R1, 0x9b            
0005f8   509c     MOV	R0, 0x9c            
0005f9   5196     MOV	0x96, R0            
0005fa   7096     JNB	0x96, 0             
0005fb   6d03     SET	0x3, 5              
0005fc   f708     LD	R0, [R1]             
0005fd   c602     JMP	#0x602              
0005fe   6503     CLR	0x3, 5              
0005ff   529c     MOV	R1, 0x9c            
000600   509b     MOV	R0, 0x9b            
000601   d603     CALL	#0x603             
000602   0008     CRET                    
000603   530a     MOV	0xa, R1             
000604   5102     MOV	0x2, R0             
000605   dfff     CALL	#0xfff             
000606   5130     MOV	0x30, R0            
000607   ffff     NOPZ                    
000608   ffff     NOPZ                    
000609   dffe     CALL	#0xffe             
00060a   5137     MOV	0x37, R0            
00060b   ffff     NOPZ                    
00060c   ffff     NOPZ                    
00060d   dffd     CALL	#0xffd             
00060e   511c     MOV	0x1c, R0            
00060f   ffff     NOPZ                    
000610   ffff     NOPZ                    
000611   dffc     CALL	#0xffc             
000612   515e     MOV	0x5e, R0            
000613   ffff     NOPZ                    
000614   ffff     NOPZ                    
000615   0008     CRET                    
                                           func.__sdcc_gsinit_startup
0006be   d65b     CALL	#0x65b             
0006bf   0008     CRET                    
                                           ID_kf8s_touch_g_lib_1
00063b   b001     RRET	R0, #0x1           
00063c   b000     RRET	R0, #0             
00063d   b002     RRET	R0, #0x2           
00063e   b000     RRET	R0, #0             
00063f   b004     RRET	R0, #0x4           
000640   b000     RRET	R0, #0             
000641   b008     RRET	R0, #0x8           
000642   b000     RRET	R0, #0             
000643   b010     RRET	R0, #0x10          
000644   b000     RRET	R0, #0             
000645   b020     RRET	R0, #0x20          
000646   b000     RRET	R0, #0             
000647   b040     RRET	R0, #0x40          
000648   b000     RRET	R0, #0             
000649   b080     RRET	R0, #0x80          
00064a   b000     RRET	R0, #0             
00064b   b000     RRET	R0, #0             
00064c   b001     RRET	R0, #0x1           
00064d   b000     RRET	R0, #0             
00064e   b002     RRET	R0, #0x2           
00064f   b000     RRET	R0, #0             
000650   b004     RRET	R0, #0x4           
000651   b000     RRET	R0, #0             
000652   b008     RRET	R0, #0x8           
000653   b000     RRET	R0, #0             
000654   b010     RRET	R0, #0x10          
000655   b000     RRET	R0, #0             
000656   b020     RRET	R0, #0x20          
000657   b000     RRET	R0, #0             
000658   b040     RRET	R0, #0x40          
000659   b000     RRET	R0, #0             
00065a   b080     RRET	R0, #0x80          
                                           func.__KF8S_Touch_Process_General_
0004b4   6003     CLR	0x3, 0              
0004b5   6503     CLR	0x3, 5              
0004b6   12cd     RLCR	0xcd               
0004b7   51e7     MOV	0xe7, R0            
0004b8   7c53     JB	0x53, 4              
0004b9   c4c1     JMP	#0x4c1              
0004ba   525f     MOV	R1, 0x5f            
0004bb   77dd     JNB	0xdd, 7             
0004bc   c4bf     JMP	#0x4bf              
0004bd   6003     CLR	0x3, 0              
0004be   ff21     RRC	R1                  
0004bf   5050     MOV	R0, 0x50            
0004c0   c4c3     JMP	#0x4c3              
0004c1   520f     MOV	R1, 0xf             
0004c2   500e     MOV	R0, 0xe             
0004c3   53c4     MOV	0xc4, R1            
0004c4   51c3     MOV	0xc3, R0            
0004c5   9802     MOV	R0, #0x2            
0004c6   21c3     ADD	0xc3, R0            
0004c7   7003     JNB	0x3, 0              
0004c8   0bc4     INC	0xc4                
0004c9   9802     MOV	R0, #0x2            
0004ca   ff10     INC	R0                  
0004cb   c4cf     JMP	#0x4cf              
0004cc   6003     CLR	0x3, 0              
0004cd   11c4     RRC	0xc4                
0004ce   11c3     RRC	0xc3                
0004cf   ff58     DECJZ	R0                
0004d0   c4cc     JMP	#0x4cc              
0004d1   50e7     MOV	R0, 0xe7            
0004d2   809d     ADD	R0, #0x9d           
0004d3   f701     LD	R1, [R0]             
0004d4   53c5     MOV	0xc5, R1            
0004d5   ff10     INC	R0                  
0004d6   f701     LD	R1, [R0]             
0004d7   53c6     MOV	0xc6, R1            
0004d8   50c5     MOV	R0, 0xc5            
0004d9   51c7     MOV	0xc7, R0            
0004da   53c8     MOV	0xc8, R1            
0004db   9802     MOV	R0, #0x2            
0004dc   21c7     ADD	0xc7, R0            
0004dd   7003     JNB	0x3, 0              
0004de   0bc8     INC	0xc8                
0004df   9802     MOV	R0, #0x2            
0004e0   ff10     INC	R0                  
0004e1   c4e5     JMP	#0x4e5              
0004e2   6003     CLR	0x3, 0              
0004e3   11c8     RRC	0xc8                
0004e4   11c7     RRC	0xc7                
0004e5   ff58     DECJZ	R0                
0004e6   c4e2     JMP	#0x4e2              
0004e7   50c7     MOV	R0, 0xc7            
0004e8   52c8     MOV	R1, 0xc8            
0004e9   39c5     SUB	0xc5, R0            
0004ea   7803     JB	0x3, 0               
0004eb   07c6     DEC	0xc6                
0004ec   3bc6     SUB	0xc6, R1            
0004ed   52c4     MOV	R1, 0xc4            
0004ee   50c3     MOV	R0, 0xc3            
0004ef   21c5     ADD	0xc5, R0            
0004f0   7003     JNB	0x3, 0              
0004f1   ff11     INC	R1                  
0004f2   23c6     ADD	0xc6, R1            
0004f3   52c5     MOV	R1, 0xc5            
0004f4   50e7     MOV	R0, 0xe7            
0004f5   809d     ADD	R0, #0x9d           
0004f6   f748     ST	[R0], R1             
0004f7   52c6     MOV	R1, 0xc6            
0004f8   ff10     INC	R0                  
0004f9   f748     ST	[R0], R1             
0004fa   70dd     JNB	0xdd, 0             
0004fb   c51b     JMP	#0x51b              
0004fc   50e7     MOV	R0, 0xe7            
0004fd   809d     ADD	R0, #0x9d           
0004fe   f701     LD	R1, [R0]             
0004ff   50e7     MOV	R0, 0xe7            
000500   80a5     ADD	R0, #0xa5           
000501   f748     ST	[R0], R1             
000502   50e7     MOV	R0, 0xe7            
000503   809e     ADD	R0, #0x9e           
000504   f701     LD	R1, [R0]             
000505   50e7     MOV	R0, 0xe7            
000506   80a6     ADD	R0, #0xa6           
000507   f748     ST	[R0], R1             
000508   50cd     MOV	R0, 0xcd            
000509   80b1     ADD	R0, #0xb1           
00050a   9900     MOV	R1, #0              
00050b   f748     ST	[R0], R1             
00050c   50cd     MOV	R0, 0xcd            
00050d   80ad     ADD	R0, #0xad           
00050e   9900     MOV	R1, #0              
00050f   f748     ST	[R0], R1             
000510   9800     MOV	R0, #0              
000511   30cd     ORL	R0, 0xcd            
000512   7a03     JB	0x3, 2               
000513   c522     JMP	#0x522              
000514   0be5     INC	0xe5                
000515   9824     MOV	R0, #0x24           
000516   38e5     SUB	R0, 0xe5            
000517   7803     JB	0x3, 0               
000518   c51a     JMP	#0x51a              
000519   68dd     SET	0xdd, 0             
00051a   c522     JMP	#0x522              
00051b   d2b5     CALL	#0x2b5             
00051c   9800     MOV	R0, #0              
00051d   6503     CLR	0x3, 5              
00051e   30cd     ORL	R0, 0xcd            
00051f   7a03     JB	0x3, 2               
000520   c522     JMP	#0x522              
000521   d009     CALL	#0x9               
000522   9906     MOV	R1, #0x6            
000523   98c0     MOV	R0, #0xc0           
000524   d6b9     CALL	#0x6b9             
000525   6503     CLR	0x3, 5              
000526   0bcd     INC	0xcd                
000527   18cd     XOR	R0, 0xcd            
000528   7203     JNB	0x3, 2              
000529   03cd     CLR	0xcd                
00052a   7453     JNB	0x53, 4             
00052b   c530     JMP	#0x530              
00052c   030e     CLR	0xe                 
00052d   030f     CLR	0xf                 
00052e   0300     CLR	0                   
00052f   c531     JMP	#0x531              
000530   0350     CLR	0x50                
000531   6003     CLR	0x3, 0              
000532   50cd     MOV	R0, 0xcd            
000533   80ae     ADD	R0, #0xae           
000534   9906     MOV	R1, #0x6            
000535   7003     JNB	0x3, 0              
000536   ff11     INC	R1                  
000537   d6b9     CALL	#0x6b9             
000538   99f0     MOV	R1, #0xf0           
000539   6503     CLR	0x3, 5              
00053a   2b53     AND	0x53, R1            
00053b   3153     ORL	0x53, R0            
00053c   9801     MOV	R0, #0x1            
00053d   ff58     DECJZ	R0                
00053e   c53d     JMP	#0x53d              
00053f   6e53     SET	0x53, 6             
000540   0000     NOP                     
000541   7e53     JB	0x53, 6              
000542   c53f     JMP	#0x53f              
000543   7453     JNB	0x53, 4             
000544   035f     CLR	0x5f                
000545   6f2c     SET	0x2c, 7             
000546   670c     CLR	0xc, 7              
000547   0008     CRET                    
                                           func.__KF8_LIBf_scan_channel_
0002b5   6003     CLR	0x3, 0              
0002b6   6503     CLR	0x3, 5              
0002b7   12cd     RLCR	0xcd               
0002b8   51e7     MOV	0xe7, R0            
0002b9   9801     MOV	R0, #0x1            
0002ba   51c3     MOV	0xc3, R0            
0002bb   03c4     CLR	0xc4                
0002bc   50cd     MOV	R0, 0xcd            
0002bd   ff10     INC	R0                  
0002be   c2c3     JMP	#0x2c3              
0002bf   6003     CLR	0x3, 0              
0002c0   6503     CLR	0x3, 5              
0002c1   13c3     RLC	0xc3                
0002c2   13c4     RLC	0xc4                
0002c3   ff58     DECJZ	R0                
0002c4   c2bf     JMP	#0x2bf              
0002c5   52e7     MOV	R1, 0xe7            
0002c6   819d     ADD	R1, #0x9d           
0002c7   f708     LD	R0, [R1]             
0002c8   51c5     MOV	0xc5, R0            
0002c9   ff11     INC	R1                  
0002ca   f708     LD	R0, [R1]             
0002cb   51c6     MOV	0xc6, R0            
0002cc   52e7     MOV	R1, 0xe7            
0002cd   81a5     ADD	R1, #0xa5           
0002ce   f708     LD	R0, [R1]             
0002cf   51c7     MOV	0xc7, R0            
0002d0   ff11     INC	R1                  
0002d1   f708     LD	R0, [R1]             
0002d2   51c8     MOV	0xc8, R0            
0002d3   d548     CALL	#0x548             
0002d4   9906     MOV	R1, #0x6            
0002d5   98c7     MOV	R0, #0xc7           
0002d6   d6b9     CALL	#0x6b9             
0002d7   8080     ADD	R0, #0x80           
0002d8   6503     CLR	0x3, 5              
0002d9   9980     MOV	R1, #0x80           
0002da   22e4     ADD	R1, 0xe4            
0002db   f848     SUB	R0, R1              
0002dc   7803     JB	0x3, 0               
0002dd   c2e7     JMP	#0x2e7              
0002de   50c1     MOV	R0, 0xc1            
0002df   28c3     AND	R0, 0xc3            
0002e0   7a03     JB	0x3, 2               
0002e1   c2e7     JMP	#0x2e7              
0002e2   50c2     MOV	R0, 0xc2            
0002e3   28c4     AND	R0, 0xc4            
0002e4   7a03     JB	0x3, 2               
0002e5   c2e7     JMP	#0x2e7              
0002e6   0be3     INC	0xe3                
0002e7   52cd     MOV	R1, 0xcd            
0002e8   81b5     ADD	R1, #0xb5           
0002e9   f708     LD	R0, [R1]             
0002ea   52e4     MOV	R1, 0xe4            
0002eb   53e6     MOV	0xe6, R1            
0002ec   39e6     SUB	0xe6, R0            
0002ed   7fe6     JB	0xe6, 7              
0002ee   c2f1     JMP	#0x2f1              
0002ef   05e6     CPL	0xe6                
0002f0   0be6     INC	0xe6                
0002f1   9906     MOV	R1, #0x6            
0002f2   98c8     MOV	R0, #0xc8           
0002f3   d6b9     CALL	#0x6b9             
0002f4   6503     CLR	0x3, 5              
0002f5   38e6     SUB	R0, 0xe6            
0002f6   7803     JB	0x3, 0               
0002f7   c2fc     JMP	#0x2fc              
0002f8   50cd     MOV	R0, 0xcd            
0002f9   80ad     ADD	R0, #0xad           
0002fa   9900     MOV	R1, #0              
0002fb   f748     ST	[R0], R1             
0002fc   50cd     MOV	R0, 0xcd            
0002fd   80b5     ADD	R0, #0xb5           
0002fe   51e8     MOV	0xe8, R0            
0002ff   0ee4     MOVZ	R0, 0xe4           
000300   52e8     MOV	R1, 0xe8            
000301   f741     ST	[R1], R0             
000302   50cd     MOV	R0, 0xcd            
000303   a801     XOR	R0, #0x1            
000304   7a03     JB	0x3, 2               
000305   c314     JMP	#0x314              
000306   50b5     MOV	R0, 0xb5            
000307   52b6     MOV	R1, 0xb6            
000308   8080     ADD	R0, #0x80           
000309   8180     ADD	R1, #0x80           
00030a   f841     SUB	R1, R0              
00030b   7803     JB	0x3, 0               
00030c   c311     JMP	#0x311              
00030d   9801     MOV	R0, #0x1            
00030e   51e2     MOV	0xe2, R0            
00030f   03e1     CLR	0xe1                
000310   c314     JMP	#0x314              
000311   9801     MOV	R0, #0x1            
000312   51e1     MOV	0xe1, R0            
000313   03e2     CLR	0xe2                
000314   9802     MOV	R0, #0x2            
000315   38cd     SUB	R0, 0xcd            
000316   7803     JB	0x3, 0               
000317   c332     JMP	#0x332              
000318   52cd     MOV	R1, 0xcd            
000319   81b5     ADD	R1, #0xb5           
00031a   f708     LD	R0, [R1]             
00031b   8080     ADD	R0, #0x80           
00031c   51e4     MOV	0xe4, R0            
00031d   52e2     MOV	R1, 0xe2            
00031e   81b5     ADD	R1, #0xb5           
00031f   f708     LD	R0, [R1]             
000320   8080     ADD	R0, #0x80           
000321   38e4     SUB	R0, 0xe4            
000322   7803     JB	0x3, 0               
000323   c332     JMP	#0x332              
000324   52e1     MOV	R1, 0xe1            
000325   81b5     ADD	R1, #0xb5           
000326   f708     LD	R0, [R1]             
000327   8080     ADD	R0, #0x80           
000328   38e4     SUB	R0, 0xe4            
000329   7003     JNB	0x3, 0              
00032a   c32e     JMP	#0x32e              
00032b   50cd     MOV	R0, 0xcd            
00032c   51e2     MOV	0xe2, R0            
00032d   c332     JMP	#0x332              
00032e   50e1     MOV	R0, 0xe1            
00032f   51e2     MOV	0xe2, R0            
000330   50cd     MOV	R0, 0xcd            
000331   51e1     MOV	0xe1, R0            
000332   71dd     JNB	0xdd, 1             
000333   c3bb     JMP	#0x3bb              
000334   50cd     MOV	R0, 0xcd            
000335   80b2     ADD	R0, #0xb2           
000336   9906     MOV	R1, #0x6            
000337   7003     JNB	0x3, 0              
000338   ff11     INC	R1                  
000339   d6b9     CALL	#0x6b9             
00033a   6503     CLR	0x3, 5              
00033b   51e4     MOV	0xe4, R0            
00033c   9806     MOV	R0, #0x6            
00033d   39e4     SUB	0xe4, R0            
00033e   50cd     MOV	R0, 0xcd            
00033f   80b5     ADD	R0, #0xb5           
000340   51e8     MOV	0xe8, R0            
000341   52e8     MOV	R1, 0xe8            
000342   f708     LD	R0, [R1]             
000343   51e9     MOV	0xe9, R0            
000344   0ee9     MOVZ	R0, 0xe9           
000345   8080     ADD	R0, #0x80           
000346   51ed     MOV	0xed, R0            
000347   0ee4     MOVZ	R0, 0xe4           
000348   8080     ADD	R0, #0x80           
000349   38ed     SUB	R0, 0xed            
00034a   7003     JNB	0x3, 0              
00034b   c3ac     JMP	#0x3ac              
00034c   50cd     MOV	R0, 0xcd            
00034d   80b1     ADD	R0, #0xb1           
00034e   51e8     MOV	0xe8, R0            
00034f   52e8     MOV	R1, 0xe8            
000350   f708     LD	R0, [R1]             
000351   51e9     MOV	0xe9, R0            
000352   9906     MOV	R1, #0x6            
000353   98c1     MOV	R0, #0xc1           
000354   d603     CALL	#0x603             
000355   6503     CLR	0x3, 5              
000356   51e8     MOV	0xe8, R0            
000357   0ee9     MOVZ	R0, 0xe9           
000358   38e8     SUB	R0, 0xe8            
000359   7003     JNB	0x3, 0              
00035a   c3bb     JMP	#0x3bb              
00035b   9906     MOV	R1, #0x6            
00035c   98c1     MOV	R0, #0xc1           
00035d   d6b9     CALL	#0x6b9             
00035e   6003     CLR	0x3, 0              
00035f   ff18     RLC	R0                  
000360   6503     CLR	0x3, 5              
000361   51e5     MOV	0xe5, R0            
000362   52cd     MOV	R1, 0xcd            
000363   81b1     ADD	R1, #0xb1           
000364   f708     LD	R0, [R1]             
000365   38e5     SUB	R0, 0xe5            
000366   7803     JB	0x3, 0               
000367   c36c     JMP	#0x36c              
000368   f708     LD	R0, [R1]             
000369   ff10     INC	R0                  
00036a   f741     ST	[R1], R0             
00036b   c3ab     JMP	#0x3ab              
00036c   0208     CLR	R0                  
00036d   f741     ST	[R1], R0             
00036e   50cd     MOV	R0, 0xcd            
00036f   80ae     ADD	R0, #0xae           
000370   9906     MOV	R1, #0x6            
000371   7003     JNB	0x3, 0              
000372   ff11     INC	R1                  
000373   d6b9     CALL	#0x6b9             
000374   6003     CLR	0x3, 0              
000375   ff18     RLC	R0                  
000376   6503     CLR	0x3, 5              
000377   51e5     MOV	0xe5, R0            
000378   803b     ADD	R0, #0x3b           
000379   9906     MOV	R1, #0x6            
00037a   7003     JNB	0x3, 0              
00037b   ff11     INC	R1                  
00037c   d6b9     CALL	#0x6b9             
00037d   ff00     CPL	R0                  
00037e   6503     CLR	0x3, 5              
00037f   29b9     AND	0xb9, R0            
000380   50e5     MOV	R0, 0xe5            
000381   ff10     INC	R0                  
000382   803b     ADD	R0, #0x3b           
000383   9906     MOV	R1, #0x6            
000384   7003     JNB	0x3, 0              
000385   ff11     INC	R1                  
000386   d6b9     CALL	#0x6b9             
000387   ff00     CPL	R0                  
000388   6503     CLR	0x3, 5              
000389   29ba     AND	0xba, R0            
00038a   9800     MOV	R0, #0              
00038b   30de     ORL	R0, 0xde            
00038c   7a03     JB	0x3, 2               
00038d   07de     DEC	0xde                
00038e   9800     MOV	R0, #0              
00038f   30de     ORL	R0, 0xde            
000390   7203     JNB	0x3, 2              
000391   c3a2     JMP	#0x3a2              
000392   50df     MOV	R0, 0xdf            
000393   18cd     XOR	R0, 0xcd            
000394   7a03     JB	0x3, 2               
000395   c3a4     JMP	#0x3a4              
000396   50e0     MOV	R0, 0xe0            
000397   18df     XOR	R0, 0xdf            
000398   7a03     JB	0x3, 2               
000399   c39f     JMP	#0x39f              
00039a   98ff     MOV	R0, #0xff           
00039b   51df     MOV	0xdf, R0            
00039c   9800     MOV	R0, #0              
00039d   51de     MOV	0xde, R0            
00039e   c3a4     JMP	#0x3a4              
00039f   50e0     MOV	R0, 0xe0            
0003a0   51df     MOV	0xdf, R0            
0003a1   c3a4     JMP	#0x3a4              
0003a2   98ff     MOV	R0, #0xff           
0003a3   51df     MOV	0xdf, R0            
0003a4   98ff     MOV	R0, #0xff           
0003a5   51e0     MOV	0xe0, R0            
0003a6   9800     MOV	R0, #0              
0003a7   51bf     MOV	0xbf, R0            
0003a8   51c0     MOV	0xc0, R0            
0003a9   51bd     MOV	0xbd, R0            
0003aa   51be     MOV	0xbe, R0            
0003ab   c3bb     JMP	#0x3bb              
0003ac   9906     MOV	R1, #0x6            
0003ad   98c1     MOV	R0, #0xc1           
0003ae   d6b9     CALL	#0x6b9             
0003af   ff10     INC	R0                  
0003b0   6503     CLR	0x3, 5              
0003b1   51e5     MOV	0xe5, R0            
0003b2   52cd     MOV	R1, 0xcd            
0003b3   81b1     ADD	R1, #0xb1           
0003b4   f708     LD	R0, [R1]             
0003b5   38e5     SUB	R0, 0xe5            
0003b6   7003     JNB	0x3, 0              
0003b7   c3bb     JMP	#0x3bb              
0003b8   f708     LD	R0, [R1]             
0003b9   ff08     DEC	R0                  
0003ba   f741     ST	[R1], R0             
0003bb   0008     CRET                    
                                           func.__KF8_LiBf_KEY_Deal_AND_BaseLine_Up
000009   9801     MOV	R0, #0x1            
00000a   6503     CLR	0x3, 5              
00000b   51c3     MOV	0xc3, R0            
00000c   03c4     CLR	0xc4                
00000d   03ee     CLR	0xee                
00000e   9906     MOV	R1, #0x6            
00000f   98c0     MOV	R0, #0xc0           
000010   d603     CALL	#0x603             
000011   6503     CLR	0x3, 5              
000012   51e8     MOV	0xe8, R0            
000013   0ee8     MOVZ	R0, 0xe8           
000014   38ee     SUB	R0, 0xee            
000015   7003     JNB	0x3, 0              
000016   c257     JMP	#0x257              
000017   6003     CLR	0x3, 0              
000018   12ee     RLCR	0xee               
000019   51e7     MOV	0xe7, R0            
00001a   50ee     MOV	R0, 0xee            
00001b   80ae     ADD	R0, #0xae           
00001c   9906     MOV	R1, #0x6            
00001d   7003     JNB	0x3, 0              
00001e   ff11     INC	R1                  
00001f   d6b9     CALL	#0x6b9             
000020   6503     CLR	0x3, 5              
000021   51e5     MOV	0xe5, R0            
000022   98ca     MOV	R0, #0xca           
000023   9906     MOV	R1, #0x6            
000024   d6b9     CALL	#0x6b9             
000025   18e5     XOR	R0, 0xe5            
000026   7a03     JB	0x3, 2               
000027   c039     JMP	#0x39               
000028   98c9     MOV	R0, #0xc9           
000029   9906     MOV	R1, #0x6            
00002a   d6b9     CALL	#0x6b9             
00002b   6503     CLR	0x3, 5              
00002c   51e4     MOV	0xe4, R0            
00002d   50ee     MOV	R0, 0xee            
00002e   80b5     ADD	R0, #0xb5           
00002f   f701     LD	R1, [R0]             
000030   f7f9     JB	R1, 7                
000031   c034     JMP	#0x34               
000032   ff01     CPL	R1                  
000033   ff11     INC	R1                  
000034   3ae4     SUB	R1, 0xe4            
000035   7003     JNB	0x3, 0              
000036   c039     JMP	#0x39               
000037   69dd     SET	0xdd, 1             
000038   03dc     CLR	0xdc                
000039   6503     CLR	0x3, 5              
00003a   50ee     MOV	R0, 0xee            
00003b   80b5     ADD	R0, #0xb5           
00003c   51e8     MOV	0xe8, R0            
00003d   52e8     MOV	R1, 0xe8            
00003e   f708     LD	R0, [R1]             
00003f   51e9     MOV	0xe9, R0            
000040   9906     MOV	R1, #0x6            
000041   98c6     MOV	R0, #0xc6           
000042   d603     CALL	#0x603             
000043   6503     CLR	0x3, 5              
000044   51e8     MOV	0xe8, R0            
000045   0ee9     MOVZ	R0, 0xe9           
000046   8080     ADD	R0, #0x80           
000047   51ed     MOV	0xed, R0            
000048   0ee8     MOVZ	R0, 0xe8           
000049   8080     ADD	R0, #0x80           
00004a   38ed     SUB	R0, 0xed            
00004b   7003     JNB	0x3, 0              
00004c   c070     JMP	#0x70               
00004d   50ee     MOV	R0, 0xee            
00004e   80ad     ADD	R0, #0xad           
00004f   f701     LD	R1, [R0]             
000050   9864     MOV	R0, #0x64           
000051   f941     XOR	R1, R0              
000052   7a03     JB	0x3, 2               
000053   c06f     JMP	#0x6f               
000054   50e7     MOV	R0, 0xe7            
000055   809d     ADD	R0, #0x9d           
000056   f701     LD	R1, [R0]             
000057   50e7     MOV	R0, 0xe7            
000058   80a5     ADD	R0, #0xa5           
000059   f748     ST	[R0], R1             
00005a   50e7     MOV	R0, 0xe7            
00005b   809e     ADD	R0, #0x9e           
00005c   f701     LD	R1, [R0]             
00005d   50e7     MOV	R0, 0xe7            
00005e   80a6     ADD	R0, #0xa6           
00005f   f748     ST	[R0], R1             
000060   50ee     MOV	R0, 0xee            
000061   80b1     ADD	R0, #0xb1           
000062   f701     LD	R1, [R0]             
000063   53e5     MOV	0xe5, R1            
000064   98c1     MOV	R0, #0xc1           
000065   9906     MOV	R1, #0x6            
000066   d6b9     CALL	#0x6b9             
000067   38e5     SUB	R0, 0xe5            
000068   7003     JNB	0x3, 0              
000069   c06f     JMP	#0x6f               
00006a   6503     CLR	0x3, 5              
00006b   50ee     MOV	R0, 0xee            
00006c   80b1     ADD	R0, #0xb1           
00006d   9900     MOV	R1, #0              
00006e   f748     ST	[R0], R1             
00006f   c153     JMP	#0x153              
000070   50ee     MOV	R0, 0xee            
000071   80b5     ADD	R0, #0xb5           
000072   51e8     MOV	0xe8, R0            
000073   52e8     MOV	R1, 0xe8            
000074   f708     LD	R0, [R1]             
000075   51ea     MOV	0xea, R0            
000076   9906     MOV	R1, #0x6            
000077   98c7     MOV	R0, #0xc7           
000078   d603     CALL	#0x603             
000079   6503     CLR	0x3, 5              
00007a   51e8     MOV	0xe8, R0            
00007b   0ee8     MOVZ	R0, 0xe8           
00007c   8080     ADD	R0, #0x80           
00007d   51ed     MOV	0xed, R0            
00007e   0eea     MOVZ	R0, 0xea           
00007f   8080     ADD	R0, #0x80           
000080   38ed     SUB	R0, 0xed            
000081   7003     JNB	0x3, 0              
000082   c0e8     JMP	#0xe8               
000083   98c5     MOV	R0, #0xc5           
000084   9906     MOV	R1, #0x6            
000085   d6b9     CALL	#0x6b9             
000086   6503     CLR	0x3, 5              
000087   38e3     SUB	R0, 0xe3            
000088   7803     JB	0x3, 0               
000089   c08c     JMP	#0x8c               
00008a   69dd     SET	0xdd, 1             
00008b   03dc     CLR	0xdc                
00008c   79dd     JB	0xdd, 1              
00008d   c0ac     JMP	#0xac               
00008e   50ee     MOV	R0, 0xee            
00008f   80ad     ADD	R0, #0xad           
000090   f701     LD	R1, [R0]             
000091   a9ec     XOR	R1, #0xec           
000092   7203     JNB	0x3, 2              
000093   c09b     JMP	#0x9b               
000094   98c2     MOV	R0, #0xc2           
000095   9906     MOV	R1, #0x6            
000096   d6b9     CALL	#0x6b9             
000097   6503     CLR	0x3, 5              
000098   18dc     XOR	R0, 0xdc            
000099   7a03     JB	0x3, 2               
00009a   c0ab     JMP	#0xab               
00009b   50e7     MOV	R0, 0xe7            
00009c   809d     ADD	R0, #0x9d           
00009d   f701     LD	R1, [R0]             
00009e   50e7     MOV	R0, 0xe7            
00009f   80a5     ADD	R0, #0xa5           
0000a0   f748     ST	[R0], R1             
0000a1   50e7     MOV	R0, 0xe7            
0000a2   809e     ADD	R0, #0x9e           
0000a3   f701     LD	R1, [R0]             
0000a4   50e7     MOV	R0, 0xe7            
0000a5   80a6     ADD	R0, #0xa6           
0000a6   f748     ST	[R0], R1             
0000a7   50c3     MOV	R0, 0xc3            
0000a8   31c1     ORL	0xc1, R0            
0000a9   50c4     MOV	R0, 0xc4            
0000aa   31c2     ORL	0xc2, R0            
0000ab   c153     JMP	#0x153              
0000ac   50ee     MOV	R0, 0xee            
0000ad   80ad     ADD	R0, #0xad           
0000ae   f701     LD	R1, [R0]             
0000af   53e4     MOV	0xe4, R1            
0000b0   9906     MOV	R1, #0x6            
0000b1   98c4     MOV	R0, #0xc4           
0000b2   d6b9     CALL	#0x6b9             
0000b3   6503     CLR	0x3, 5              
0000b4   18e4     XOR	R0, 0xe4            
0000b5   7a03     JB	0x3, 2               
0000b6   c0e7     JMP	#0xe7               
0000b7   50ee     MOV	R0, 0xee            
0000b8   80b1     ADD	R0, #0xb1           
0000b9   f701     LD	R1, [R0]             
0000ba   53e5     MOV	0xe5, R1            
0000bb   98c1     MOV	R0, #0xc1           
0000bc   9906     MOV	R1, #0x6            
0000bd   d6b9     CALL	#0x6b9             
0000be   6503     CLR	0x3, 5              
0000bf   38e5     SUB	R0, 0xe5            
0000c0   7003     JNB	0x3, 0              
0000c1   c0df     JMP	#0xdf               
0000c2   50de     MOV	R0, 0xde            
0000c3   a802     XOR	R0, #0x2            
0000c4   7a03     JB	0x3, 2               
0000c5   c0d3     JMP	#0xd3               
0000c6   50e7     MOV	R0, 0xe7            
0000c7   809d     ADD	R0, #0x9d           
0000c8   f701     LD	R1, [R0]             
0000c9   50e7     MOV	R0, 0xe7            
0000ca   80a5     ADD	R0, #0xa5           
0000cb   f748     ST	[R0], R1             
0000cc   50e7     MOV	R0, 0xe7            
0000cd   809e     ADD	R0, #0x9e           
0000ce   f701     LD	R1, [R0]             
0000cf   50e7     MOV	R0, 0xe7            
0000d0   80a6     ADD	R0, #0xa6           
0000d1   f748     ST	[R0], R1             
0000d2   c0e3     JMP	#0xe3               
0000d3   50e7     MOV	R0, 0xe7            
0000d4   80a5     ADD	R0, #0xa5           
0000d5   f701     LD	R1, [R0]             
0000d6   81ff     ADD	R1, #0xff           
0000d7   f748     ST	[R0], R1             
0000d8   7003     JNB	0x3, 0              
0000d9   c0e3     JMP	#0xe3               
0000da   ff10     INC	R0                  
0000db   f701     LD	R1, [R0]             
0000dc   ff09     DEC	R1                  
0000dd   f748     ST	[R0], R1             
0000de   c0e3     JMP	#0xe3               
0000df   50c3     MOV	R0, 0xc3            
0000e0   31c1     ORL	0xc1, R0            
0000e1   50c4     MOV	R0, 0xc4            
0000e2   31c2     ORL	0xc2, R0            
0000e3   50ee     MOV	R0, 0xee            
0000e4   80ad     ADD	R0, #0xad           
0000e5   9900     MOV	R1, #0              
0000e6   f748     ST	[R0], R1             
0000e7   c153     JMP	#0x153              
0000e8   71dd     JNB	0xdd, 1             
0000e9   c0ee     JMP	#0xee               
0000ea   04c3     CPLR	0xc3               
0000eb   29c1     AND	0xc1, R0            
0000ec   04c4     CPLR	0xc4               
0000ed   29c2     AND	0xc2, R0            
0000ee   50ee     MOV	R0, 0xee            
0000ef   80ad     ADD	R0, #0xad           
0000f0   f701     LD	R1, [R0]             
0000f1   53e4     MOV	0xe4, R1            
0000f2   98c4     MOV	R0, #0xc4           
0000f3   9906     MOV	R1, #0x6            
0000f4   d6b9     CALL	#0x6b9             
0000f5   6503     CLR	0x3, 5              
0000f6   18e4     XOR	R0, 0xe4            
0000f7   7203     JNB	0x3, 2              
0000f8   c100     JMP	#0x100              
0000f9   9906     MOV	R1, #0x6            
0000fa   98c3     MOV	R0, #0xc3           
0000fb   d6b9     CALL	#0x6b9             
0000fc   6503     CLR	0x3, 5              
0000fd   18e4     XOR	R0, 0xe4            
0000fe   7a03     JB	0x3, 2               
0000ff   c153     JMP	#0x153              
000100   50ee     MOV	R0, 0xee            
000101   80ad     ADD	R0, #0xad           
000102   9900     MOV	R1, #0              
000103   f748     ST	[R0], R1             
000104   50e7     MOV	R0, 0xe7            
000105   80a5     ADD	R0, #0xa5           
000106   f701     LD	R1, [R0]             
000107   53c5     MOV	0xc5, R1            
000108   ff10     INC	R0                  
000109   f701     LD	R1, [R0]             
00010a   53c6     MOV	0xc6, R1            
00010b   9901     MOV	R1, #0x1            
00010c   6003     CLR	0x3, 0              
00010d   11c6     RRC	0xc6                
00010e   11c5     RRC	0xc5                
00010f   6003     CLR	0x3, 0              
000110   ff19     RLC	R1                  
000111   f8c8     MOV	R0, R1              
000112   a808     XOR	R0, #0x8            
000113   7a03     JB	0x3, 2               
000114   c10c     JMP	#0x10c              
000115   50e7     MOV	R0, 0xe7            
000116   809d     ADD	R0, #0x9d           
000117   f701     LD	R1, [R0]             
000118   53c7     MOV	0xc7, R1            
000119   ff10     INC	R0                  
00011a   f701     LD	R1, [R0]             
00011b   53c8     MOV	0xc8, R1            
00011c   9901     MOV	R1, #0x1            
00011d   6003     CLR	0x3, 0              
00011e   11c8     RRC	0xc8                
00011f   11c7     RRC	0xc7                
000120   6003     CLR	0x3, 0              
000121   ff19     RLC	R1                  
000122   f8c8     MOV	R0, R1              
000123   a808     XOR	R0, #0x8            
000124   7a03     JB	0x3, 2               
000125   c11d     JMP	#0x11d              
000126   52c5     MOV	R1, 0xc5            
000127   3bc7     SUB	0xc7, R1            
000128   52c6     MOV	R1, 0xc6            
000129   7803     JB	0x3, 0               
00012a   ff11     INC	R1                  
00012b   3bc8     SUB	0xc8, R1            
00012c   50e7     MOV	R0, 0xe7            
00012d   80a5     ADD	R0, #0xa5           
00012e   f701     LD	R1, [R0]             
00012f   22c7     ADD	R1, 0xc7            
000130   f748     ST	[R0], R1             
000131   ff10     INC	R0                  
000132   f701     LD	R1, [R0]             
000133   7003     JNB	0x3, 0              
000134   ff11     INC	R1                  
000135   22c8     ADD	R1, 0xc8            
000136   f748     ST	[R0], R1             
000137   50ee     MOV	R0, 0xee            
000138   80b5     ADD	R0, #0xb5           
000139   f701     LD	R1, [R0]             
00013a   f7b9     JNB	R1, 7               
00013b   c148     JMP	#0x148              
00013c   50e7     MOV	R0, 0xe7            
00013d   80a5     ADD	R0, #0xa5           
00013e   f701     LD	R1, [R0]             
00013f   81ff     ADD	R1, #0xff           
000140   f748     ST	[R0], R1             
000141   7003     JNB	0x3, 0              
000142   c153     JMP	#0x153              
000143   ff10     INC	R0                  
000144   f701     LD	R1, [R0]             
000145   ff09     DEC	R1                  
000146   f748     ST	[R0], R1             
000147   c153     JMP	#0x153              
000148   50e7     MOV	R0, 0xe7            
000149   80a5     ADD	R0, #0xa5           
00014a   f701     LD	R1, [R0]             
00014b   8101     ADD	R1, #0x1            
00014c   f748     ST	[R0], R1             
00014d   7803     JB	0x3, 0               
00014e   c153     JMP	#0x153              
00014f   ff10     INC	R0                  
000150   f701     LD	R1, [R0]             
000151   ff11     INC	R1                  
000152   f748     ST	[R0], R1             
000153   6503     CLR	0x3, 5              
000154   79dd     JB	0xdd, 1              
000155   c165     JMP	#0x165              
000156   50ee     MOV	R0, 0xee            
000157   80b1     ADD	R0, #0xb1           
000158   f701     LD	R1, [R0]             
000159   53e5     MOV	0xe5, R1            
00015a   9906     MOV	R1, #0x6            
00015b   98c1     MOV	R0, #0xc1           
00015c   d6b9     CALL	#0x6b9             
00015d   6503     CLR	0x3, 5              
00015e   39e5     SUB	0xe5, R0            
00015f   7003     JNB	0x3, 0              
000160   c165     JMP	#0x165              
000161   50ee     MOV	R0, 0xee            
000162   80b1     ADD	R0, #0xb1           
000163   9900     MOV	R1, #0              
000164   f748     ST	[R0], R1             
000165   50ee     MOV	R0, 0xee            
000166   80b5     ADD	R0, #0xb5           
000167   51e8     MOV	0xe8, R0            
000168   52e8     MOV	R1, 0xe8            
000169   f708     LD	R0, [R1]             
00016a   51eb     MOV	0xeb, R0            
00016b   6803     SET	0x3, 0              
00016c   7feb     JB	0xeb, 7              
00016d   6003     CLR	0x3, 0              
00016e   7003     JNB	0x3, 0              
00016f   c176     JMP	#0x176              
000170   50ee     MOV	R0, 0xee            
000171   80ad     ADD	R0, #0xad           
000172   f701     LD	R1, [R0]             
000173   ff09     DEC	R1                  
000174   f748     ST	[R0], R1             
000175   c17b     JMP	#0x17b              
000176   50ee     MOV	R0, 0xee            
000177   80ad     ADD	R0, #0xad           
000178   f701     LD	R1, [R0]             
000179   ff11     INC	R1                  
00017a   f748     ST	[R0], R1             
00017b   71dd     JNB	0xdd, 1             
00017c   c252     JMP	#0x252              
00017d   0ee1     MOVZ	R0, 0xe1           
00017e   18ee     XOR	R0, 0xee            
00017f   7203     JNB	0x3, 2              
000180   c185     JMP	#0x185              
000181   0ee2     MOVZ	R0, 0xe2           
000182   18ee     XOR	R0, 0xee            
000183   7a03     JB	0x3, 2               
000184   c23f     JMP	#0x23f              
000185   50ee     MOV	R0, 0xee            
000186   80b5     ADD	R0, #0xb5           
000187   51e8     MOV	0xe8, R0            
000188   52e8     MOV	R1, 0xe8            
000189   f708     LD	R0, [R1]             
00018a   51eb     MOV	0xeb, R0            
00018b   98b2     MOV	R0, #0xb2           
00018c   20ee     ADD	R0, 0xee            
00018d   51e8     MOV	0xe8, R0            
00018e   9806     MOV	R0, #0x6            
00018f   51ea     MOV	0xea, R0            
000190   0208     CLR	R0                  
000191   7003     JNB	0x3, 0              
000192   ff10     INC	R0                  
000193   7203     JNB	0x3, 2              
000194   c196     JMP	#0x196              
000195   21ea     ADD	0xea, R0            
000196   52ea     MOV	R1, 0xea            
000197   50e8     MOV	R0, 0xe8            
000198   d603     CALL	#0x603             
000199   6503     CLR	0x3, 5              
00019a   51ec     MOV	0xec, R0            
00019b   0eec     MOVZ	R0, 0xec           
00019c   8080     ADD	R0, #0x80           
00019d   51ed     MOV	0xed, R0            
00019e   0eeb     MOVZ	R0, 0xeb           
00019f   8080     ADD	R0, #0x80           
0001a0   38ed     SUB	R0, 0xed            
0001a1   7003     JNB	0x3, 0              
0001a2   c23f     JMP	#0x23f              
0001a3   50ee     MOV	R0, 0xee            
0001a4   80b1     ADD	R0, #0xb1           
0001a5   f701     LD	R1, [R0]             
0001a6   53e5     MOV	0xe5, R1            
0001a7   9906     MOV	R1, #0x6            
0001a8   98c1     MOV	R0, #0xc1           
0001a9   d6b9     CALL	#0x6b9             
0001aa   6503     CLR	0x3, 5              
0001ab   38e5     SUB	R0, 0xe5            
0001ac   7003     JNB	0x3, 0              
0001ad   c1b2     JMP	#0x1b2              
0001ae   0ae5     INCR	0xe5               
0001af   52ee     MOV	R1, 0xee            
0001b0   81b1     ADD	R1, #0xb1           
0001b1   f741     ST	[R1], R0             
0001b2   9900     MOV	R1, #0              
0001b3   9802     MOV	R0, #0x2            
0001b4   d603     CALL	#0x603             
0001b5   6503     CLR	0x3, 5              
0001b6   51e8     MOV	0xe8, R0            
0001b7   9900     MOV	R1, #0              
0001b8   9803     MOV	R0, #0x3            
0001b9   d603     CALL	#0x603             
0001ba   6503     CLR	0x3, 5              
0001bb   51ea     MOV	0xea, R0            
0001bc   0ee8     MOVZ	R0, 0xe8           
0001bd   30ea     ORL	R0, 0xea            
0001be   7203     JNB	0x3, 2              
0001bf   c1dc     JMP	#0x1dc              
0001c0   0ede     MOVZ	R0, 0xde           
0001c1   a801     XOR	R0, #0x1            
0001c2   7a03     JB	0x3, 2               
0001c3   c1dc     JMP	#0x1dc              
0001c4   0eea     MOVZ	R0, 0xea           
0001c5   38c0     SUB	R0, 0xc0            
0001c6   7a03     JB	0x3, 2               
0001c7   c1ca     JMP	#0x1ca              
0001c8   0ee8     MOVZ	R0, 0xe8           
0001c9   38bf     SUB	R0, 0xbf            
0001ca   7003     JNB	0x3, 0              
0001cb   c1dc     JMP	#0x1dc              
0001cc   0bbf     INC	0xbf                
0001cd   7a03     JB	0x3, 2               
0001ce   c1d0     JMP	#0x1d0              
0001cf   0bc0     INC	0xc0                
0001d0   0ee8     MOVZ	R0, 0xe8           
0001d1   18bf     XOR	R0, 0xbf            
0001d2   7a03     JB	0x3, 2               
0001d3   c1dc     JMP	#0x1dc              
0001d4   0eea     MOVZ	R0, 0xea           
0001d5   18c0     XOR	R0, 0xc0            
0001d6   7a03     JB	0x3, 2               
0001d7   c1dc     JMP	#0x1dc              
0001d8   9802     MOV	R0, #0x2            
0001d9   51de     MOV	0xde, R0            
0001da   0edf     MOVZ	R0, 0xdf           
0001db   51e0     MOV	0xe0, R0            
0001dc   50ee     MOV	R0, 0xee            
0001dd   80b1     ADD	R0, #0xb1           
0001de   51e8     MOV	0xe8, R0            
0001df   52e8     MOV	R1, 0xe8            
0001e0   f708     LD	R0, [R1]             
0001e1   51eb     MOV	0xeb, R0            
0001e2   9906     MOV	R1, #0x6            
0001e3   98c1     MOV	R0, #0xc1           
0001e4   d603     CALL	#0x603             
0001e5   6503     CLR	0x3, 5              
0001e6   51e8     MOV	0xe8, R0            
0001e7   0ee8     MOVZ	R0, 0xe8           
0001e8   18eb     XOR	R0, 0xeb            
0001e9   7a03     JB	0x3, 2               
0001ea   c252     JMP	#0x252              
0001eb   0eb9     MOVZ	R0, 0xb9           
0001ec   30ba     ORL	R0, 0xba            
0001ed   7203     JNB	0x3, 2              
0001ee   c217     JMP	#0x217              
0001ef   50de     MOV	R0, 0xde            
0001f0   a801     XOR	R0, #0x1            
0001f1   7a03     JB	0x3, 2               
0001f2   c212     JMP	#0x212              
0001f3   9802     MOV	R0, #0x2            
0001f4   51de     MOV	0xde, R0            
0001f5   50ee     MOV	R0, 0xee            
0001f6   51e0     MOV	0xe0, R0            
0001f7   50ee     MOV	R0, 0xee            
0001f8   80ae     ADD	R0, #0xae           
0001f9   9906     MOV	R1, #0x6            
0001fa   7003     JNB	0x3, 0              
0001fb   ff11     INC	R1                  
0001fc   d6b9     CALL	#0x6b9             
0001fd   6003     CLR	0x3, 0              
0001fe   ff18     RLC	R0                  
0001ff   6503     CLR	0x3, 5              
000200   51e5     MOV	0xe5, R0            
000201   803b     ADD	R0, #0x3b           
000202   9906     MOV	R1, #0x6            
000203   7003     JNB	0x3, 0              
000204   ff11     INC	R1                  
000205   d6b9     CALL	#0x6b9             
000206   6503     CLR	0x3, 5              
000207   31b9     ORL	0xb9, R0            
000208   50e5     MOV	R0, 0xe5            
000209   ff10     INC	R0                  
00020a   803b     ADD	R0, #0x3b           
00020b   9906     MOV	R1, #0x6            
00020c   7003     JNB	0x3, 0              
00020d   ff11     INC	R1                  
00020e   d6b9     CALL	#0x6b9             
00020f   6503     CLR	0x3, 5              
000210   31ba     ORL	0xba, R0            
000211   c216     JMP	#0x216              
000212   50ee     MOV	R0, 0xee            
000213   80b1     ADD	R0, #0xb1           
000214   9900     MOV	R1, #0              
000215   f748     ST	[R0], R1             
000216   c239     JMP	#0x239              
000217   50ee     MOV	R0, 0xee            
000218   80ae     ADD	R0, #0xae           
000219   9906     MOV	R1, #0x6            
00021a   7003     JNB	0x3, 0              
00021b   ff11     INC	R1                  
00021c   d6b9     CALL	#0x6b9             
00021d   6003     CLR	0x3, 0              
00021e   ff18     RLC	R0                  
00021f   6503     CLR	0x3, 5              
000220   51e5     MOV	0xe5, R0            
000221   803b     ADD	R0, #0x3b           
000222   9906     MOV	R1, #0x6            
000223   7003     JNB	0x3, 0              
000224   ff11     INC	R1                  
000225   d6b9     CALL	#0x6b9             
000226   6503     CLR	0x3, 5              
000227   51b9     MOV	0xb9, R0            
000228   50e5     MOV	R0, 0xe5            
000229   ff10     INC	R0                  
00022a   803b     ADD	R0, #0x3b           
00022b   9906     MOV	R1, #0x6            
00022c   7003     JNB	0x3, 0              
00022d   ff11     INC	R1                  
00022e   d6b9     CALL	#0x6b9             
00022f   6503     CLR	0x3, 5              
000230   51ba     MOV	0xba, R0            
000231   9801     MOV	R0, #0x1            
000232   51de     MOV	0xde, R0            
000233   51bf     MOV	0xbf, R0            
000234   03c0     CLR	0xc0                
000235   50ee     MOV	R0, 0xee            
000236   51df     MOV	0xdf, R0            
000237   98ff     MOV	R0, #0xff           
000238   51e0     MOV	0xe0, R0            
000239   50ee     MOV	R0, 0xee            
00023a   80b1     ADD	R0, #0xb1           
00023b   f701     LD	R1, [R0]             
00023c   ff11     INC	R1                  
00023d   f748     ST	[R0], R1             
00023e   c252     JMP	#0x252              
00023f   50ee     MOV	R0, 0xee            
000240   80b1     ADD	R0, #0xb1           
000241   51e8     MOV	0xe8, R0            
000242   52e8     MOV	R1, 0xe8            
000243   f708     LD	R0, [R1]             
000244   51ec     MOV	0xec, R0            
000245   9906     MOV	R1, #0x6            
000246   98c1     MOV	R0, #0xc1           
000247   d603     CALL	#0x603             
000248   6503     CLR	0x3, 5              
000249   51e8     MOV	0xe8, R0            
00024a   0ee8     MOVZ	R0, 0xe8           
00024b   38ec     SUB	R0, 0xec            
00024c   7003     JNB	0x3, 0              
00024d   c252     JMP	#0x252              
00024e   50ee     MOV	R0, 0xee            
00024f   80b1     ADD	R0, #0xb1           
000250   9900     MOV	R1, #0              
000251   f748     ST	[R0], R1             
000252   6003     CLR	0x3, 0              
000253   13c3     RLC	0xc3                
000254   13c4     RLC	0xc4                
000255   0bee     INC	0xee                
000256   c00e     JMP	#0xe                
000257   03e3     CLR	0xe3                
000258   79dd     JB	0xdd, 1              
000259   c264     JMP	#0x264              
00025a   98c2     MOV	R0, #0xc2           
00025b   9906     MOV	R1, #0x6            
00025c   d6b9     CALL	#0x6b9             
00025d   6503     CLR	0x3, 5              
00025e   0bdc     INC	0xdc                
00025f   52dc     MOV	R1, 0xdc            
000260   f841     SUB	R1, R0              
000261   7003     JNB	0x3, 0              
000262   c264     JMP	#0x264              
000263   61dd     CLR	0xdd, 1             
000264   9906     MOV	R1, #0x6            
000265   98bc     MOV	R0, #0xbc           
000266   d603     CALL	#0x603             
000267   6503     CLR	0x3, 5              
000268   51e8     MOV	0xe8, R0            
000269   9906     MOV	R1, #0x6            
00026a   98bd     MOV	R0, #0xbd           
00026b   d603     CALL	#0x603             
00026c   6503     CLR	0x3, 5              
00026d   51ec     MOV	0xec, R0            
00026e   0ee8     MOVZ	R0, 0xe8           
00026f   30ec     ORL	R0, 0xec            
000270   7203     JNB	0x3, 2              
000271   c2b4     JMP	#0x2b4              
000272   0eb9     MOVZ	R0, 0xb9           
000273   30ba     ORL	R0, 0xba            
000274   7203     JNB	0x3, 2              
000275   c2b4     JMP	#0x2b4              
000276   0bbd     INC	0xbd                
000277   7a03     JB	0x3, 2               
000278   c27a     JMP	#0x27a              
000279   0bbe     INC	0xbe                
00027a   98bc     MOV	R0, #0xbc           
00027b   9906     MOV	R1, #0x6            
00027c   d6b9     CALL	#0x6b9             
00027d   6503     CLR	0x3, 5              
00027e   18bd     XOR	R0, 0xbd            
00027f   7a03     JB	0x3, 2               
000280   c2b4     JMP	#0x2b4              
000281   98bd     MOV	R0, #0xbd           
000282   9906     MOV	R1, #0x6            
000283   d6b9     CALL	#0x6b9             
000284   6503     CLR	0x3, 5              
000285   18be     XOR	R0, 0xbe            
000286   7a03     JB	0x3, 2               
000287   c2b4     JMP	#0x2b4              
000288   03b9     CLR	0xb9                
000289   03ba     CLR	0xba                
00028a   50de     MOV	R0, 0xde            
00028b   a802     XOR	R0, #0x2            
00028c   7a03     JB	0x3, 2               
00028d   c29d     JMP	#0x29d              
00028e   50e0     MOV	R0, 0xe0            
00028f   6003     CLR	0x3, 0              
000290   ff18     RLC	R0                  
000291   51e5     MOV	0xe5, R0            
000292   809d     ADD	R0, #0x9d           
000293   f701     LD	R1, [R0]             
000294   50e5     MOV	R0, 0xe5            
000295   80a5     ADD	R0, #0xa5           
000296   f748     ST	[R0], R1             
000297   50e5     MOV	R0, 0xe5            
000298   809e     ADD	R0, #0x9e           
000299   f701     LD	R1, [R0]             
00029a   50e5     MOV	R0, 0xe5            
00029b   80a6     ADD	R0, #0xa6           
00029c   f748     ST	[R0], R1             
00029d   50df     MOV	R0, 0xdf            
00029e   6003     CLR	0x3, 0              
00029f   ff18     RLC	R0                  
0002a0   51e5     MOV	0xe5, R0            
0002a1   809d     ADD	R0, #0x9d           
0002a2   f701     LD	R1, [R0]             
0002a3   50e5     MOV	R0, 0xe5            
0002a4   80a5     ADD	R0, #0xa5           
0002a5   f748     ST	[R0], R1             
0002a6   50e5     MOV	R0, 0xe5            
0002a7   809e     ADD	R0, #0x9e           
0002a8   f701     LD	R1, [R0]             
0002a9   50e5     MOV	R0, 0xe5            
0002aa   80a6     ADD	R0, #0xa6           
0002ab   f748     ST	[R0], R1             
0002ac   03de     CLR	0xde                
0002ad   98ff     MOV	R0, #0xff           
0002ae   51df     MOV	0xdf, R0            
0002af   51e0     MOV	0xe0, R0            
0002b0   03bf     CLR	0xbf                
0002b1   03c0     CLR	0xc0                
0002b2   03bd     CLR	0xbd                
0002b3   03be     CLR	0xbe                
0002b4   0008     CRET                    
                                           func.__KF8S_Init_Touch_General_
0005c5   6503     CLR	0x3, 5              
0005c6   03e5     CLR	0xe5                
0005c7   60dd     CLR	0xdd, 0             
0005c8   61dd     CLR	0xdd, 1             
0005c9   03c1     CLR	0xc1                
0005ca   03c2     CLR	0xc2                
0005cb   03cd     CLR	0xcd                
0005cc   03b9     CLR	0xb9                
0005cd   03ba     CLR	0xba                
0005ce   03e5     CLR	0xe5                
0005cf   6f2c     SET	0x2c, 7             
0005d0   670c     CLR	0xc, 7              
0005d1   7edd     JB	0xdd, 6              
0005d2   c5d7     JMP	#0x5d7              
0005d3   9890     MOV	R0, #0x90           
0005d4   5153     MOV	0x53, R0            
0005d5   0350     CLR	0x50                
0005d6   c5df     JMP	#0x5df              
0005d7   682c     SET	0x2c, 0             
0005d8   600c     CLR	0xc, 0              
0005d9   030f     CLR	0xf                 
0005da   030e     CLR	0xe                 
0005db   9801     MOV	R0, #0x1            
0005dc   5110     MOV	0x10, R0            
0005dd   9880     MOV	R0, #0x80           
0005de   5153     MOV	0x53, R0            
0005df   98ae     MOV	R0, #0xae           
0005e0   9906     MOV	R1, #0x6            
0005e1   d6b9     CALL	#0x6b9             
0005e2   3153     ORL	0x53, R0            
0005e3   9802     MOV	R0, #0x2            
0005e4   ff58     DECJZ	R0                
0005e5   c5e4     JMP	#0x5e4              
0005e6   6e53     SET	0x53, 6             
0005e7   0000     NOP                     
0005e8   7e53     JB	0x53, 6              
0005e9   c5e6     JMP	#0x5e6              
0005ea   7453     JNB	0x53, 4             
0005eb   035f     CLR	0x5f                
0005ec   6e0b     SET	0xb, 6              
0005ed   6f0b     SET	0xb, 7              
0005ee   0008     CRET                    
                                           func.__KF8_lib_Baihualv_get_
000548   6503     CLR	0x3, 5              
000549   50c7     MOV	R0, 0xc7            
00054a   39c5     SUB	0xc5, R0            
00054b   52c8     MOV	R1, 0xc8            
00054c   7803     JB	0x3, 0               
00054d   ff11     INC	R1                  
00054e   3bc6     SUB	0xc6, R1            
00054f   7803     JB	0x3, 0               
000550   c552     JMP	#0x552              
000551   c559     JMP	#0x559              
000552   64dd     CLR	0xdd, 4             
000553   05c5     CPL	0xc5                
000554   05c6     CPL	0xc6                
000555   0bc5     INC	0xc5                
000556   7203     JNB	0x3, 2              
000557   0bc6     INC	0xc6                
000558   c55a     JMP	#0x55a              
000559   6cdd     SET	0xdd, 4             
00055a   50c6     MOV	R0, 0xc6            
00055b   88fc     AND	R0, #0xfc           
00055c   7a03     JB	0x3, 2               
00055d   c574     JMP	#0x574              
00055e   9806     MOV	R0, #0x6            
00055f   ff10     INC	R0                  
000560   c564     JMP	#0x564              
000561   6003     CLR	0x3, 0              
000562   13c5     RLC	0xc5                
000563   13c6     RLC	0xc6                
000564   ff58     DECJZ	R0                
000565   c561     JMP	#0x561              
000566   9808     MOV	R0, #0x8            
000567   21c7     ADD	0xc7, R0            
000568   7803     JB	0x3, 0               
000569   c56b     JMP	#0x56b              
00056a   0bc8     INC	0xc8                
00056b   9804     MOV	R0, #0x4            
00056c   ff10     INC	R0                  
00056d   c571     JMP	#0x571              
00056e   6003     CLR	0x3, 0              
00056f   11c8     RRC	0xc8                
000570   11c7     RRC	0xc7                
000571   ff58     DECJZ	R0                
000572   c56e     JMP	#0x56e              
000573   c582     JMP	#0x582              
000574   6003     CLR	0x3, 0              
000575   13c5     RLC	0xc5                
000576   13c6     RLC	0xc6                
000577   6003     CLR	0x3, 0              
000578   13c5     RLC	0xc5                
000579   13c6     RLC	0xc6                
00057a   9880     MOV	R0, #0x80           
00057b   21c7     ADD	0xc7, R0            
00057c   7803     JB	0x3, 0               
00057d   c57f     JMP	#0x57f              
00057e   0bc8     INC	0xc8                
00057f   50c8     MOV	R0, 0xc8            
000580   51c7     MOV	0xc7, R0            
000581   03c8     CLR	0xc8                
000582   03e4     CLR	0xe4                
000583   50c7     MOV	R0, 0xc7            
000584   39c5     SUB	0xc5, R0            
000585   52c8     MOV	R1, 0xc8            
000586   7803     JB	0x3, 0               
000587   ff11     INC	R1                  
000588   3bc6     SUB	0xc6, R1            
000589   7803     JB	0x3, 0               
00058a   c58c     JMP	#0x58c              
00058b   c58d     JMP	#0x58d              
00058c   c593     JMP	#0x593              
00058d   0be4     INC	0xe4                
00058e   50e4     MOV	R0, 0xe4            
00058f   a07e     SUB	R0, #0x7e           
000590   7803     JB	0x3, 0               
000591   c593     JMP	#0x593              
000592   c583     JMP	#0x583              
000593   7cdd     JB	0xdd, 4              
000594   c597     JMP	#0x597              
000595   05e4     CPL	0xe4                
000596   0be4     INC	0xe4                
000597   0008     CRET                    
                                           func.__R2PCHPCL
0006b9   530a     MOV	0xa, R1             
0006ba   5102     MOV	0x2, R0             
0006bb   0008     CRET                    
                                           .cinit
00065b   6503     CLR	0x3, 5              
00065c   9890     MOV	R0, #0x90           
00065d   995e     MOV	R1, #0x5e           
00065e   0000     NOP                     
00065f   d672     CALL	#0x672             
000660   0380     CLR	0x80                
000661   0381     CLR	0x81                
000662   0382     CLR	0x82                
000663   0383     CLR	0x83                
000664   0384     CLR	0x84                
000665   0385     CLR	0x85                
000666   0386     CLR	0x86                
000667   0387     CLR	0x87                
000668   0388     CLR	0x88                
000669   0389     CLR	0x89                
00066a   038a     CLR	0x8a                
00066b   038b     CLR	0x8b                
00066c   038c     CLR	0x8c                
00066d   038d     CLR	0x8d                
00066e   038e     CLR	0x8e                
00066f   038f     CLR	0x8f                
000670   03ee     CLR	0xee                
000671   0008     CRET                    
000672   020a     CLR	R2                  
000673   f750     ST	[R0], R2             
000674   ff10     INC	R0                  
000675   ff59     DECJZ	R1                
000676   c673     JMP	#0x673              
000677   0008     CRET                    
