gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 8-2-2019  16:46:35
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 16:46:32 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../EEPROM.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_DATA_EE_WRITE_FUN
                                           	.global	_DATA_EE_READ_FUN
                                           	.global	_DATA_EE_WRITE_ONE
                                           	.global	_DATA_EE_READ_ONE
                                           	.global	_DATA_EE_BUFFER
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_EEPROM_0	.udata
                                           _DATA_EE_BUFFER	.res	16
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_EEPROM_0	.udata
                                           r0x1002	.res	1
                                           UDL_EEPROM_1	.udata
                                           r0x1003	.res	1
                                           UDL_EEPROM_2	.udata
                                           r0x1000	.res	1
                                           UDL_EEPROM_3	.udata
                                           r0x1001	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           
                                           func._DATA_EE_WRITE_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _DATA_EE_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;3 compiler assigned registers:
                                           ;   STK00
                                           ;   r0x1000
                                           ;   r0x1001
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _DATA_EE_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	214; "../EEPROM.c"	void DATA_EE_WRITE_FUN(unsigned char address,unsigned char length)
00104f   e100     MOVB	#0x00               	BANKSEL	_NVMADDRL
001050   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK00
001051   0eaa     MOVZ	R0, 0xaa            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1000
001052   5184     MOV	0x84, R0             	MOV	r0x1000, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
001053   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
001054   660b     CLR	0xb, 6               	CLR _INTCTL,_PUIE
001055   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001056   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
001057   c055     JMP	#0x55                	JMP $-2
                                           	;
001058   9830     MOV	R0, #0x30            	MOV R0,#0x30
001059   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
00105a   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
00105b   9b87     MOV	R3, #0x87            	MOV R3,#_DATA_EE_BUFFER
                                           	
                                           ;	::->op : =
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00013_DS_
                                           ;	.line	237; "../EEPROM.c"	while(length--)		// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1000
00105c   0e84     MOVZ	R0, 0x84            	MOVZ	R0, r0x1000
                                           	BANKSEL	r0x1001
00105d   5183     MOV	0x83, R0             	MOV	r0x1001, R0
                                           ;	::->op : -
                                           	BANKSEL	r0x1000
00105e   0784     DEC	0x84                 	DEC	r0x1000
                                           ;	::->op : IFX
00105f   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1001
001060   3083     ORL	R0, 0x83             	ORL	R0, r0x1001
001061   7203     JNB	0x3, 2               	JNB	PSW, 2
001062   c07e     JMP	#0x7e                	JMP	_00015_DS_
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _DATA_EE_BUFFER
001063   f71e     LD	R6, [R3]              	LD R6,[R3]
001064   ff13     INC	R3                   	INC R3
                                           	BANKSEL _NVMDATAL
001065   5d39     MOV	0x39, R6             	MOV _NVMDATAL,R6
                                           	;
001066   9d04     MOV	R5, #0x4             	MOV R5 ,#0x04
001067   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001068   9d69     MOV	R5, #0x69            	MOV R5,#0x69
001069   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
00106a   9d96     MOV	R5, #0x96            	MOV R5,#0x96
00106b   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
00106c   693c     SET	0x3c, 1              	SET _NVMCTL0 , 1 ;
00106d   ffff     NOPZ                     	NOPZ
00106e   ffff     NOPZ                     	NOPZ
00106f   ffff     NOPZ                     	NOPZ
001070   ffff     NOPZ                     	NOPZ
001071   ffff     NOPZ                     	NOPZ
001072   ffff     NOPZ                     	NOPZ ;
001073   ffff     NOPZ                     	NOPZ
001074   ffff     NOPZ                     	NOPZ
001075   ffff     NOPZ                     	NOPZ
001076   ffff     NOPZ                     	NOPZ
001077   9d00     MOV	R5, #0               	MOV R5,#0X00
001078   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
                                           	;
001079   7f0c     JB	0xc, 7                	JB _EIF1,7
00107a   c079     JMP	#0x79                	JMP $-1
00107b   670c     CLR	0xc, 7               	CLR _EIF1,7
                                           	;
                                           	BANKSEL _NVMADDRL
00107c   0b3b     INC	0x3b                 	INC _NVMADDRL
                                           	
                                           ;	::->op : GOTO
00107d   c05c     JMP	#0x5c                	JMP	_00013_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : INLINEASM
                                           _00015_DS_
                                           	;
                                           	BANKSEL _OSCCTL
00107e   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
00107f   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
001080   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
001081   0008     CRET                     	CRET	
                                           ; exit point of _DATA_EE_WRITE_FUN
                                           
                                           
                                           
                                           func._DATA_EE_READ_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _DATA_EE_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;3 compiler assigned registers:
                                           ;   STK00
                                           ;   r0x1002
                                           ;   r0x1003
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _DATA_EE_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	100; "../EEPROM.c"	void DATA_EE_READ_FUN(unsigned char address,unsigned char length)
0010a8   e100     MOVB	#0x00               	BANKSEL	_NVMADDRL
0010a9   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK00
0010aa   0eaa     MOVZ	R0, 0xaa            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1002
0010ab   5186     MOV	0x86, R0             	MOV	r0x1002, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
0010ac   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
0010ad   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
0010ae   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
0010af   c0ad     JMP	#0xad                	JMP $-2
                                           	;
0010b0   9830     MOV	R0, #0x30            	MOV R0,#0x30
0010b1   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
0010b2   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
0010b3   9b87     MOV	R3, #0x87            	MOV R3,#_DATA_EE_BUFFER
                                           	
                                           ;	::->op : =
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00005_DS_
                                           ;	.line	122; "../EEPROM.c"	while(length--)	// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1002
0010b4   0e86     MOVZ	R0, 0x86            	MOVZ	R0, r0x1002
                                           	BANKSEL	r0x1003
0010b5   5185     MOV	0x85, R0             	MOV	r0x1003, R0
                                           ;	::->op : -
                                           	BANKSEL	r0x1002
0010b6   0786     DEC	0x86                 	DEC	r0x1002
                                           ;	::->op : IFX
0010b7   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1003
0010b8   3085     ORL	R0, 0x85             	ORL	R0, r0x1003
0010b9   7203     JNB	0x3, 2               	JNB	PSW, 2
0010ba   c0c6     JMP	#0xc6                	JMP	_00007_DS_
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _NVMCTL0
0010bb   9d01     MOV	R5, #0x1             	MOV R5,#0x01
0010bc   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
0010bd   ffff     NOPZ                     	NOPZ
0010be   ffff     NOPZ                     	NOPZ
0010bf   ffff     NOPZ                     	NOPZ
0010c0   ffff     NOPZ                     	NOPZ
                                           	;
                                           	BANKSEL _NVMDATAL
0010c1   5c39     MOV	R6, 0x39             	MOV R6,_NVMDATAL
                                           	BANKSEL _DATA_EE_BUFFER
0010c2   f773     ST	[R3], R6              	ST [R3],R6
0010c3   ff13     INC	R3                   	INC R3
                                           	;
                                           	BANKSEL _NVMADDRL
0010c4   0b3b     INC	0x3b                 	INC _NVMADDRL
                                           	
                                           ;	::->op : GOTO
0010c5   c0b4     JMP	#0xb4                	JMP	_00005_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : INLINEASM
                                           _00007_DS_
                                           	;
                                           	BANKSEL _OSCCTL
0010c6   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
0010c7   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
0010c8   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0010c9   0008     CRET                     	CRET	
                                           ; exit point of _DATA_EE_READ_FUN
                                           
                                           
                                           
                                           func._DATA_EE_WRITE_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _DATA_EE_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;1 compiler assigned register :
                                           ;   STK00
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _DATA_EE_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	32; "../EEPROM.c"	void DATA_EE_WRITE_ONE(unsigned char address,unsigned char value)
001082   e100     MOVB	#0x00               	BANKSEL	_NVMADDRL
001083   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK00
001084   0eaa     MOVZ	R0, 0xaa            	MOVZ	R0, STK00
                                           	BANKSEL	_NVMDATAL
001085   5139     MOV	0x39, R0             	MOV	_NVMDATAL, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
001086   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
001087   660b     CLR	0xb, 6               	CLR _INTCTL,_PUIE
001088   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001089   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
00108a   c088     JMP	#0x88                	JMP $-2
                                           	;
00108b   9830     MOV	R0, #0x30            	MOV R0,#0x30
00108c   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
00108d   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
00108e   9d04     MOV	R5, #0x4             	MOV R5 ,#0x04
00108f   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001090   9d69     MOV	R5, #0x69            	MOV R5,#0x69
001091   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
001092   9d96     MOV	R5, #0x96            	MOV R5,#0x96
001093   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
001094   693c     SET	0x3c, 1              	SET _NVMCTL0 , 1 ;
001095   ffff     NOPZ                     	NOPZ
001096   ffff     NOPZ                     	NOPZ
001097   ffff     NOPZ                     	NOPZ
001098   ffff     NOPZ                     	NOPZ
001099   ffff     NOPZ                     	NOPZ
00109a   ffff     NOPZ                     	NOPZ ;
00109b   ffff     NOPZ                     	NOPZ
00109c   ffff     NOPZ                     	NOPZ
00109d   ffff     NOPZ                     	NOPZ
00109e   ffff     NOPZ                     	NOPZ
00109f   9d00     MOV	R5, #0               	MOV R5,#0X00
0010a0   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
                                           	;
0010a1   7f0c     JB	0xc, 7                	JB _EIF1,7
0010a2   c0a1     JMP	#0xa1                	JMP $-1
0010a3   670c     CLR	0xc, 7               	CLR _EIF1,7
                                           	;
0010a4   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
0010a5   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
0010a6   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0010a7   0008     CRET                     	CRET	
                                           ; exit point of _DATA_EE_WRITE_ONE
                                           
                                           
                                           
                                           func._DATA_EE_READ_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _DATA_EE_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _DATA_EE_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	12; "../EEPROM.c"	uchar DATA_EE_READ_ONE(unsigned char address)
001103   e100     MOVB	#0x00               	BANKSEL	_NVMADDRL
001104   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : INLINEASM
                                           	;
001105   9801     MOV	R0, #0x1             	MOV R0,#0X01
001106   513c     MOV	0x3c, R0             	MOV NVMCTL0,R0
001107   ffff     NOPZ                     	NOPZ
001108   ffff     NOPZ                     	NOPZ
001109   ffff     NOPZ                     	NOPZ
00110a   ffff     NOPZ                     	NOPZ
00110b   ffff     NOPZ                     	NOPZ
                                           	
                                           ;	::->op : RETURN
                                           ;	.line	24; "../EEPROM.c"	return 	NVMDATAL;
                                           	BANKSEL	_NVMDATAL
00110c   0e39     MOVZ	R0, 0x39            	MOVZ	R0, _NVMDATAL
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
00110d   0008     CRET                     	CRET	
                                           ; exit point of _DATA_EE_READ_ONE
                                           
                                           
                                           ;	code size estimation:
                                           ;	   31+   19 =    50 instructions (  138 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 16:46:33 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x1dd4
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 16:46:34 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_DATA_EE_READ_ONE
                                           	.extern	_DATA_EE_WRITE_ONE
                                           	.extern	_DATA_EE_READ_FUN
                                           	.extern	_DATA_EE_WRITE_FUN
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_DATA_EE_BUFFER
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Sys_Init
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           
                                           	.global I0R1
                                           	.global I0R7
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1R7
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata
                                           I0R1		.res 1
                                           I0R7		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1R7		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1000	.res	1
                                           UDL_main_1	.udata
                                           r0x1001	.res	1
                                           UDL_main_2	.udata
                                           r0x1002	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e010     MOVP	#0x10               	PAGESEL	init_imp
000002   c10e     JMP	#0x10e               	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
00110e   e010     MOVP	#0x10               	PAGESEL	_startup
00110f   d0ca     CALL	#0xca               	CALL	_startup
001110   e010     MOVP	#0x10               	PAGESEL	__gsinit_startup
001111   d114     CALL	#0x114              	CALL	__gsinit_startup
001112   e010     MOVP	#0x10               	PAGESEL	_main
001113   c000     JMP	#0                   	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           _00025_DS_
                                           ;	.line	71; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00027_DS_
                                           ;	.line	78; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _Sys_Init
                                           ;   _DATA_EE_WRITE_FUN
                                           ;   _DATA_EE_READ_ONE
                                           ;   _DATA_EE_WRITE_ONE
                                           ;   _DATA_EE_WRITE_FUN
                                           ;   _DATA_EE_READ_FUN
                                           ;   _DATA_EE_WRITE_FUN
                                           ;   _Sys_Init
                                           ;   _DATA_EE_WRITE_FUN
                                           ;   _DATA_EE_READ_ONE
                                           ;   _DATA_EE_WRITE_ONE
                                           ;   _DATA_EE_WRITE_FUN
                                           ;   _DATA_EE_READ_FUN
                                           ;   _DATA_EE_WRITE_FUN
                                           ;4 compiler assigned registers:
                                           ;   r0x1000
                                           ;   r0x1001
                                           ;   r0x1002
                                           ;   STK00
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	::->op : CALL
                                           ;	.line	35; "../main.c"	Sys_Init();
001000   e010     MOVP	#0x10               	PAGESEL	_Sys_Init
001001   d0eb     CALL	#0xeb               	CALL	_Sys_Init
001002   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : =
                                           ;	.line	38; "../main.c"	for (i = 0; i < DATA_EE_BUFFER_MAX; i++)
001003   e100     MOVB	#0x00               	BANKSEL	r0x1000
001004   0382     CLR	0x82                 	CLR	r0x1000
                                           ;	::->op : =
                                           	BANKSEL	r0x1001
001005   0381     CLR	0x81                 	CLR	r0x1001
                                           ;	::->op : LABEL
                                           ;	::->op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00006_DS_
001006   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	r0x1001
001007   3881     SUB	R0, 0x81             	SUB	R0, r0x1001
                                           ;comparing bytes at offset 0
001008   7003     JNB	0x3, 0               	JNB	PSW, 0
001009   c014     JMP	#0x14                	JMP	_00009_DS_
                                           ;	::->op : +
                                           ;	.line	40; "../main.c"	DATA_EE_BUFFER[i] = temp;
                                           	BANKSEL	r0x1001
00100a   5081     MOV	R0, 0x81             	MOV	R0, r0x1001
00100b   8087     ADD	R0, #0x87            	ADD	R0,# (_DATA_EE_BUFFER + 0)
                                           	BANKSEL	r0x1002
00100c   5180     MOV	0x80, R0             	MOV	r0x1002, R0
                                           ;	::->op :*  =
                                           	BANKSEL	r0x1000
00100d   0e82     MOVZ	R0, 0x82            	MOVZ	R0, r0x1000
                                           	BANKSEL	r0x1002
00100e   5280     MOV	R1, 0x80             	MOV	R1, r0x1002
                                           	BANKSEL	_DATA_EE_BUFFER
00100f   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : +
                                           ;	.line	41; "../main.c"	temp+=0x11;
001010   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
                                           	BANKSEL	r0x1000
001011   2182     ADD	0x82, R0             	ADD	r0x1000, R0
                                           ;	::->op : +
                                           ;	.line	38; "../main.c"	for (i = 0; i < DATA_EE_BUFFER_MAX; i++)
                                           	BANKSEL	r0x1001
001012   0b81     INC	0x81                 	INC	r0x1001
                                           ;	::->op : GOTO
001013   c006     JMP	#0x6                 	JMP	_00006_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           _00009_DS_
                                           ;	.line	44; "../main.c"	DATA_EE_WRITE_FUN(0x00,DATA_EE_BUFFER_MAX);
001014   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK00
001015   51aa     MOV	0xaa, R0             	MOV	STK00, R0
001016   9800     MOV	R0, #0               	MOV	R0,# 0x00
001017   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_WRITE_FUN
001018   d04f     CALL	#0x4f               	CALL	_DATA_EE_WRITE_FUN
001019   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	47; "../main.c"	temp=DATA_EE_READ_ONE(0x09);
00101a   9809     MOV	R0, #0x9             	MOV	R0,# 0x09
00101b   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_READ_ONE
00101c   d103     CALL	#0x103              	CALL	_DATA_EE_READ_ONE
00101d   e010     MOVP	#0x10               	PAGESEL	$
00101e   e100     MOVB	#0x00               	BANKSEL	r0x1000
00101f   5182     MOV	0x82, R0             	MOV	r0x1000, R0
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	49; "../main.c"	DATA_EE_WRITE_ONE(0x40,temp);
                                           	BANKSEL	r0x1000
001020   0e82     MOVZ	R0, 0x82            	MOVZ	R0, r0x1000
                                           	BANKSEL	STK00
001021   51aa     MOV	0xaa, R0             	MOV	STK00, R0
001022   9840     MOV	R0, #0x40            	MOV	R0,# 0x40
001023   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_WRITE_ONE
001024   d082     CALL	#0x82               	CALL	_DATA_EE_WRITE_ONE
001025   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : =
                                           ;	.line	52; "../main.c"	for (i = 0; i < DATA_EE_BUFFER_MAX; i++)
001026   e100     MOVB	#0x00               	BANKSEL	r0x1000
001027   0382     CLR	0x82                 	CLR	r0x1000
                                           ;	::->op : =
                                           	BANKSEL	r0x1001
001028   0381     CLR	0x81                 	CLR	r0x1001
                                           ;	::->op : LABEL
                                           ;	::->op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00010_DS_
001029   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	r0x1001
00102a   3881     SUB	R0, 0x81             	SUB	R0, r0x1001
                                           ;comparing bytes at offset 0
00102b   7003     JNB	0x3, 0               	JNB	PSW, 0
00102c   c037     JMP	#0x37                	JMP	_00013_DS_
                                           ;	::->op : +
                                           ;	.line	54; "../main.c"	DATA_EE_BUFFER[i] = temp;
                                           	BANKSEL	r0x1001
00102d   5081     MOV	R0, 0x81             	MOV	R0, r0x1001
00102e   8087     ADD	R0, #0x87            	ADD	R0,# (_DATA_EE_BUFFER + 0)
                                           	BANKSEL	r0x1002
00102f   5180     MOV	0x80, R0             	MOV	r0x1002, R0
                                           ;	::->op :*  =
                                           	BANKSEL	r0x1000
001030   0e82     MOVZ	R0, 0x82            	MOVZ	R0, r0x1000
                                           	BANKSEL	r0x1002
001031   5280     MOV	R1, 0x80             	MOV	R1, r0x1002
                                           	BANKSEL	_DATA_EE_BUFFER
001032   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : +
                                           ;	.line	55; "../main.c"	temp+=0x11;
001033   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
                                           	BANKSEL	r0x1000
001034   2182     ADD	0x82, R0             	ADD	r0x1000, R0
                                           ;	::->op : +
                                           ;	.line	52; "../main.c"	for (i = 0; i < DATA_EE_BUFFER_MAX; i++)
                                           	BANKSEL	r0x1001
001035   0b81     INC	0x81                 	INC	r0x1001
                                           ;	::->op : GOTO
001036   c029     JMP	#0x29                	JMP	_00010_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           _00013_DS_
                                           ;	.line	57; "../main.c"	DATA_EE_WRITE_FUN(0x40,DATA_EE_BUFFER_MAX);
001037   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK00
001038   51aa     MOV	0xaa, R0             	MOV	STK00, R0
001039   9840     MOV	R0, #0x40            	MOV	R0,# 0x40
00103a   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_WRITE_FUN
00103b   d04f     CALL	#0x4f               	CALL	_DATA_EE_WRITE_FUN
00103c   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	59; "../main.c"	DATA_EE_READ_FUN(0x40,DATA_EE_BUFFER_MAX);
00103d   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
00103e   e100     MOVB	#0x00               	BANKSEL	STK00
00103f   51aa     MOV	0xaa, R0             	MOV	STK00, R0
001040   9840     MOV	R0, #0x40            	MOV	R0,# 0x40
001041   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_READ_FUN
001042   d0a8     CALL	#0xa8               	CALL	_DATA_EE_READ_FUN
001043   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op :*  =
                                           ;	.line	60; "../main.c"	DATA_EE_BUFFER[0]=0xFE;
001044   98fe     MOV	R0, #0xfe            	MOV	R0,# 0xfe
001045   e100     MOVB	#0x00               	BANKSEL	_DATA_EE_BUFFER
001046   5187     MOV	0x87, R0             	MOV	 (_DATA_EE_BUFFER + 0), R0
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	61; "../main.c"	DATA_EE_WRITE_FUN(0x20,DATA_EE_BUFFER_MAX);
001047   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK00
001048   51aa     MOV	0xaa, R0             	MOV	STK00, R0
001049   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
00104a   e010     MOVP	#0x10               	PAGESEL	_DATA_EE_WRITE_FUN
00104b   d04f     CALL	#0x4f               	CALL	_DATA_EE_WRITE_FUN
00104c   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : LABEL
                                           ;	::->op : GOTO
                                           _00004_DS_
                                           ;	.line	62; "../main.c"	while(1)
00104d   c04d     JMP	#0x4d                	JMP	_00004_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
00104e   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._Sys_Init	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;	::->op : =
                                           ;	.line	18; "../main.c"	OSCCTL = 0x70;		//Ê±ÖÓÅäÖÃÎªÄÚ²¿16M
0010eb   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
0010ec   e100     MOVB	#0x00               	BANKSEL	_OSCCTL
0010ed   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	::->op : =
                                           ;	.line	19; "../main.c"	TR0=0;
                                           	BANKSEL	_TR0
0010ee   0325     CLR	0x25                 	CLR	_TR0
                                           ;	::->op : =
                                           ;	.line	20; "../main.c"	TR1=0;
                                           	BANKSEL	_TR1
0010ef   0327     CLR	0x27                 	CLR	_TR1
                                           ;	::->op : =
                                           ;	.line	21; "../main.c"	TR2=0;
                                           	BANKSEL	_TR2
0010f0   0326     CLR	0x26                 	CLR	_TR2
                                           ;	::->op : =
                                           ;	.line	22; "../main.c"	TR3=0;
                                           	BANKSEL	_TR3
0010f1   0349     CLR	0x49                 	CLR	_TR3
                                           ;	::->op : =
                                           ;	.line	23; "../main.c"	P0=0;
                                           	BANKSEL	_P0
0010f2   0305     CLR	0x5                  	CLR	_P0
                                           ;	::->op : =
                                           ;	.line	24; "../main.c"	P1=0;
                                           	BANKSEL	_P1
0010f3   0307     CLR	0x7                  	CLR	_P1
                                           ;	::->op : =
                                           ;	.line	25; "../main.c"	P2=0;
                                           	BANKSEL	_P2
0010f4   0306     CLR	0x6                  	CLR	_P2
                                           ;	::->op : =
                                           ;	.line	26; "../main.c"	P3=0;
                                           	BANKSEL	_P3
0010f5   0308     CLR	0x8                  	CLR	_P3
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0010f6   0008     CRET                     	CRET	
                                           ; exit point of _Sys_Init
                                           
                                           
                                           ;	code size estimation:
                                           ;	   87+   37 =   124 instructions (  322 byte)
                                           
                                           
                                           	.end
                                           .config
002007   1dd4     XOR	0xd4, R2            
002008   ffff     NOPZ                    
                                           func.__gsinit_startup
001114   e010     MOVP	#0x10              
001115   d0f7     CALL	#0xf7              
001116   e010     MOVP	#0x10              
001117   0008     CRET                    
                                           _sartup_A100EON
0010ca   e01f     MOVP	#0x1F              
0010cb   e100     MOVB	#0x00              
0010cc   dfff     CALL	#0xfff             
0010cd   5130     MOV	0x30, R0            
0010ce   ffff     NOPZ                    
0010cf   ffff     NOPZ                    
0010d0   dffe     CALL	#0xffe             
0010d1   5137     MOV	0x37, R0            
0010d2   ffff     NOPZ                    
0010d3   ffff     NOPZ                    
0010d4   dffd     CALL	#0xffd             
0010d5   514c     MOV	0x4c, R0            
0010d6   ffff     NOPZ                    
0010d7   ffff     NOPZ                    
0010d8   dffc     CALL	#0xffc             
0010d9   514d     MOV	0x4d, R0            
0010da   ffff     NOPZ                    
0010db   ffff     NOPZ                    
0010dc   dffb     CALL	#0xffb             
0010dd   512a     MOV	0x2a, R0            
0010de   ffff     NOPZ                    
0010df   e101     MOVB	#0x01              
0010e0   dffa     CALL	#0xffa             
0010e1   5159     MOV	0x59, R0            
0010e2   ffff     NOPZ                    
0010e3   dff9     CALL	#0xff9             
0010e4   515a     MOV	0x5a, R0            
0010e5   ffff     NOPZ                    
0010e6   dff8     CALL	#0xff8             
0010e7   5165     MOV	0x65, R0            
0010e8   ffff     NOPZ                    
0010e9   ffff     NOPZ                    
0010ea   0008     CRET                    
                                           .cinit
0010f7   e100     MOVB	#0x00              
0010f8   9880     MOV	R0, #0x80           
0010f9   992b     MOV	R1, #0x2b           
0010fa   e010     MOVP	#0x10              
0010fb   d0fd     CALL	#0xfd              
0010fc   0008     CRET                    
0010fd   020a     CLR	R2                  
0010fe   f750     ST	[R0], R2             
0010ff   ff10     INC	R0                  
001100   ff59     DECJZ	R1                
001101   c0fe     JMP	#0xfe               
001102   0008     CRET                    
