gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 8-4-2019  20:07:56
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Sun Aug 04 20:07:53 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../UART.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_UART_SendBuf
                                           	.global	_UART_Init
                                           	.global	_UART_BUF
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_UART_0	.udata
                                           _UART_BUF	.res	50
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           
                                           func._UART_SendBuf	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _UART_SendBuf	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _UART_SendBuf	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	34; "../UART.c"	void UART_SendBuf(unsigned char SendTemp)
0000c9   e101     MOVB	#0x01               	BANKSEL	_TXSDR
0000ca   5121     MOV	0x21, R0             	MOV	_TXSDR, R0
                                           ;	::->op : LABEL
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           _00003_DS_
                                           ;	.line	37; "../UART.c"	while(TXSRS==0);
                                           	BANKSEL	_TSCTL_bits
0000cb   7924     JB	0x24, 1               	JB	_TSCTL_bits, 1
0000cc   c0cb     JMP	#0xcb                	JMP	_00003_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0000cd   0008     CRET                     	CRET	
                                           ; exit point of _UART_SendBuf
                                           
                                           
                                           
                                           func._UART_Init	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _UART_Init	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _UART_Init	;Function start
                                           ; 2 exit points
                                           ;	::->op : =
                                           ;	.line	14; "../UART.c"	BRCTL=0x40;		// 	½ÓÊÕ¿ÕÏÐ  Ê¹ÓÃ8Î»¼ÆÊýÆ÷£¬²»¿¼ÂÇ»½ÐÑÊÇÊ¹ÄÜºÍ×Ô¶¯²¨ÌØÂÊ¼ì²â
000099   9840     MOV	R0, #0x40            	MOV	R0,# 0x40
00009a   e101     MOVB	#0x01               	BANKSEL	_BRCTL
00009b   5123     MOV	0x23, R0             	MOV	_BRCTL, R0
                                           ;	::->op : =
                                           ;	.line	16; "../UART.c"	EUBRGH=0x00;	// ²¨ÌØÂÊ¹«Ê½=SCLK/(m*y+1),ÆäÖÐSCLKÏµÍ³Ê±ÖÓ£¬ÈçÕâÀï8M£¬mÎª±¶ÆµÊý£¬¼ûÊÖ²á£¬yÎª8Î»»ò16Î»²¨ÌØÂÊ¼ÆÊýÖµ
                                           	BANKSEL	_EUBRGH
00009c   0326     CLR	0x26                 	CLR	_EUBRGH
                                           ;	::->op : =
                                           ;	.line	17; "../UART.c"	EUBRGL=0x19; 	// SYNC=0(È«Ë«¹¤Òì²½Ä£Ê½),BRG16=0(Ê¹ÓÃ8Î»²¨ÌØÂÊ·¢ÉúÆ÷),HBRG=0(µÍËÙ)£¬Baud=8000000/(64*(12+1))=9615
00009d   9819     MOV	R0, #0x19            	MOV	R0,# 0x19
                                           	BANKSEL	_EUBRGL
00009e   5125     MOV	0x25, R0             	MOV	_EUBRGL, R0
                                           ;	::->op : =
                                           ;	.line	18; "../UART.c"	TSCTL=0x22;  	// 8Î» ·¢ËÍ£¬Ê¹ÄÜ·¢ËÍ£¬È«Ë«¹¤Òì²½Ä£Ê½SYNC=0£¬µÍËÙÄ£Ê½HBRG=0£¬·¢ËÍÒÆÎ»¿Õ,²»·¢ËÍÍ¬²½¼ä¸ô·û
00009f   9822     MOV	R0, #0x22            	MOV	R0,# 0x22
                                           	BANKSEL	_TSCTL
0000a0   5124     MOV	0x24, R0             	MOV	_TSCTL, R0
                                           ;	::->op : =
                                           ;	.line	19; "../UART.c"	RSCTL=0x90;  	// ´®¿ÚÊ¹ÄÜ£¨ÅäÖÃÒý½ÅÎª´®ÐÐ¿ÚÒý½Å£©£¬8Î»½ÓÊÕ£¬½ÓÊÕÊ¹ÄÜ£¬ÎÞÖ¡´íÎó£¬Òç³ö´íÎó£¬²»¿¼ÂÇµØÖ·Ê¶±ðºÍµÚ9Î»
0000a1   9890     MOV	R0, #0x90            	MOV	R0,# 0x90
                                           	BANKSEL	_RSCTL
0000a2   5120     MOV	0x20, R0             	MOV	_RSCTL, R0
                                           ;	::->op :*  =
                                           ;	.line	21; "../UART.c"	TXIF=0;
0000a3   e100     MOVB	#0x00               	BANKSEL	_EIF2_bits
0000a4   640d     CLR	0xd, 4               	CLR	_EIF2_bits, 4
                                           ;	::->op :*  =
                                           ;	.line	22; "../UART.c"	TXIE=0;
                                           	BANKSEL	_EIE2_bits
0000a5   642d     CLR	0x2d, 4              	CLR	_EIE2_bits, 4
                                           ;	::->op :*  =
                                           ;	.line	23; "../UART.c"	RCIF=0;
                                           	BANKSEL	_EIF2_bits
0000a6   650d     CLR	0xd, 5               	CLR	_EIF2_bits, 5
                                           ;	::->op :*  =
                                           ;	.line	24; "../UART.c"	RCIE=1;
                                           	BANKSEL	_EIE2_bits
0000a7   6d2d     SET	0x2d, 5              	SET	_EIE2_bits, 5
                                           ;	::->op :*  =
                                           ;	.line	25; "../UART.c"	AIE=1;	PUIE=1;    // Ê¹ÄÜÍâ²¿ÖÐ¶Ï PUIE Ê¹ÄÜ×ÜÖÐ¶Ï AIE
                                           	BANKSEL	_INTCTL_bits
0000a8   6f0b     SET	0xb, 7               	SET	_INTCTL_bits, 7
                                           ;	::->op :*  =
                                           	BANKSEL	_INTCTL_bits
0000a9   6e0b     SET	0xb, 6               	SET	_INTCTL_bits, 6
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0000aa   0008     CRET                     	CRET	
                                           ; exit point of _UART_Init
                                           
                                           
                                           ;	code size estimation:
                                           ;	   20+   13 =    33 instructions (   92 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Sun Aug 04 20:07:54 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x1dd4
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Sun Aug 04 20:07:55 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_UART_Init
                                           	.extern	_UART_SendBuf
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_UART_BUF
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Sys_Init
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           	.global	_Rev_Flag
                                           	.global	_Rev_StopFlag
                                           	.global	_Rev_count
                                           
                                           	.global I0R1
                                           	.global I0R7
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1R7
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata
                                           I0R1		.res 1
                                           I0R7		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1R7		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_main_0	.udata
                                           _Rev_Flag	.res	1
                                           
                                           UD_main_1	.udata
                                           _Rev_StopFlag	.res	1
                                           
                                           UD_main_2	.udata
                                           _Rev_count	.res	1
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1035	.res	1
                                           UDL_main_1	.udata
                                           r0x1036	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e000     MOVP	#0x00               	PAGESEL	init_imp
000002   c0c3     JMP	#0xc3                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
0000c3   e000     MOVP	#0x00               	PAGESEL	_startup
0000c4   d078     CALL	#0x78               	CALL	_startup
0000c5   e000     MOVP	#0x00               	PAGESEL	__gsinit_startup
0000c6   d0ce     CALL	#0xce               	CALL	__gsinit_startup
0000c7   e000     MOVP	#0x00               	PAGESEL	_main
0000c8   c046     JMP	#0x46                	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           interrupt_0x04	.code	0x4
000004   f8c2     MOV	R2, R0               	MOV		R2,R0
000005   5617     MOV	R3, 0x17             	MOV		R3,BANK
000006   5003     MOV	R0, 0x3              	MOV		R0,PSW
000007   e100     MOVB	#0x00               	BANKSEL	I0PSW
000008   5187     MOV	0x87, R0             	MOV		I0PSW,R0
000009   500a     MOV	R0, 0xa              	MOV		R0,PCH
00000a   e100     MOVB	#0x00               	BANKSEL	I0PCH
00000b   5188     MOV	0x88, R0             	MOV		I0PCH,R0
00000c   5385     MOV	0x85, R1             	MOV		I0R1,R1
00000d   5f86     MOV	0x86, R7             	MOV		I0R7,R7
00000e   e000     MOVP	#0x00               	PAGESEL	interrupt_service_routine_0x04
00000f   c010     JMP	#0x10                	JMP		interrupt_service_routine_0x04
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;2 compiler assigned registers:
                                           ;   r0x1035
                                           ;   r0x1036
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           ;	.line	62; "../main.c"	if(RCIF)
000010   e100     MOVB	#0x00               	BANKSEL	_EIF2_bits
000011   7d0d     JB	0xd, 5                	JB	_EIF2_bits, 5
000012   c03d     JMP	#0x3d                	JMP	_00031_DS_
                                           ;	::->op : +
                                           ;	.line	64; "../main.c"	UART_BUF[Rev_count]=RXSDR;  	//ÇåÁã RXIF
                                           	BANKSEL	_Rev_count
000013   5082     MOV	R0, 0x82             	MOV	R0, _Rev_count
000014   8099     ADD	R0, #0x99            	ADD	R0,# (_UART_BUF + 0)
                                           	BANKSEL	r0x1035
000015   5181     MOV	0x81, R0             	MOV	r0x1035, R0
                                           ;	::->op :*  =
000016   e101     MOVB	#0x01               	BANKSEL	_RXSDR
000017   0e22     MOVZ	R0, 0x22            	MOVZ	R0, _RXSDR
000018   e100     MOVB	#0x00               	BANKSEL	r0x1035
000019   5281     MOV	R1, 0x81             	MOV	R1, r0x1035
                                           	BANKSEL	_UART_BUF
00001a   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : +
                                           ;	.line	65; "../main.c"	if(UART_BUF[Rev_count] == 0x0D)
                                           	BANKSEL	_Rev_count
00001b   5082     MOV	R0, 0x82             	MOV	R0, _Rev_count
00001c   8099     ADD	R0, #0x99            	ADD	R0,# (_UART_BUF + 0)
                                           	BANKSEL	r0x1035
00001d   5181     MOV	0x81, R0             	MOV	r0x1035, R0
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x1035
00001e   5281     MOV	R1, 0x81             	MOV	R1, r0x1035
                                           	BANKSEL	_UART_BUF
00001f   f708     LD	R0, [R1]              	LD	R0, [R1]
                                           	BANKSEL	r0x1036
000020   5180     MOV	0x80, R0             	MOV	r0x1036, R0
                                           ;	::->op : EQ_OP
                                           	BANKSEL	r0x1036
000021   0e80     MOVZ	R0, 0x80            	MOVZ	R0, r0x1036
000022   a80d     XOR	R0, #0xd             	XOR	R0,# 0x0d
000023   7a03     JB	0x3, 2                	JB	PSW, 2
000024   c028     JMP	#0x28                	JMP	_00027_DS_
                                           ;	::->op : =
                                           ;	.line	67; "../main.c"	Rev_StopFlag=1;
000025   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_Rev_StopFlag
000026   5183     MOV	0x83, R0             	MOV	_Rev_StopFlag, R0
                                           ;	::->op : GOTO
000027   c03c     JMP	#0x3c                	JMP	_00028_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : IFX
                                           _00027_DS_
                                           ;	.line	71; "../main.c"	if(Rev_StopFlag)
000028   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	_Rev_StopFlag
000029   3083     ORL	R0, 0x83             	ORL	R0, _Rev_StopFlag
00002a   7203     JNB	0x3, 2               	JNB	PSW, 2
00002b   c03b     JMP	#0x3b                	JMP	_00024_DS_
                                           ;	::->op : +
                                           ;	.line	73; "../main.c"	if(UART_BUF[Rev_count] == 0x0A)
                                           	BANKSEL	_Rev_count
00002c   5082     MOV	R0, 0x82             	MOV	R0, _Rev_count
00002d   8099     ADD	R0, #0x99            	ADD	R0,# (_UART_BUF + 0)
                                           	BANKSEL	r0x1035
00002e   5181     MOV	0x81, R0             	MOV	r0x1035, R0
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x1035
00002f   5281     MOV	R1, 0x81             	MOV	R1, r0x1035
                                           	BANKSEL	_UART_BUF
000030   f708     LD	R0, [R1]              	LD	R0, [R1]
                                           	BANKSEL	r0x1036
000031   5180     MOV	0x80, R0             	MOV	r0x1036, R0
                                           ;	::->op : EQ_OP
                                           	BANKSEL	r0x1036
000032   0e80     MOVZ	R0, 0x80            	MOVZ	R0, r0x1036
000033   a80a     XOR	R0, #0xa             	XOR	R0,# 0x0a
000034   7a03     JB	0x3, 2                	JB	PSW, 2
000035   c039     JMP	#0x39                	JMP	_00021_DS_
                                           ;	::->op : =
                                           ;	.line	74; "../main.c"	Rev_Flag=1;
000036   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_Rev_Flag
000037   5184     MOV	0x84, R0             	MOV	_Rev_Flag, R0
                                           ;	::->op : GOTO
000038   c03c     JMP	#0x3c                	JMP	_00028_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00021_DS_
                                           ;	.line	75; "../main.c"	else Rev_StopFlag=0;
                                           	BANKSEL	_Rev_StopFlag
000039   0383     CLR	0x83                 	CLR	_Rev_StopFlag
                                           ;	::->op : GOTO
00003a   c03c     JMP	#0x3c                	JMP	_00028_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00024_DS_
                                           ;	.line	79; "../main.c"	Rev_StopFlag=0;
                                           	BANKSEL	_Rev_StopFlag
00003b   0383     CLR	0x83                 	CLR	_Rev_StopFlag
                                           ;	::->op : LABEL
                                           ;	::->op : +
                                           _00028_DS_
                                           ;	.line	82; "../main.c"	Rev_count++;
                                           	BANKSEL	_Rev_count
00003c   0b82     INC	0x82                 	INC	_Rev_count
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           _00031_DS_
                                           	BANKSEL	I0R1
00003d   5285     MOV	R1, 0x85             	MOV	R1, I0R1
                                           	BANKSEL	I0R7
00003e   5e86     MOV	R7, 0x86             	MOV	R7, I0R7
                                           	BANKSEL	I0PCH
00003f   5088     MOV	R0, 0x88             	MOV	R0, I0PCH
000040   510a     MOV	0xa, R0              	MOV	PCH, R0
                                           	BANKSEL	I0PSW
000041   5087     MOV	R0, 0x87             	MOV	R0, I0PSW
000042   5103     MOV	0x3, R0              	MOV	PSW, R0
000043   5717     MOV	0x17, R3             	MOV	BANK, R3
000044   f8d0     MOV	R0, R2               	MOV	R0, R2
000045   0009     IRET                     	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00037_DS_
                                           ;	.line	91; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _Sys_Init
                                           ;   _UART_Init
                                           ;   _UART_SendBuf
                                           ;   _UART_SendBuf
                                           ;   _UART_SendBuf
                                           ;   _Sys_Init
                                           ;   _UART_Init
                                           ;   _UART_SendBuf
                                           ;   _UART_SendBuf
                                           ;   _UART_SendBuf
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	::->op : CALL
                                           ;	.line	34; "../main.c"	Sys_Init();
000046   e000     MOVP	#0x00               	PAGESEL	_Sys_Init
000047   d0ab     CALL	#0xab               	CALL	_Sys_Init
000048   e000     MOVP	#0x00               	PAGESEL	$
                                           ;	::->op : CALL
                                           ;	.line	35; "../main.c"	UART_Init();
000049   e000     MOVP	#0x00               	PAGESEL	_UART_Init
00004a   d099     CALL	#0x99               	CALL	_UART_Init
00004b   e000     MOVP	#0x00               	PAGESEL	$
                                           ;	::->op :*  =
                                           ;	.line	36; "../main.c"	AIE=1;			//¿ªÆôÖÐ¶Ï
00004c   e100     MOVB	#0x00               	BANKSEL	_INTCTL_bits
00004d   6f0b     SET	0xb, 7               	SET	_INTCTL_bits, 7
                                           ;	::->op :*  =
                                           ;	.line	37; "../main.c"	PUIE=1;
                                           	BANKSEL	_INTCTL_bits
00004e   6e0b     SET	0xb, 6               	SET	_INTCTL_bits, 6
                                           ;	::->op : LABEL
                                           ;	::->op : EQ_OP
                                           _00011_DS_
                                           ;	.line	40; "../main.c"	if(Rev_Flag == 1)
                                           	BANKSEL	_Rev_Flag
00004f   0e84     MOVZ	R0, 0x84            	MOVZ	R0, _Rev_Flag
000050   a801     XOR	R0, #0x1             	XOR	R0,# 0x01
000051   7a03     JB	0x3, 2                	JB	PSW, 2
000052   c04f     JMP	#0x4f                	JMP	_00011_DS_
                                           ;	::->op : =
                                           ;	.line	42; "../main.c"	Rev_Flag=0;
                                           	BANKSEL	_Rev_Flag
000053   0384     CLR	0x84                 	CLR	_Rev_Flag
                                           ;	::->op : EQ_OP
                                           ;	.line	43; "../main.c"	if(Rev_count == 5)
                                           	BANKSEL	_Rev_count
000054   0e82     MOVZ	R0, 0x82            	MOVZ	R0, _Rev_count
000055   a805     XOR	R0, #0x5             	XOR	R0,# 0x05
000056   7a03     JB	0x3, 2                	JB	PSW, 2
000057   c074     JMP	#0x74                	JMP	_00007_DS_
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           ;	.line	45; "../main.c"	DIVAH = UART_BUF[0];	//×ªÔØÊý¾Ý
                                           	BANKSEL	_UART_BUF
000058   0e99     MOVZ	R0, 0x99            	MOVZ	R0,  (_UART_BUF + 0)
000059   e101     MOVB	#0x01               	BANKSEL	_DIVAH
00005a   513a     MOV	0x3a, R0             	MOV	_DIVAH, R0
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           ;	.line	46; "../main.c"	DIVAL = UART_BUF[1];	//±»³ýÊý
00005b   e100     MOVB	#0x00               	BANKSEL	_UART_BUF
00005c   0e9a     MOVZ	R0, 0x9a            	MOVZ	R0,  (_UART_BUF + 1)
00005d   e101     MOVB	#0x01               	BANKSEL	_DIVAL
00005e   513b     MOV	0x3b, R0             	MOV	_DIVAL, R0
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           ;	.line	47; "../main.c"	DIVB  = UART_BUF[2];	//³ýÊý
00005f   e100     MOVB	#0x00               	BANKSEL	_UART_BUF
000060   0e9b     MOVZ	R0, 0x9b            	MOVZ	R0,  (_UART_BUF + 2)
000061   e101     MOVB	#0x01               	BANKSEL	_DIVB
000062   513c     MOV	0x3c, R0             	MOV	_DIVB, R0
                                           ;	::->op :*  =
                                           ;	.line	48; "../main.c"	DIVEN=1;				//¿ªÊ¼ÔËËã
                                           	BANKSEL	_DIVCTL_bits
000063   6839     SET	0x39, 0              	SET	_DIVCTL_bits, 0
                                           ;	::->op : LABEL
                                           ;	::->op : GET_VALUE_AT_ADDRESS
                                           _00003_DS_
                                           ;	.line	49; "../main.c"	while(!	DIVOEN);
                                           	BANKSEL	_DIVCTL_bits
000064   7939     JB	0x39, 1               	JB	_DIVCTL_bits, 1
000065   c064     JMP	#0x64                	JMP	_00003_DS_
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	51; "../main.c"	UART_SendBuf(DIVQH);	//ÉÌ¸ß
                                           	BANKSEL	_DIVQH
000066   0e3d     MOVZ	R0, 0x3d            	MOVZ	R0, _DIVQH
000067   e000     MOVP	#0x00               	PAGESEL	_UART_SendBuf
000068   d0c9     CALL	#0xc9               	CALL	_UART_SendBuf
000069   e000     MOVP	#0x00               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	52; "../main.c"	UART_SendBuf(DIVQL);	//ÉÌµÍ
00006a   e101     MOVB	#0x01               	BANKSEL	_DIVQL
00006b   0e3e     MOVZ	R0, 0x3e            	MOVZ	R0, _DIVQL
00006c   e000     MOVP	#0x00               	PAGESEL	_UART_SendBuf
00006d   d0c9     CALL	#0xc9               	CALL	_UART_SendBuf
00006e   e000     MOVP	#0x00               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	53; "../main.c"	UART_SendBuf(DIVR);		//ÓàÊý
00006f   e101     MOVB	#0x01               	BANKSEL	_DIVR
000070   0e3f     MOVZ	R0, 0x3f            	MOVZ	R0, _DIVR
000071   e000     MOVP	#0x00               	PAGESEL	_UART_SendBuf
000072   d0c9     CALL	#0xc9               	CALL	_UART_SendBuf
000073   e000     MOVP	#0x00               	PAGESEL	$
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00007_DS_
                                           ;	.line	55; "../main.c"	Rev_count=0;
000074   e100     MOVB	#0x00               	BANKSEL	_Rev_count
000075   0382     CLR	0x82                 	CLR	_Rev_count
                                           ;	::->op : GOTO
000076   c04f     JMP	#0x4f                	JMP	_00011_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
000077   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._Sys_Init	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;	::->op : =
                                           ;	.line	20; "../main.c"	OSCCTL = 0x70;		//Ê±ÖÓÅäÖÃÎªÄÚ²¿16M
0000ab   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
0000ac   e100     MOVB	#0x00               	BANKSEL	_OSCCTL
0000ad   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	::->op : =
                                           ;	.line	21; "../main.c"	TR0=0;
                                           	BANKSEL	_TR0
0000ae   0325     CLR	0x25                 	CLR	_TR0
                                           ;	::->op : =
                                           ;	.line	22; "../main.c"	TR1=0;
                                           	BANKSEL	_TR1
0000af   0327     CLR	0x27                 	CLR	_TR1
                                           ;	::->op : =
                                           ;	.line	23; "../main.c"	TR2=0;
                                           	BANKSEL	_TR2
0000b0   0326     CLR	0x26                 	CLR	_TR2
                                           ;	::->op : =
                                           ;	.line	24; "../main.c"	TR3=0;
                                           	BANKSEL	_TR3
0000b1   0349     CLR	0x49                 	CLR	_TR3
                                           ;	::->op : =
                                           ;	.line	25; "../main.c"	P0=0;
                                           	BANKSEL	_P0
0000b2   0305     CLR	0x5                  	CLR	_P0
                                           ;	::->op : =
                                           ;	.line	26; "../main.c"	P1=0;
                                           	BANKSEL	_P1
0000b3   0307     CLR	0x7                  	CLR	_P1
                                           ;	::->op : =
                                           ;	.line	27; "../main.c"	P2=0;
                                           	BANKSEL	_P2
0000b4   0306     CLR	0x6                  	CLR	_P2
                                           ;	::->op : =
                                           ;	.line	28; "../main.c"	P3=0;
                                           	BANKSEL	_P3
0000b5   0308     CLR	0x8                  	CLR	_P3
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0000b6   0008     CRET                     	CRET	
                                           ; exit point of _Sys_Init
                                           
                                           
                                           ;	code size estimation:
                                           ;	  104+   54 =   158 instructions (  424 byte)
                                           
                                           
                                           	.end
                                           .config
002007   1dd4     XOR	0xd4, R2            
002008   ffff     NOPZ                    
                                           func.__gsinit_startup
0000ce   e000     MOVP	#0x00              
0000cf   d0b7     CALL	#0xb7              
0000d0   e000     MOVP	#0x00              
0000d1   0008     CRET                    
                                           _sartup_A100EON
000078   e01f     MOVP	#0x1F              
000079   e100     MOVB	#0x00              
00007a   dfff     CALL	#0xfff             
00007b   5130     MOV	0x30, R0            
00007c   ffff     NOPZ                    
00007d   ffff     NOPZ                    
00007e   dffe     CALL	#0xffe             
00007f   5137     MOV	0x37, R0            
000080   ffff     NOPZ                    
000081   ffff     NOPZ                    
000082   dffd     CALL	#0xffd             
000083   514c     MOV	0x4c, R0            
000084   ffff     NOPZ                    
000085   ffff     NOPZ                    
000086   dffc     CALL	#0xffc             
000087   514d     MOV	0x4d, R0            
000088   ffff     NOPZ                    
000089   ffff     NOPZ                    
00008a   dffb     CALL	#0xffb             
00008b   512a     MOV	0x2a, R0            
00008c   ffff     NOPZ                    
00008d   e101     MOVB	#0x01              
00008e   dffa     CALL	#0xffa             
00008f   5159     MOV	0x59, R0            
000090   ffff     NOPZ                    
000091   dff9     CALL	#0xff9             
000092   515a     MOV	0x5a, R0            
000093   ffff     NOPZ                    
000094   dff8     CALL	#0xff8             
000095   5165     MOV	0x65, R0            
000096   ffff     NOPZ                    
000097   ffff     NOPZ                    
000098   0008     CRET                    
                                           .cinit
0000b7   e100     MOVB	#0x00              
0000b8   9880     MOV	R0, #0x80           
0000b9   994b     MOV	R1, #0x4b           
0000ba   e000     MOVP	#0x00              
0000bb   d0bd     CALL	#0xbd              
0000bc   0008     CRET                    
0000bd   020a     CLR	R2                  
0000be   f750     ST	[R0], R2             
0000bf   ff10     INC	R0                  
0000c0   ff59     DECJZ	R1                
0000c1   c0be     JMP	#0xbe               
0000c2   0008     CRET                    
