gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 8-2-2019  17:42:46
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 17:42:42 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../Flash.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_FLASH_WRITE_ONE
                                           	.global	_FLASH_WRITE_FUN
                                           	.global	_FLASH_READ_FUN
                                           	.global	_FLASH_READ_ONE
                                           	.global	_FLASH_READ_BUF
                                           	.global	_FLASH_BUFFER
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_Flash_0	.udata
                                           _FLASH_READ_BUF	.res	2
                                           
                                           UD_Flash_1	.udata
                                           _FLASH_BUFFER	.res	32
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_Flash_0	.udata
                                           r0x1030	.res	1
                                           UDL_Flash_1	.udata
                                           r0x1031	.res	1
                                           UDL_Flash_2	.udata
                                           r0x1023	.res	1
                                           UDL_Flash_3	.udata
                                           r0x1022	.res	1
                                           UDL_Flash_4	.udata
                                           r0x1024	.res	1
                                           UDL_Flash_5	.udata
                                           r0x1028	.res	1
                                           UDL_Flash_6	.udata
                                           r0x1027	.res	1
                                           UDL_Flash_7	.udata
                                           r0x102A	.res	1
                                           UDL_Flash_8	.udata
                                           r0x1029	.res	1
                                           UDL_Flash_9	.udata
                                           r0x102B	.res	1
                                           UDL_Flash_10	.udata
                                           r0x102C	.res	1
                                           UDL_Flash_11	.udata
                                           r0x102D	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           
                                           func._FLASH_WRITE_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _FLASH_READ_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;11 compiler assigned registers:
                                           ;   r0x1027
                                           ;   STK00
                                           ;   r0x1028
                                           ;   STK01
                                           ;   r0x1029
                                           ;   STK02
                                           ;   r0x102A
                                           ;   r0x102B
                                           ;   r0x102C
                                           ;   r0x102D
                                           ;   r0x102E
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _FLASH_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	388; "../Flash.c"	void FLASH_WRITE_ONE(unsigned int address,unsigned int value)
0010c3   e100     MOVB	#0x00               	BANKSEL	r0x1027
0010c4   518a     MOV	0x8a, R0             	MOV	r0x1027, R0
                                           	BANKSEL	r0x102C
0010c5   5186     MOV	0x86, R0             	MOV	r0x102C, R0
                                           	BANKSEL	STK00
0010c6   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1028
0010c7   518b     MOV	0x8b, R0             	MOV	r0x1028, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK01
0010c8   0ea5     MOVZ	R0, 0xa5            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1029
0010c9   5188     MOV	0x88, R0             	MOV	r0x1029, R0
                                           	BANKSEL	STK02
0010ca   0ea4     MOVZ	R0, 0xa4            	MOVZ	R0, STK02
                                           	BANKSEL	r0x102A
0010cb   5189     MOV	0x89, R0             	MOV	r0x102A, R0
                                           ;	::->op : BITWISEAND
                                           ;	.line	391; "../Flash.c"	FLASH_READ_FUN(address&0xFFE0,FLASH_BUFFER_MAX);
0010cc   98e0     MOV	R0, #0xe0            	MOV	R0,# 0xe0
                                           	BANKSEL	r0x1028
0010cd   288b     AND	R0, 0x8b             	AND	R0, r0x1028
                                           	BANKSEL	r0x102B
0010ce   5187     MOV	0x87, R0             	MOV	r0x102B, R0
                                           ;;106	MOVZ	R0, r0x1027
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
0010cf   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
0010d0   51a5     MOV	0xa5, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x102B
0010d1   0e87     MOVZ	R0, 0x87            	MOVZ	R0, r0x102B
                                           	BANKSEL	STK00
0010d2   51a6     MOV	0xa6, R0             	MOV	STK00, R0
                                           	BANKSEL	r0x102C
0010d3   0e86     MOVZ	R0, 0x86            	MOVZ	R0, r0x102C
0010d4   e010     MOVP	#0x10               	PAGESEL	_FLASH_READ_FUN
0010d5   d0f4     CALL	#0xf4               	CALL	_FLASH_READ_FUN
0010d6   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : BITWISEAND
                                           ;	.line	393; "../Flash.c"	FLASH_BUFFER[address&0x1F] = value;
0010d7   981f     MOV	R0, #0x1f            	MOV	R0,# 0x1f
0010d8   e100     MOVB	#0x00               	BANKSEL	r0x1028
0010d9   288b     AND	R0, 0x8b             	AND	R0, r0x1028
                                           	BANKSEL	r0x102B
0010da   5187     MOV	0x87, R0             	MOV	r0x102B, R0
                                           	BANKSEL	r0x102C
0010db   0386     CLR	0x86                 	CLR	r0x102C
                                           ;	::->op : LEFT_OP
0010dc   6003     CLR	0x3, 0               	CLR	PSW, 0
                                           	BANKSEL	r0x102B
0010dd   1287     RLCR	0x87                	RLCR	r0x102B
                                           	BANKSEL	r0x102D
0010de   5185     MOV	0x85, R0             	MOV	r0x102D, R0
                                           	BANKSEL	r0x102C
0010df   1286     RLCR	0x86                	RLCR	r0x102C
                                           ;;1	MOV	r0x102E, R0
                                           ;	::->op : +
                                           	BANKSEL	r0x102D
0010e0   5085     MOV	R0, 0x85             	MOV	R0, r0x102D
0010e1   80a7     ADD	R0, #0xa7            	ADD	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x102B
0010e2   5187     MOV	0x87, R0             	MOV	r0x102B, R0
                                           ;	::->op :*  =
                                           	BANKSEL	r0x102A
0010e3   0e89     MOVZ	R0, 0x89            	MOVZ	R0, r0x102A
                                           	BANKSEL	r0x102B
0010e4   5287     MOV	R1, 0x87             	MOV	R1, r0x102B
                                           	BANKSEL	_FLASH_BUFFER
0010e5   f741     ST	[R1], R0              	ST	[R1], R0
0010e6   ff11     INC	R1                   	INC	R1
                                           	BANKSEL	r0x1029
0010e7   0e88     MOVZ	R0, 0x88            	MOVZ	R0, r0x1029
                                           	BANKSEL	_FLASH_BUFFER
0010e8   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : BITWISEAND
                                           ;	.line	395; "../Flash.c"	FLASH_WRITE_FUN(address&0xFFE0,FLASH_BUFFER_MAX);
0010e9   98e0     MOV	R0, #0xe0            	MOV	R0,# 0xe0
                                           	BANKSEL	r0x1028
0010ea   298b     AND	0x8b, R0             	AND	r0x1028, R0
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
0010eb   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
0010ec   51a5     MOV	0xa5, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x1028
0010ed   0e8b     MOVZ	R0, 0x8b            	MOVZ	R0, r0x1028
                                           	BANKSEL	STK00
0010ee   51a6     MOV	0xa6, R0             	MOV	STK00, R0
                                           	BANKSEL	r0x1027
0010ef   0e8a     MOVZ	R0, 0x8a            	MOVZ	R0, r0x1027
0010f0   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_FUN
0010f1   d088     CALL	#0x88               	CALL	_FLASH_WRITE_FUN
0010f2   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0010f3   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_WRITE_ONE
                                           
                                           
                                           
                                           func._FLASH_WRITE_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;7 compiler assigned registers:
                                           ;   r0x1022
                                           ;   STK00
                                           ;   r0x1023
                                           ;   STK01
                                           ;   r0x1024
                                           ;   r0x1025
                                           ;   r0x1026
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _FLASH_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	234; "../Flash.c"	void FLASH_WRITE_FUN(unsigned int address,unsigned char length)
001088   e100     MOVB	#0x00               	BANKSEL	r0x1022
001089   518d     MOV	0x8d, R0             	MOV	r0x1022, R0
                                           	BANKSEL	STK00
00108a   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1023
00108b   518e     MOV	0x8e, R0             	MOV	r0x1023, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK01
00108c   0ea5     MOVZ	R0, 0xa5            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1024
00108d   518c     MOV	0x8c, R0             	MOV	r0x1024, R0
                                           ;	::->op : RIGHT_OP
                                           ;;105	MOVZ	R0, r0x1022
                                           ;;103	MOV	r0x1025, R0
                                           ;;1	CLR	r0x1026
                                           ;	::->op : CAST
                                           ;;104	MOVZ	R0, r0x1025
                                           ;	.line	238; "../Flash.c"	NVMADDRH=(unsigned char) (address>>8);
                                           	BANKSEL	r0x1022
00108e   0e8d     MOVZ	R0, 0x8d            	MOVZ	R0, r0x1022
                                           	BANKSEL	_NVMADDRH
00108f   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	::->op : CAST
                                           ;	.line	239; "../Flash.c"	NVMADDRL=address;
                                           	BANKSEL	r0x1023
001090   0e8e     MOVZ	R0, 0x8e            	MOVZ	R0, r0x1023
                                           	BANKSEL	_NVMADDRL
001091   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
001092   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
001093   660b     CLR	0xb, 6               	CLR _INTCTL,_PUIE
001094   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001095   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
001096   c094     JMP	#0x94                	JMP $-2
                                           	;
001097   9830     MOV	R0, #0x30            	MOV R0,#0x30
001098   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
001099   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
00109a   9ba7     MOV	R3, #0xa7            	MOV R3,#_FLASH_BUFFER
                                           	
                                           ;	::->op : =
                                           ;	.line	258; "../Flash.c"	while(length--)		// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1024
00109b   0e8c     MOVZ	R0, 0x8c            	MOVZ	R0, r0x1024
                                           	BANKSEL	r0x1023
00109c   518e     MOV	0x8e, R0             	MOV	r0x1023, R0
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00011_DS_
                                           	BANKSEL	r0x1023
00109d   0e8e     MOVZ	R0, 0x8e            	MOVZ	R0, r0x1023
                                           	BANKSEL	r0x1022
00109e   518d     MOV	0x8d, R0             	MOV	r0x1022, R0
                                           ;	::->op : -
                                           	BANKSEL	r0x1023
00109f   078e     DEC	0x8e                 	DEC	r0x1023
                                           ;	::->op : IFX
0010a0   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1022
0010a1   308d     ORL	R0, 0x8d             	ORL	R0, r0x1022
0010a2   7203     JNB	0x3, 2               	JNB	PSW, 2
0010a3   c0bf     JMP	#0xbf                	JMP	_00013_DS_
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _FLASH_BUFFER
0010a4   f71e     LD	R6, [R3]              	LD R6,[R3]
0010a5   ff13     INC	R3                   	INC R3
0010a6   f71f     LD	R7, [R3]              	LD R7,[R3]
0010a7   ff13     INC	R3                   	INC R3
                                           	BANKSEL _NVMDATAH
0010a8   5f38     MOV	0x38, R7             	MOV _NVMDATAH,R7
0010a9   5d39     MOV	0x39, R6             	MOV _NVMDATAL,R6
                                           	;
0010aa   9d84     MOV	R5, #0x84            	MOV R5 ,#0x84
0010ab   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
0010ac   9d69     MOV	R5, #0x69            	MOV R5,#0x69
0010ad   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
0010ae   9d96     MOV	R5, #0x96            	MOV R5,#0x96
0010af   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
0010b0   693c     SET	0x3c, 1              	SET _NVMCTL0 , 1 ;
0010b1   ffff     NOPZ                     	NOPZ
0010b2   ffff     NOPZ                     	NOPZ
0010b3   ffff     NOPZ                     	NOPZ
0010b4   ffff     NOPZ                     	NOPZ
0010b5   ffff     NOPZ                     	NOPZ
0010b6   ffff     NOPZ                     	NOPZ ;
0010b7   ffff     NOPZ                     	NOPZ
0010b8   ffff     NOPZ                     	NOPZ
0010b9   ffff     NOPZ                     	NOPZ
0010ba   ffff     NOPZ                     	NOPZ
0010bb   9d80     MOV	R5, #0x80            	MOV R5,#0X80
0010bc   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
                                           	;
                                           	BANKSEL _NVMADDRL
0010bd   0b3b     INC	0x3b                 	INC _NVMADDRL
                                           	
                                           ;	::->op : GOTO
0010be   c09d     JMP	#0x9d                	JMP	_00011_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : INLINEASM
                                           _00013_DS_
                                           	;
                                           	BANKSEL _OSCCTL
0010bf   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
0010c0   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
0010c1   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
0010c2   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_WRITE_FUN
                                           
                                           
                                           
                                           func._FLASH_READ_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;7 compiler assigned registers:
                                           ;   r0x1022
                                           ;   STK00
                                           ;   r0x1023
                                           ;   STK01
                                           ;   r0x1024
                                           ;   r0x1025
                                           ;   r0x1026
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _FLASH_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;	.line	104; "../Flash.c"	void FLASH_READ_FUN(unsigned int address,unsigned char length)
0010f4   e100     MOVB	#0x00               	BANKSEL	r0x1022
0010f5   518d     MOV	0x8d, R0             	MOV	r0x1022, R0
                                           	BANKSEL	STK00
0010f6   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1023
0010f7   518e     MOV	0x8e, R0             	MOV	r0x1023, R0
                                           ;	::->op : RECEIVE
                                           	BANKSEL	STK01
0010f8   0ea5     MOVZ	R0, 0xa5            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1024
0010f9   518c     MOV	0x8c, R0             	MOV	r0x1024, R0
                                           ;	::->op : RIGHT_OP
                                           ;;102	MOVZ	R0, r0x1022
                                           ;;100	MOV	r0x1025, R0
                                           ;;1	CLR	r0x1026
                                           ;	::->op : CAST
                                           ;;101	MOVZ	R0, r0x1025
                                           ;	.line	108; "../Flash.c"	NVMADDRH=(unsigned char) (address>>8);
                                           	BANKSEL	r0x1022
0010fa   0e8d     MOVZ	R0, 0x8d            	MOVZ	R0, r0x1022
                                           	BANKSEL	_NVMADDRH
0010fb   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	::->op : CAST
                                           ;	.line	109; "../Flash.c"	NVMADDRL=address;
                                           	BANKSEL	r0x1023
0010fc   0e8e     MOVZ	R0, 0x8e            	MOVZ	R0, r0x1023
                                           	BANKSEL	_NVMADDRL
0010fd   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
0010fe   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
0010ff   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001100   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
001101   c0ff     JMP	#0xff                	JMP $-2
                                           	;
001102   9830     MOV	R0, #0x30            	MOV R0,#0x30
001103   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
001104   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
001105   9ba7     MOV	R3, #0xa7            	MOV R3,#_FLASH_BUFFER
                                           	
                                           ;	::->op : =
                                           ;	.line	127; "../Flash.c"	while(length--)	// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1024
001106   0e8c     MOVZ	R0, 0x8c            	MOVZ	R0, r0x1024
                                           	BANKSEL	r0x1023
001107   518e     MOV	0x8e, R0             	MOV	r0x1023, R0
                                           ;	::->op : LABEL
                                           ;	::->op : =
                                           _00003_DS_
                                           	BANKSEL	r0x1023
001108   0e8e     MOVZ	R0, 0x8e            	MOVZ	R0, r0x1023
                                           	BANKSEL	r0x1022
001109   518d     MOV	0x8d, R0             	MOV	r0x1022, R0
                                           ;	::->op : -
                                           	BANKSEL	r0x1023
00110a   078e     DEC	0x8e                 	DEC	r0x1023
                                           ;	::->op : IFX
00110b   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1022
00110c   308d     ORL	R0, 0x8d             	ORL	R0, r0x1022
00110d   7203     JNB	0x3, 2               	JNB	PSW, 2
00110e   c11f     JMP	#0x11f               	JMP	_00005_DS_
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _NVMCTL0
00110f   9d81     MOV	R5, #0x81            	MOV R5,#0x81
001110   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001111   ffff     NOPZ                     	NOPZ
001112   ffff     NOPZ                     	NOPZ
001113   ffff     NOPZ                     	NOPZ ;
001114   ffff     NOPZ                     	NOPZ
                                           	;
                                           	BANKSEL _NVMDATAL
001115   5c39     MOV	R6, 0x39             	MOV R6,_NVMDATAL
001116   5e38     MOV	R7, 0x38             	MOV R7,_NVMDATAH
                                           	BANKSEL _FLASH_BUFFER
001117   f773     ST	[R3], R6              	ST [R3],R6
001118   ff13     INC	R3                   	INC R3
001119   f77b     ST	[R3], R7              	ST [R3],R7
00111a   ff13     INC	R3                   	INC R3
                                           	;
                                           	BANKSEL _NVMADDRL
00111b   0b3b     INC	0x3b                 	INC _NVMADDRL
00111c   7203     JNB	0x3, 2               	JNB _PSW,_Z
00111d   0b3a     INC	0x3a                 	INC _NVMADDRH
                                           	
                                           ;	::->op : GOTO
00111e   c108     JMP	#0x108               	JMP	_00003_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : INLINEASM
                                           _00005_DS_
                                           	;
                                           	BANKSEL _OSCCTL
00111f   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
001120   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
001121   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
001122   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_READ_FUN
                                           
                                           
                                           
                                           func._FLASH_READ_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x102F
                                           ;   STK00
                                           ;   r0x1030
                                           ;   r0x1031
                                           ;   r0x1032
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _FLASH_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;	::->op : RECEIVE
                                           ;;1	MOV	r0x102F, R0
                                           ;	.line	12; "../Flash.c"	unsigned int FLASH_READ_ONE(unsigned int address)
001144   e100     MOVB	#0x00               	BANKSEL	r0x1031
001145   518f     MOV	0x8f, R0             	MOV	r0x1031, R0
                                           	BANKSEL	STK00
001146   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1030
001147   5190     MOV	0x90, R0             	MOV	r0x1030, R0
                                           ;	::->op : RIGHT_OP
                                           ;;99	MOVZ	R0, r0x102F
                                           ;;1	CLR	r0x1032
                                           ;	::->op : CAST
                                           ;	.line	18; "../Flash.c"	NVMADDRH=(unsigned char)(address>>8);
                                           	BANKSEL	r0x1031
001148   0e8f     MOVZ	R0, 0x8f            	MOVZ	R0, r0x1031
                                           	BANKSEL	_NVMADDRH
001149   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	::->op : CAST
                                           ;	.line	19; "../Flash.c"	NVMADDRL=(unsigned char)address;
                                           	BANKSEL	r0x1030
00114a   0e90     MOVZ	R0, 0x90            	MOVZ	R0, r0x1030
                                           	BANKSEL	_NVMADDRL
00114b   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	::->op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
00114c   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
00114d   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
00114e   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
00114f   c14d     JMP	#0x14d               	JMP $-2
                                           	;
001150   9830     MOV	R0, #0x30            	MOV R0,#0x30
001151   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
001152   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
                                           	BANKSEL _NVMCTL0
001153   9d81     MOV	R5, #0x81            	MOV R5,#0x81
001154   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001155   ffff     NOPZ                     	NOPZ
001156   ffff     NOPZ                     	NOPZ
001157   ffff     NOPZ                     	NOPZ
001158   ffff     NOPZ                     	NOPZ
                                           	;
001159   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
00115a   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
00115b   330b     ORL	0xb, R1              	ORL INTCTL,R1
                                           	;
                                           	BANKSEL _NVMDATAL
00115c   5c39     MOV	R6, 0x39             	MOV R6,_NVMDATAL
00115d   5e38     MOV	R7, 0x38             	MOV R7,_NVMDATAH
                                           	BANKSEL _FLASH_READ_BUF
00115e   5d91     MOV	0x91, R6             	MOV (_FLASH_READ_BUF),R6
00115f   5f92     MOV	0x92, R7             	MOV (_FLASH_READ_BUF+1),R7
                                           	
                                           ;	::->op : RETURN
                                           ;	.line	52; "../Flash.c"	return 	FLASH_READ_BUF;
                                           	BANKSEL	_FLASH_READ_BUF
001160   0e91     MOVZ	R0, 0x91            	MOVZ	R0, _FLASH_READ_BUF
                                           	BANKSEL	STK00
001161   51a6     MOV	0xa6, R0             	MOV	STK00, R0
                                           	BANKSEL	_FLASH_READ_BUF
001162   0e92     MOVZ	R0, 0x92            	MOVZ	R0, (_FLASH_READ_BUF + 1)
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
001163   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_READ_ONE
                                           
                                           
                                           ;	code size estimation:
                                           ;	   98+   72 =   170 instructions (  484 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 17:42:43 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x1dd4
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0R7
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1R7
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : ChipON  inc.
                                           ; Version 3.0.4#6752 (Feb 19 2019 20:27:19) (MSVC)
                                           ; This file was generated Fri Aug 02 17:42:45 2019
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.radix dec
                                           	.include "KF8A100EON.inc"
                                           ;************************************************************
                                           ;       Header file for the KungFu8
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           T0			.EQU                 0x01
                                           PCL			.EQU                 0x02
                                           PSW			.EQU                 0x03
                                           P0			.EQU                 0x05
                                           P2			.EQU                 0x06
                                           P1			.EQU                 0x07
                                           P3			.EQU                 0x08
                                           PCH			.EQU                 0x0A
                                           INTCTL			.EQU                 0x0B
                                           EIF1			.EQU                 0x0C
                                           EIF2			.EQU                 0x0D
                                           T1L			.EQU                 0x0E
                                           T1H			.EQU                 0x0F
                                           T1CTL			.EQU                 0x10
                                           T2L			.EQU                 0x11
                                           T2CTL0			.EQU                 0x12
                                           PWM1L			.EQU                 0x13
                                           PWM1H			.EQU                 0x14
                                           PWMCTL			.EQU                 0x15
                                           PP1			.EQU                 0x16
                                           BANK			.EQU                 0x17
                                           ADSCANCTL		.EQU                 0x18
                                           C1CTL			.EQU                 0x19
                                           VDACS			.EQU                 0x1A
                                           AMPCTL			.EQU                 0x1B
                                           ANSEH			.EQU                 0x1D
                                           ADCDATA0H		.EQU                 0x1E
                                           ADCCTL0			.EQU                 0x1F
                                           AMPDT			.EQU                 0x20
                                           OPTR			.EQU                 0x21
                                           IP0			.EQU                 0x22
                                           IP1			.EQU                 0x23
                                           IP2			.EQU                 0x24
                                           TR0			.EQU                 0x25
                                           TR2			.EQU                 0x26
                                           TR1			.EQU                 0x27
                                           OSCSTA			.EQU                 0x28
                                           IP3			.EQU                 0x29
                                           VRECAL1			.EQU                 0x2A
                                           VRECTL			.EQU                 0x2B
                                           EIE1			.EQU                 0x2C
                                           EIE2			.EQU                 0x2D
                                           PCTL			.EQU                 0x2E
                                           OSCCTL			.EQU                 0x2F
                                           OSCCAL0			.EQU                 0x30
                                           ANSEL			.EQU                 0x31
                                           PP2			.EQU                 0x32
                                           PWM2L			.EQU                 0x33
                                           PWM2H			.EQU                 0x34
                                           PUR0			.EQU                 0x35
                                           IOCL			.EQU                 0x36
                                           OSCCAL1			.EQU                 0x37
                                           NVMDATAH		.EQU                 0x38
                                           NVMDATAL		.EQU                 0x39
                                           NVMADDRH		.EQU                 0x3A
                                           NVMADDRL		.EQU                 0x3B
                                           NVMCTL0			.EQU                 0x3C
                                           NVMCTL1			.EQU                 0x3D
                                           ADCDATA0L		.EQU                 0x3E
                                           ADCCTL1			.EQU                 0x3F
                                           T2CCRH			.EQU                 0x40
                                           T2H			.EQU                 0x41
                                           PP5H			.EQU                 0x42
                                           PWM5H0			.EQU                 0x43
                                           PWM5H1			.EQU                 0x44
                                           P0LR			.EQU                 0x45
                                           P2LR			.EQU                 0x46
                                           P1LR			.EQU                 0x47
                                           P3LR			.EQU                 0x48
                                           TR3			.EQU                 0x49
                                           EIE3			.EQU                 0x4A
                                           EIF3			.EQU                 0x4B
                                           OSCCAL2			.EQU                 0x4C
                                           OSCCAL3			.EQU                 0x4D
                                           T3CTL			.EQU                 0x4E
                                           T3L			.EQU                 0x4F
                                           PP5L			.EQU                 0x52
                                           T3CTL1			.EQU                 0x53
                                           T2CCRL			.EQU                 0x54
                                           PWM5L0			.EQU                 0x55
                                           PWM5L1			.EQU                 0x56
                                           PWM5CTL0		.EQU                 0x57
                                           PWM5CTL1		.EQU                 0x5B
                                           P5ASCTL			.EQU                 0x5C
                                           PSTRCTL			.EQU                 0x5D
                                           T3H			.EQU                 0x5F
                                           PUR1			.EQU                 0x60
                                           PUR2			.EQU                 0x61
                                           INTEDGCTL		.EQU                 0x67
                                           VBIASCTL		.EQU                 0x6B
                                           VBIAS1EN		.EQU                 0x6C
                                           VBIAS2EN		.EQU                 0x6D
                                           PWM5OC			.EQU                 0x10E
                                           T2CTL1			.EQU                 0x10F
                                           VDAC			.EQU                 0x112
                                           PWM5CTL2		.EQU                 0x11C
                                           PWM5PC			.EQU                 0x11D
                                           RSCTL			.EQU                 0x120
                                           TXSDR			.EQU                 0x121
                                           RXSDR			.EQU                 0x122
                                           BRCTL			.EQU                 0x123
                                           TSCTL			.EQU                 0x124
                                           EUBRGL			.EQU                 0x125
                                           EUBRGH			.EQU                 0x126
                                           SSCICTL0		.EQU                 0x128
                                           SSCICTL1		.EQU                 0x12A
                                           SSCISTA			.EQU                 0x12B
                                           SSCIBUFR		.EQU                 0x12C
                                           SSCIADD			.EQU                 0x12E
                                           SSCIMSK			.EQU                 0x12E
                                           WDTPS			.EQU                 0x12F
                                           MULAH			.EQU                 0x130
                                           MULAL			.EQU                 0x131
                                           MULBH			.EQU                 0x132
                                           MULBL			.EQU                 0x133
                                           MULCTL			.EQU                 0x134
                                           MULRES3			.EQU                 0x135
                                           MULRES2			.EQU                 0x136
                                           MULRES1			.EQU                 0x137
                                           MULRES0			.EQU                 0x138
                                           DIVCTL			.EQU                 0x139
                                           DIVAH			.EQU                 0x13A
                                           DIVAL			.EQU                 0x13B
                                           DIVB			.EQU                 0x13C
                                           DIVQH			.EQU                 0x13D
                                           DIVQL			.EQU                 0x13E
                                           DIVR			.EQU                 0x13F
                                           LEDCTL			.EQU                 0x140
                                           LEDPRE			.EQU                 0x141
                                           LEDDATA0		.EQU                 0x142
                                           LEDDATA1		.EQU                 0x143
                                           LEDDATA2		.EQU                 0x144
                                           LEDDATA3		.EQU                 0x145
                                           LEDDATA4		.EQU                 0x146
                                           LEDDATA5		.EQU                 0x147
                                           LEDDATA6		.EQU                 0x148
                                           LEDDATA7		.EQU                 0x149
                                           C1FILTCTL		.EQU                 0x14A
                                           C1FILTPRE		.EQU                 0x14B
                                           LEDOMS1			.EQU                 0x150
                                           CCRL			.EQU                 0x151
                                           CCPCTL			.EQU                 0x152
                                           CCRH			.EQU                 0x154
                                           LEDODS0			.EQU                 0x155
                                           LEDOMS0			.EQU                 0x157
                                           LEDODS1			.EQU                 0x158
                                           VRECAL2			.EQU                 0x159
                                           VRECAL3			.EQU                 0x15A
                                           LEDLUM			.EQU                 0x15C
                                           PWM5FC			.EQU                 0x15D
                                           T4L			.EQU                 0x160
                                           T4H			.EQU                 0x161
                                           T4REL			.EQU                 0x162
                                           T4REH			.EQU                 0x163
                                           T4CTL			.EQU                 0x164
                                           RC32KCAL		.EQU                 0x165
                                           
                                           
                                           ;  03H  PSW   Bits-------------------------------------
                                           TO			.EQU                4
                                           PD			.EQU                3
                                           Z			.EQU                2
                                           DC			.EQU                1
                                           CY			.EQU                0
                                           _TO			.EQU                4
                                           _PD			.EQU                3
                                           _Z			.EQU                2
                                           _DC			.EQU                1
                                           _CY			.EQU                0
                                           
                                           ;  05H  P0   Bits-------------------------------------
                                           P05			.EQU                5
                                           P04			.EQU                4
                                           P03			.EQU                3
                                           P02			.EQU                2
                                           P01			.EQU                1
                                           P00			.EQU                0
                                           _P05			.EQU                5
                                           _P04			.EQU                4
                                           _P03			.EQU                3
                                           _P02			.EQU                2
                                           _P01			.EQU                1
                                           _P00			.EQU                0
                                           
                                           ;  06H  P2   Bits-------------------------------------
                                           P27			.EQU                7
                                           P26			.EQU                6
                                           P25			.EQU                5
                                           P24			.EQU                4
                                           P23			.EQU                3
                                           P22			.EQU                2
                                           P21			.EQU                1
                                           P20			.EQU                0
                                           _P27			.EQU                7
                                           _P26			.EQU                6
                                           _P25			.EQU                5
                                           _P24			.EQU                4
                                           _P23			.EQU                3
                                           _P22			.EQU                2
                                           _P21			.EQU                1
                                           _P20			.EQU                0
                                           
                                           ;  07H  P1   Bits-------------------------------------
                                           P17			.EQU                7
                                           P16			.EQU                6
                                           P15			.EQU                5
                                           P14			.EQU                4
                                           P13			.EQU                3
                                           P12			.EQU                2
                                           P11			.EQU                1
                                           P10			.EQU                0
                                           _P17			.EQU                7
                                           _P16			.EQU                6
                                           _P15			.EQU                5
                                           _P14			.EQU                4
                                           _P13			.EQU                3
                                           _P12			.EQU                2
                                           _P11			.EQU                1
                                           _P10			.EQU                0
                                           
                                           ;  08H  P3   Bits-------------------------------------
                                           P37			.EQU                7
                                           P36			.EQU                6
                                           P35			.EQU                5
                                           P34			.EQU                4
                                           P33			.EQU                3
                                           P32			.EQU                2
                                           P31			.EQU                1
                                           P30			.EQU                0
                                           _P37			.EQU                7
                                           _P36			.EQU                6
                                           _P35			.EQU                5
                                           _P34			.EQU                4
                                           _P33			.EQU                3
                                           _P32			.EQU                2
                                           _P31			.EQU                1
                                           _P30			.EQU                0
                                           
                                           ;  0AH  PCH   Bits-------------------------------------
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIE			.EQU                7
                                           PUIE			.EQU                6
                                           T0IE			.EQU                5
                                           INT0IE			.EQU                4
                                           P0IE			.EQU                3
                                           T0IF			.EQU                2
                                           INT0IF			.EQU                1
                                           P0IF			.EQU                0
                                           _AIE			.EQU                7
                                           _PUIE			.EQU                6
                                           _T0IE			.EQU                5
                                           _INT0IE			.EQU                4
                                           _P0IE			.EQU                3
                                           _T0IF			.EQU                2
                                           _INT0IF			.EQU                1
                                           _P0IF			.EQU                0
                                           
                                           ;  0BH  INTCTL   Bits-------------------------------------
                                           AIEH			.EQU                7
                                           AIEL			.EQU                6
                                           _AIEH			.EQU                7
                                           _AIEL			.EQU                6
                                           
                                           ;  0CH  EIF1   Bits-------------------------------------
                                           EEIF			.EQU                7
                                           ADIF			.EQU                6
                                           INT2IF			.EQU                5
                                           INT1IF			.EQU                4
                                           C1IF			.EQU                3
                                           PWM2IF			.EQU                2
                                           T2IF			.EQU                1
                                           T1IF			.EQU                0
                                           _EEIF			.EQU                7
                                           _ADIF			.EQU                6
                                           _INT2IF			.EQU                5
                                           _INT1IF			.EQU                4
                                           _C1IF			.EQU                3
                                           _PWM2IF			.EQU                2
                                           _T2IF			.EQU                1
                                           _T1IF			.EQU                0
                                           
                                           ;  0DH  EIF2   Bits-------------------------------------
                                           T3IF			.EQU                7
                                           RCIF			.EQU                5
                                           TXIF			.EQU                4
                                           CCPIF			.EQU                2
                                           BCLIF			.EQU                1
                                           SSCIIF			.EQU                0
                                           _T3IF			.EQU                7
                                           _RCIF			.EQU                5
                                           _TXIF			.EQU                4
                                           _CCPIF			.EQU                2
                                           _BCLIF			.EQU                1
                                           _SSCIIF			.EQU                0
                                           
                                           ;  10H  T1CTL   Bits-------------------------------------
                                           T1RLD			.EQU                7
                                           T1GC			.EQU                6
                                           T1CKS1			.EQU                5
                                           T1CKS0			.EQU                4
                                           T1OSCEN			.EQU                3
                                           T1SY			.EQU                2
                                           T1CS			.EQU                1
                                           T1ON			.EQU                0
                                           _T1RLD			.EQU                7
                                           _T1GC			.EQU                6
                                           _T1CKS1			.EQU                5
                                           _T1CKS0			.EQU                4
                                           _T1OSCEN		.EQU                3
                                           _T1SY			.EQU                2
                                           _T1CS			.EQU                1
                                           _T1ON			.EQU                0
                                           
                                           ;  12H  T2CTL0   Bits-------------------------------------
                                           T2CKBS3			.EQU                6
                                           T2CKBS2			.EQU                5
                                           T2CKBS1			.EQU                4
                                           T2CKBS0			.EQU                3
                                           T2ON			.EQU                2
                                           T2CKPS1			.EQU                1
                                           T2CKPS0			.EQU                0
                                           _T2CKBS3		.EQU                6
                                           _T2CKBS2		.EQU                5
                                           _T2CKBS1		.EQU                4
                                           _T2CKBS0		.EQU                3
                                           _T2ON			.EQU                2
                                           _T2CKPS1		.EQU                1
                                           _T2CKPS0		.EQU                0
                                           
                                           ;  15H  PWMCTL   Bits-------------------------------------
                                           PWM2ON			.EQU                4
                                           PWM1ON			.EQU                0
                                           _PWM2ON			.EQU                4
                                           _PWM1ON			.EQU                0
                                           
                                           ;  17H  BANK   Bits-------------------------------------
                                           PR3			.EQU                3
                                           PR2			.EQU                2
                                           PR1			.EQU                1
                                           PR0			.EQU                0
                                           _PR3			.EQU                3
                                           _PR2			.EQU                2
                                           _PR1			.EQU                1
                                           _PR0			.EQU                0
                                           
                                           ;  18H  ADSCANCTL   Bits-------------------------------------
                                           ADSCANEN		.EQU                7
                                           SMOD1			.EQU                6
                                           SMOD0			.EQU                5
                                           STIM4			.EQU                4
                                           STIM3			.EQU                3
                                           STIM2			.EQU                2
                                           STIM1			.EQU                1
                                           STIM0			.EQU                0
                                           _ADSCANEN		.EQU                7
                                           _SMOD1			.EQU                6
                                           _SMOD0			.EQU                5
                                           _STIM4			.EQU                4
                                           _STIM3			.EQU                3
                                           _STIM2			.EQU                2
                                           _STIM1			.EQU                1
                                           _STIM0			.EQU                0
                                           
                                           ;  19H  C1CTL   Bits-------------------------------------
                                           C1MOD2			.EQU                6
                                           C1MOD1			.EQU                5
                                           C1MOD0			.EQU                4
                                           C1OUT			.EQU                1
                                           C1EN			.EQU                0
                                           _C1MOD2			.EQU                6
                                           _C1MOD1			.EQU                5
                                           _C1MOD0			.EQU                4
                                           _C1OUT			.EQU                1
                                           _C1EN			.EQU                0
                                           
                                           ;  1AH  VDACS   Bits-------------------------------------
                                           VCEN			.EQU                6
                                           _VCEN			.EQU                6
                                           
                                           ;  1BH  AMPCTL   Bits-------------------------------------
                                           AMPCALD			.EQU                7
                                           INPS1			.EQU                5
                                           INPS0			.EQU                4
                                           AMPCALEN		.EQU                1
                                           AMPON			.EQU                0
                                           _AMPCALD		.EQU                7
                                           _INPS1			.EQU                5
                                           _INPS0			.EQU                4
                                           _AMPCALEN		.EQU                1
                                           _AMPON			.EQU                0
                                           
                                           ;  1DH  ANSEH   Bits-------------------------------------
                                           ANS13			.EQU                5
                                           ANS12			.EQU                4
                                           ANS11			.EQU                3
                                           ANS10			.EQU                2
                                           ANS9			.EQU                1
                                           ANS8			.EQU                0
                                           _ANS13			.EQU                5
                                           _ANS12			.EQU                4
                                           _ANS11			.EQU                3
                                           _ANS10			.EQU                2
                                           _ANS9			.EQU                1
                                           _ANS8			.EQU                0
                                           
                                           ;  1FH  ADCCTL0   Bits-------------------------------------
                                           ADLR			.EQU                7
                                           T2CCRON			.EQU                6
                                           CHS3			.EQU                5
                                           CHS2			.EQU                4
                                           CHS1			.EQU                3
                                           CHS0			.EQU                2
                                           START			.EQU                1
                                           ADEN			.EQU                0
                                           _ADLR			.EQU                7
                                           _T2CCRON		.EQU                6
                                           _CHS3			.EQU                5
                                           _CHS2			.EQU                4
                                           _CHS1			.EQU                3
                                           _CHS0			.EQU                2
                                           _START			.EQU                1
                                           _ADEN			.EQU                0
                                           
                                           ;  20H  AMPDT   Bits-------------------------------------
                                           AMPDT7			.EQU                7
                                           AMPDT6			.EQU                6
                                           AMPDT5			.EQU                5
                                           AMPDT4			.EQU                4
                                           AMPDT3			.EQU                3
                                           AMPDT2			.EQU                2
                                           AMPDT1			.EQU                1
                                           AMPDT0			.EQU                0
                                           _AMPDT7			.EQU                7
                                           _AMPDT6			.EQU                6
                                           _AMPDT5			.EQU                5
                                           _AMPDT4			.EQU                4
                                           _AMPDT3			.EQU                3
                                           _AMPDT2			.EQU                2
                                           _AMPDT1			.EQU                1
                                           _AMPDT0			.EQU                0
                                           
                                           ;  21H  OPTR   Bits-------------------------------------
                                           PUPH			.EQU                7
                                           INT0SE			.EQU                6
                                           T0CS			.EQU                5
                                           T0SE			.EQU                4
                                           PSA			.EQU                3
                                           PS2			.EQU                2
                                           PS1			.EQU                1
                                           PS0			.EQU                0
                                           _PUPH			.EQU                7
                                           _INT0SE			.EQU                6
                                           _T0CS			.EQU                5
                                           _T0SE			.EQU                4
                                           _PSA			.EQU                3
                                           _PS2			.EQU                2
                                           _PS1			.EQU                1
                                           _PS0			.EQU                0
                                           
                                           ;  22H  IP0   Bits-------------------------------------
                                           PT0			.EQU                2
                                           PINT0			.EQU                1
                                           PP0			.EQU                0
                                           _PT0			.EQU                2
                                           _PINT0			.EQU                1
                                           _PP0			.EQU                0
                                           
                                           ;  23H  IP1   Bits-------------------------------------
                                           PEE			.EQU                7
                                           PADC			.EQU                6
                                           PINT2			.EQU                5
                                           PINT1			.EQU                4
                                           PC1			.EQU                3
                                           PPWM2			.EQU                2
                                           PT2			.EQU                1
                                           PT1			.EQU                0
                                           _PEE			.EQU                7
                                           _PADC			.EQU                6
                                           _PINT2			.EQU                5
                                           _PINT1			.EQU                4
                                           _PC1			.EQU                3
                                           _PPWM2			.EQU                2
                                           _PT2			.EQU                1
                                           _PT1			.EQU                0
                                           
                                           ;  24H  IP2   Bits-------------------------------------
                                           PT3			.EQU                7
                                           PRC			.EQU                5
                                           PTX			.EQU                4
                                           PCCP			.EQU                2
                                           PBCL			.EQU                1
                                           PSSCI			.EQU                0
                                           _PT3			.EQU                7
                                           _PRC			.EQU                5
                                           _PTX			.EQU                4
                                           _PCCP			.EQU                2
                                           _PBCL			.EQU                1
                                           _PSSCI			.EQU                0
                                           
                                           ;  25H  TR0   Bits-------------------------------------
                                           TR05			.EQU                5
                                           TR04			.EQU                4
                                           TR03			.EQU                3
                                           TR02			.EQU                2
                                           TR01			.EQU                1
                                           TR00			.EQU                0
                                           _TR05			.EQU                5
                                           _TR04			.EQU                4
                                           _TR03			.EQU                3
                                           _TR02			.EQU                2
                                           _TR01			.EQU                1
                                           _TR00			.EQU                0
                                           
                                           ;  26H  TR2   Bits-------------------------------------
                                           TR27			.EQU                7
                                           TR26			.EQU                6
                                           TR25			.EQU                5
                                           TR24			.EQU                4
                                           TR23			.EQU                3
                                           TR22			.EQU                2
                                           TR21			.EQU                1
                                           TR20			.EQU                0
                                           _TR27			.EQU                7
                                           _TR26			.EQU                6
                                           _TR25			.EQU                5
                                           _TR24			.EQU                4
                                           _TR23			.EQU                3
                                           _TR22			.EQU                2
                                           _TR21			.EQU                1
                                           _TR20			.EQU                0
                                           
                                           ;  27H  TR1   Bits-------------------------------------
                                           TR17			.EQU                7
                                           TR16			.EQU                6
                                           TR15			.EQU                5
                                           TR14			.EQU                4
                                           TR13			.EQU                3
                                           TR12			.EQU                2
                                           TR11			.EQU                1
                                           TR10			.EQU                0
                                           _TR17			.EQU                7
                                           _TR16			.EQU                6
                                           _TR15			.EQU                5
                                           _TR14			.EQU                4
                                           _TR13			.EQU                3
                                           _TR12			.EQU                2
                                           _TR11			.EQU                1
                                           _TR10			.EQU                0
                                           
                                           ;  28H  OSCSTA   Bits-------------------------------------
                                           OSTS			.EQU                6
                                           HTS			.EQU                5
                                           LTS			.EQU                4
                                           SCF1			.EQU                1
                                           SCF0			.EQU                0
                                           _OSTS			.EQU                6
                                           _HTS			.EQU                5
                                           _LTS			.EQU                4
                                           _SCF1			.EQU                1
                                           _SCF0			.EQU                0
                                           
                                           ;  29H  IP3   Bits-------------------------------------
                                           PT4			.EQU                7
                                           POSCFAIL		.EQU                5
                                           _PT4			.EQU                7
                                           _POSCFAIL		.EQU                5
                                           
                                           ;  2BH  VRECTL   Bits-------------------------------------
                                           VRESEL1			.EQU                7
                                           VRESEL0			.EQU                6
                                           VRECKEN			.EQU                4
                                           VREOE			.EQU                3
                                           VREEN			.EQU                1
                                           _VRESEL1		.EQU                7
                                           _VRESEL0		.EQU                6
                                           _VRECKEN		.EQU                4
                                           _VREOE			.EQU                3
                                           _VREEN			.EQU                1
                                           
                                           ;  2CH  EIE1   Bits-------------------------------------
                                           EEIE			.EQU                7
                                           ADIE			.EQU                6
                                           INT2IE			.EQU                5
                                           INT1IE			.EQU                4
                                           C1IE			.EQU                3
                                           PWM2IE			.EQU                2
                                           T2IE			.EQU                1
                                           T1IE			.EQU                0
                                           _EEIE			.EQU                7
                                           _ADIE			.EQU                6
                                           _INT2IE			.EQU                5
                                           _INT1IE			.EQU                4
                                           _C1IE			.EQU                3
                                           _PWM2IE			.EQU                2
                                           _T2IE			.EQU                1
                                           _T1IE			.EQU                0
                                           
                                           ;  2DH  EIE2   Bits-------------------------------------
                                           T3IE			.EQU                7
                                           RCIE			.EQU                5
                                           TXIE			.EQU                4
                                           CCPIE			.EQU                2
                                           BCLIE			.EQU                1
                                           SSCIIE			.EQU                0
                                           _T3IE			.EQU                7
                                           _RCIE			.EQU                5
                                           _TXIE			.EQU                4
                                           _CCPIE			.EQU                2
                                           _BCLIE			.EQU                1
                                           _SSCIIE			.EQU                0
                                           
                                           ;  2EH  PCTL   Bits-------------------------------------
                                           SLVREN			.EQU                4
                                           IPEN			.EQU                3
                                           SWDTEN			.EQU                2
                                           POR			.EQU                1
                                           LVR			.EQU                0
                                           _SLVREN			.EQU                4
                                           _IPEN			.EQU                3
                                           _SWDTEN			.EQU                2
                                           _POR			.EQU                1
                                           _LVR			.EQU                0
                                           
                                           ;  2FH  OSCCTL   Bits-------------------------------------
                                           CLKOE			.EQU                7
                                           IRCS2			.EQU                6
                                           IRCS1			.EQU                5
                                           IRCS0			.EQU                4
                                           SCS1			.EQU                3
                                           SCS0			.EQU                2
                                           IESO			.EQU                1
                                           FSCM			.EQU                0
                                           _CLKOE			.EQU                7
                                           _IRCS2			.EQU                6
                                           _IRCS1			.EQU                5
                                           _IRCS0			.EQU                4
                                           _SCS1			.EQU                3
                                           _SCS0			.EQU                2
                                           _IESO			.EQU                1
                                           _FSCM			.EQU                0
                                           
                                           ;  31H  ANSEL   Bits-------------------------------------
                                           ANS7			.EQU                7
                                           ANS6			.EQU                6
                                           ANS5			.EQU                5
                                           ANS4			.EQU                4
                                           ANS3			.EQU                3
                                           ANS2			.EQU                2
                                           ANS1			.EQU                1
                                           ANS0			.EQU                0
                                           _ANS7			.EQU                7
                                           _ANS6			.EQU                6
                                           _ANS5			.EQU                5
                                           _ANS4			.EQU                4
                                           _ANS3			.EQU                3
                                           _ANS2			.EQU                2
                                           _ANS1			.EQU                1
                                           _ANS0			.EQU                0
                                           
                                           ;  35H  PUR0   Bits-------------------------------------
                                           PUR05			.EQU                5
                                           PUR04			.EQU                4
                                           PUR03			.EQU                3
                                           PUR02			.EQU                2
                                           PUR01			.EQU                1
                                           PUR00			.EQU                0
                                           _PUR05			.EQU                5
                                           _PUR04			.EQU                4
                                           _PUR03			.EQU                3
                                           _PUR02			.EQU                2
                                           _PUR01			.EQU                1
                                           _PUR00			.EQU                0
                                           
                                           ;  36H  IOCL   Bits-------------------------------------
                                           IOCL5			.EQU                5
                                           IOCL4			.EQU                4
                                           IOCL3			.EQU                3
                                           IOCL2			.EQU                2
                                           IOCL1			.EQU                1
                                           IOCL0			.EQU                0
                                           _IOCL5			.EQU                5
                                           _IOCL4			.EQU                4
                                           _IOCL3			.EQU                3
                                           _IOCL2			.EQU                2
                                           _IOCL1			.EQU                1
                                           _IOCL0			.EQU                0
                                           
                                           ;  3FH  ADCCTL1   Bits-------------------------------------
                                           ADCALEN			.EQU                7
                                           ADCS2			.EQU                6
                                           ADCS1			.EQU                5
                                           ADCS0			.EQU                4
                                           VCFG1			.EQU                3
                                           VCFG0			.EQU                2
                                           ADCIM			.EQU                0
                                           _ADCALEN		.EQU                7
                                           _ADCS2			.EQU                6
                                           _ADCS1			.EQU                5
                                           _ADCS0			.EQU                4
                                           _VCFG1			.EQU                3
                                           _VCFG0			.EQU                2
                                           _ADCIM			.EQU                0
                                           
                                           ;  45H  P0LR   Bits-------------------------------------
                                           P0LR5			.EQU                5
                                           P0LR4			.EQU                4
                                           P0LR3			.EQU                3
                                           P0LR2			.EQU                2
                                           P0LR1			.EQU                1
                                           P0LR0			.EQU                0
                                           _P0LR5			.EQU                5
                                           _P0LR4			.EQU                4
                                           _P0LR3			.EQU                3
                                           _P0LR2			.EQU                2
                                           _P0LR1			.EQU                1
                                           _P0LR0			.EQU                0
                                           
                                           ;  46H  P2LR   Bits-------------------------------------
                                           P2LR7			.EQU                7
                                           P2LR6			.EQU                6
                                           P2LR5			.EQU                5
                                           P2LR4			.EQU                4
                                           P2LR3			.EQU                3
                                           P2LR2			.EQU                2
                                           P2LR1			.EQU                1
                                           P2LR0			.EQU                0
                                           _P2LR7			.EQU                7
                                           _P2LR6			.EQU                6
                                           _P2LR5			.EQU                5
                                           _P2LR4			.EQU                4
                                           _P2LR3			.EQU                3
                                           _P2LR2			.EQU                2
                                           _P2LR1			.EQU                1
                                           _P2LR0			.EQU                0
                                           
                                           ;  47H  P1LR   Bits-------------------------------------
                                           P1LR7			.EQU                7
                                           P1LR6			.EQU                6
                                           P1LR5			.EQU                5
                                           P1LR4			.EQU                4
                                           P1LR3			.EQU                3
                                           P1LR2			.EQU                2
                                           P1LR1			.EQU                1
                                           P1LR0			.EQU                0
                                           _P1LR7			.EQU                7
                                           _P1LR6			.EQU                6
                                           _P1LR5			.EQU                5
                                           _P1LR4			.EQU                4
                                           _P1LR3			.EQU                3
                                           _P1LR2			.EQU                2
                                           _P1LR1			.EQU                1
                                           _P1LR0			.EQU                0
                                           
                                           ;  48H  P3LR   Bits-------------------------------------
                                           P3LR7			.EQU                7
                                           P3LR6			.EQU                6
                                           P3LR5			.EQU                5
                                           P3LR4			.EQU                4
                                           P3LR3			.EQU                3
                                           P3LR2			.EQU                2
                                           P3LR1			.EQU                1
                                           P3LR0			.EQU                0
                                           _P3LR7			.EQU                7
                                           _P3LR6			.EQU                6
                                           _P3LR5			.EQU                5
                                           _P3LR4			.EQU                4
                                           _P3LR3			.EQU                3
                                           _P3LR2			.EQU                2
                                           _P3LR1			.EQU                1
                                           _P3LR0			.EQU                0
                                           
                                           ;  49H  TR3   Bits-------------------------------------
                                           TR37			.EQU                7
                                           TR36			.EQU                6
                                           TR35			.EQU                5
                                           TR34			.EQU                4
                                           TR33			.EQU                3
                                           TR32			.EQU                2
                                           TR31			.EQU                1
                                           TR30			.EQU                0
                                           _TR37			.EQU                7
                                           _TR36			.EQU                6
                                           _TR35			.EQU                5
                                           _TR34			.EQU                4
                                           _TR33			.EQU                3
                                           _TR32			.EQU                2
                                           _TR31			.EQU                1
                                           _TR30			.EQU                0
                                           
                                           ;  4AH  EIE3   Bits-------------------------------------
                                           T4IE			.EQU                7
                                           OSCFAILIE		.EQU                5
                                           _T4IE			.EQU                7
                                           _OSCFAILIE		.EQU                5
                                           
                                           ;  4BH  EIF3   Bits-------------------------------------
                                           T4IF			.EQU                7
                                           OSCFAILIF		.EQU                5
                                           _T4IF			.EQU                7
                                           _OSCFAILIF		.EQU                5
                                           
                                           ;  4EH  T3CTL   Bits-------------------------------------
                                           T3EN			.EQU                7
                                           T3CKS1			.EQU                6
                                           T3CKS0			.EQU                5
                                           T3CS			.EQU                4
                                           _T3EN			.EQU                7
                                           _T3CKS1			.EQU                6
                                           _T3CKS0			.EQU                5
                                           _T3CS			.EQU                4
                                           
                                           ;  53H  T3CTL1   Bits-------------------------------------
                                           T3CLR			.EQU                5
                                           _T3CLR			.EQU                5
                                           
                                           ;  57H  PWM5CTL0   Bits-------------------------------------
                                           P5CH1MOD1		.EQU                7
                                           P5CH1MOD0		.EQU                6
                                           P5MOD3			.EQU                3
                                           P5MOD2			.EQU                2
                                           P5MOD1			.EQU                1
                                           P5MOD0			.EQU                0
                                           _P5CH1MOD1		.EQU                7
                                           _P5CH1MOD0		.EQU                6
                                           _P5MOD3			.EQU                3
                                           _P5MOD2			.EQU                2
                                           _P5MOD1			.EQU                1
                                           _P5MOD0			.EQU                0
                                           
                                           ;  5BH  PWM5CTL1   Bits-------------------------------------
                                           P5RSEN			.EQU                7
                                           P5DC6			.EQU                6
                                           P5DC5			.EQU                5
                                           P5DC4			.EQU                4
                                           P5DC3			.EQU                3
                                           P5DC2			.EQU                2
                                           P5DC1			.EQU                1
                                           P5DC0			.EQU                0
                                           _P5RSEN			.EQU                7
                                           _P5DC6			.EQU                6
                                           _P5DC5			.EQU                5
                                           _P5DC4			.EQU                4
                                           _P5DC3			.EQU                3
                                           _P5DC2			.EQU                2
                                           _P5DC1			.EQU                1
                                           _P5DC0			.EQU                0
                                           
                                           ;  5CH  P5ASCTL   Bits-------------------------------------
                                           P5ASE			.EQU                7
                                           P5ASS2			.EQU                6
                                           P5ASS1			.EQU                5
                                           P5ASS0			.EQU                4
                                           P5SSAC1			.EQU                3
                                           P5SSAC0			.EQU                2
                                           P5SSBD1			.EQU                1
                                           P5SSBD0			.EQU                0
                                           _P5ASE			.EQU                7
                                           _P5ASS2			.EQU                6
                                           _P5ASS1			.EQU                5
                                           _P5ASS0			.EQU                4
                                           _P5SSAC1		.EQU                3
                                           _P5SSAC0		.EQU                2
                                           _P5SSBD1		.EQU                1
                                           _P5SSBD0		.EQU                0
                                           
                                           ;  5DH  PSTRCTL   Bits-------------------------------------
                                           STRSYNC			.EQU                4
                                           STREND			.EQU                3
                                           STRENC			.EQU                2
                                           STRENB			.EQU                1
                                           STRENA			.EQU                0
                                           _STRSYNC		.EQU                4
                                           _STREND			.EQU                3
                                           _STRENC			.EQU                2
                                           _STRENB			.EQU                1
                                           _STRENA			.EQU                0
                                           
                                           ;  60H  PUR1   Bits-------------------------------------
                                           PUR17			.EQU                7
                                           PUR16			.EQU                6
                                           PUR15			.EQU                5
                                           PUR14			.EQU                4
                                           PUR13			.EQU                3
                                           PUR12			.EQU                2
                                           PUR11			.EQU                1
                                           PUR10			.EQU                0
                                           _PUR17			.EQU                7
                                           _PUR16			.EQU                6
                                           _PUR15			.EQU                5
                                           _PUR14			.EQU                4
                                           _PUR13			.EQU                3
                                           _PUR12			.EQU                2
                                           _PUR11			.EQU                1
                                           _PUR10			.EQU                0
                                           
                                           ;  61H  PUR2   Bits-------------------------------------
                                           PUR27			.EQU                7
                                           PUR26			.EQU                6
                                           PUR25			.EQU                5
                                           PUR24			.EQU                4
                                           PUR23			.EQU                3
                                           PUR22			.EQU                2
                                           PUR21			.EQU                1
                                           PUR20			.EQU                0
                                           _PUR27			.EQU                7
                                           _PUR26			.EQU                6
                                           _PUR25			.EQU                5
                                           _PUR24			.EQU                4
                                           _PUR23			.EQU                3
                                           _PUR22			.EQU                2
                                           _PUR21			.EQU                1
                                           _PUR20			.EQU                0
                                           
                                           ;  67H  INTEDGCTL   Bits-------------------------------------
                                           INT2SE			.EQU                7
                                           INT1SE			.EQU                6
                                           T1CLKEN			.EQU                0
                                           _INT2SE			.EQU                7
                                           _INT1SE			.EQU                6
                                           _T1CLKEN		.EQU                0
                                           
                                           ;  6BH  VBIASCTL   Bits-------------------------------------
                                           VBIASEN			.EQU                7
                                           VBSEL			.EQU                6
                                           ISEL1			.EQU                1
                                           ISEL0			.EQU                0
                                           _VBIASEN		.EQU                7
                                           _VBSEL			.EQU                6
                                           _ISEL1			.EQU                1
                                           _ISEL0			.EQU                0
                                           
                                           ;  6CH  VBIAS1EN   Bits-------------------------------------
                                           VBS17EN			.EQU                7
                                           VBS16EN			.EQU                6
                                           VBS15EN			.EQU                5
                                           VBS14EN			.EQU                4
                                           VBS13EN			.EQU                3
                                           VBS12EN			.EQU                2
                                           VBS11EN			.EQU                1
                                           VBS10EN			.EQU                0
                                           _VBS17EN		.EQU                7
                                           _VBS16EN		.EQU                6
                                           _VBS15EN		.EQU                5
                                           _VBS14EN		.EQU                4
                                           _VBS13EN		.EQU                3
                                           _VBS12EN		.EQU                2
                                           _VBS11EN		.EQU                1
                                           _VBS10EN		.EQU                0
                                           
                                           ;  6DH  VBIAS2EN   Bits-------------------------------------
                                           VBS27EN			.EQU                7
                                           VBS26EN			.EQU                6
                                           VBS25EN			.EQU                5
                                           VBS24EN			.EQU                4
                                           VBS23EN 		.EQU                3
                                           VBS22EN			.EQU                2
                                           VBS21EN			.EQU                1
                                           VBS20EN			.EQU                0
                                           _VBS27EN		.EQU                7
                                           _VBS26EN		.EQU                6
                                           _VBS25EN		.EQU                5
                                           _VBS24EN		.EQU                4
                                           _VBS23EN 		.EQU                3
                                           _VBS22EN		.EQU                2
                                           _VBS21EN		.EQU                1
                                           _VBS20EN		.EQU                0
                                           
                                           ;  10EH  PWM5OC   Bits-------------------------------------
                                           OCA			.EQU                1
                                           OCB			.EQU                0
                                           _OCA			.EQU                1
                                           _OCB			.EQU                0
                                           
                                           ;  10FH  T2CTL1   Bits-------------------------------------
                                           T2MOD1			.EQU                7
                                           T2MOD0			.EQU                6
                                           T2OFS1			.EQU                5
                                           T2OFS0			.EQU                4
                                           T2TRIGEN		.EQU                3
                                           T2DIR			.EQU                0
                                           _T2MOD1			.EQU                7
                                           _T2MOD0			.EQU                6
                                           _T2OFS1			.EQU                5
                                           _T2OFS0			.EQU                4
                                           _T2TRIGEN		.EQU                3
                                           _T2DIR			.EQU                0
                                           
                                           ;  112H  VDAC   Bits-------------------------------------
                                           VDAC3			.EQU                7
                                           VDAC2			.EQU                6
                                           VDAC1			.EQU                5
                                           VDAC0			.EQU                4
                                           _VDAC3			.EQU                7
                                           _VDAC2			.EQU                6
                                           _VDAC1			.EQU                5
                                           _VDAC0			.EQU                4
                                           
                                           ;  11CH  PWM5CTL2   Bits-------------------------------------
                                           PFUSES			.EQU                5
                                           UDEVT1			.EQU                2
                                           UDEVT0			.EQU                1
                                           UDEN			.EQU                0
                                           _PFUSES			.EQU                5
                                           _UDEVT1			.EQU                2
                                           _UDEVT0			.EQU                1
                                           _UDEN			.EQU                0
                                           
                                           ;  11DH  PWM5PC   Bits-------------------------------------
                                           PCA			.EQU                1
                                           PCB			.EQU                0
                                           _PCA			.EQU                1
                                           _PCB			.EQU                0
                                           
                                           ;  120H  RSCTL   Bits-------------------------------------
                                           SPEN			.EQU                7
                                           RX9			.EQU                6
                                           SRXEN			.EQU                5
                                           CRXEN			.EQU                4
                                           ADREN			.EQU                3
                                           FRER			.EQU                2
                                           OVFER			.EQU                1
                                           RX9D			.EQU                0
                                           _SPEN			.EQU                7
                                           _RX9			.EQU                6
                                           _SRXEN			.EQU                5
                                           _CRXEN			.EQU                4
                                           _ADREN			.EQU                3
                                           _FRER			.EQU                2
                                           _OVFER			.EQU                1
                                           _RX9D			.EQU                0
                                           
                                           ;  123H  BRCTL   Bits-------------------------------------
                                           ABRDOVF			.EQU                7
                                           RCIDLF			.EQU                6
                                           SCKPS			.EQU                5
                                           BRG16			.EQU                4
                                           WUEN			.EQU                1
                                           ABRDEN			.EQU                0
                                           _ABRDOVF		.EQU                7
                                           _RCIDLF			.EQU                6
                                           _SCKPS			.EQU                5
                                           _BRG16			.EQU                4
                                           _WUEN			.EQU                1
                                           _ABRDEN			.EQU                0
                                           
                                           ;  124H  TSCTL   Bits-------------------------------------
                                           CSRS			.EQU                7
                                           TX9			.EQU                6
                                           TXEN			.EQU                5
                                           SYNC			.EQU                4
                                           SENDB			.EQU                3
                                           HBRG			.EQU                2
                                           TXSRS			.EQU                1
                                           TX9D			.EQU                0
                                           _CSRS			.EQU                7
                                           _TX9			.EQU                6
                                           _TXEN			.EQU                5
                                           _SYNC			.EQU                4
                                           _SENDB			.EQU                3
                                           _HBRG			.EQU                2
                                           _TXSRS			.EQU                1
                                           _TX9D			.EQU                0
                                           
                                           ;  128H  SSCICTL0   Bits-------------------------------------
                                           SSCIWCFL		.EQU                7
                                           SSCIOV			.EQU                6
                                           SSCIEN			.EQU                5
                                           SSCICKP			.EQU                4
                                           SSCIMOD3		.EQU                3
                                           SSCIMOD2		.EQU                2
                                           SSCIMOD1		.EQU                1
                                           SSCIMOD0		.EQU                0
                                           _SSCIWCFL		.EQU                7
                                           _SSCIOV			.EQU                6
                                           _SSCIEN			.EQU                5
                                           _SSCICKP		.EQU                4
                                           _SSCIMOD3		.EQU                3
                                           _SSCIMOD2		.EQU                2
                                           _SSCIMOD1		.EQU                1
                                           _SSCIMOD0		.EQU                0
                                           
                                           ;  12AH  SSCICTL1   Bits-------------------------------------
                                           SSCICALLEN		.EQU                7
                                           SSCIACKSTA		.EQU                6
                                           SSCIACKDAT		.EQU                5
                                           SSCIACKEN		.EQU                4
                                           SSCIRCEN		.EQU                3
                                           STOPEN			.EQU                2
                                           RESTARTEN		.EQU                1
                                           STARTEN			.EQU                0
                                           _SSCICALLEN		.EQU                7
                                           _SSCIACKSTA		.EQU                6
                                           _SSCIACKDAT		.EQU                5
                                           _SSCIACKEN		.EQU                4
                                           _SSCIRCEN		.EQU                3
                                           _STOPEN			.EQU                2
                                           _RESTARTEN		.EQU                1
                                           _STARTEN		.EQU                0
                                           
                                           ;  12BH  SSCISTA   Bits-------------------------------------
                                           SAMPLE			.EQU                7
                                           CKEGE			.EQU                6
                                           SSCIDA			.EQU                5
                                           SSCISTOP		.EQU                4
                                           SSCISTART		.EQU                3
                                           SSCIRW			.EQU                2
                                           SSCIUA			.EQU                1
                                           SSCIBUF			.EQU                0
                                           _SAMPLE			.EQU                7
                                           _CKEGE			.EQU                6
                                           _SSCIDA			.EQU                5
                                           _SSCISTOP		.EQU                4
                                           _SSCISTART		.EQU                3
                                           _SSCIRW			.EQU                2
                                           _SSCIUA			.EQU                1
                                           _SSCIBUF		.EQU                0
                                           
                                           ;  12EH  SSCIMSK   Bits-------------------------------------
                                           SSCIMSK7		.EQU                7
                                           SSCIMSK6		.EQU                6
                                           SSCIMSK5		.EQU                5
                                           SSCIMSK4		.EQU                4
                                           SSCIMSK3		.EQU                3
                                           SSCIMSK2		.EQU                2
                                           SSCIMSK1		.EQU                1
                                           SSCIMSK0		.EQU                0
                                           _SSCIMSK7		.EQU                7
                                           _SSCIMSK6		.EQU                6
                                           _SSCIMSK5		.EQU                5
                                           _SSCIMSK4		.EQU                4
                                           _SSCIMSK3		.EQU                3
                                           _SSCIMSK2		.EQU                2
                                           _SSCIMSK1		.EQU                1
                                           _SSCIMSK0		.EQU                0
                                           
                                           ;  12FH  WDTPS   Bits-------------------------------------
                                           WDTPS3			.EQU                3
                                           WDTPS2			.EQU                2
                                           WDTPS1			.EQU                1
                                           WDTPS0			.EQU                0
                                           _WDTPS3			.EQU                3
                                           _WDTPS2			.EQU                2
                                           _WDTPS1			.EQU                1
                                           _WDTPS0			.EQU                0
                                           
                                           ;  134H  MULCTL   Bits-------------------------------------
                                           MULEN			.EQU                1
                                           MULIF			.EQU                0
                                           _MULEN			.EQU                1
                                           _MULIF			.EQU                0
                                           
                                           ;  139H  DIVCTL   Bits-------------------------------------
                                           DIVOEN			.EQU                1
                                           DIVEN			.EQU                0
                                           _DIVOEN			.EQU                1
                                           _DIVEN			.EQU                0
                                           
                                           ;  140H  LEDCTL   Bits-------------------------------------
                                           LEDEN			.EQU                7
                                           DIGEN2			.EQU                4
                                           DIGEN1			.EQU                3
                                           DIGEN0			.EQU                2
                                           PNS1			.EQU                1
                                           PNS0			.EQU                0
                                           _LEDEN			.EQU                7
                                           _DIGEN2			.EQU                4
                                           _DIGEN1			.EQU                3
                                           _DIGEN0			.EQU                2
                                           _PNS1			.EQU                1
                                           _PNS0			.EQU                0
                                           
                                           ;  141H  LEDPRE   Bits-------------------------------------
                                           LEDCKS13		.EQU                7
                                           LEDCKS12		.EQU                6
                                           LEDCKS11		.EQU                5
                                           LEDCKS10		.EQU                4
                                           LEDCKS03		.EQU                3
                                           LEDCKS02		.EQU                2
                                           LEDCKS01		.EQU                1
                                           LEDCKS00		.EQU                0
                                           _LEDCKS13		.EQU                7
                                           _LEDCKS12		.EQU                6
                                           _LEDCKS11		.EQU                5
                                           _LEDCKS10		.EQU                4
                                           _LEDCKS03		.EQU                3
                                           _LEDCKS02		.EQU                2
                                           _LEDCKS01		.EQU                1
                                           _LEDCKS00		.EQU                0
                                           
                                           ;  142H  LEDDATA0   Bits-------------------------------------
                                           DAT07			.EQU                7
                                           DAT06			.EQU                6
                                           DAT05			.EQU                5
                                           DAT04			.EQU                4
                                           DAT03			.EQU                3
                                           DAT02			.EQU                2
                                           DAT01			.EQU                1
                                           DAT00			.EQU                0
                                           _DAT07			.EQU                7
                                           _DAT06			.EQU                6
                                           _DAT05			.EQU                5
                                           _DAT04			.EQU                4
                                           _DAT03			.EQU                3
                                           _DAT02			.EQU                2
                                           _DAT01			.EQU                1
                                           _DAT00			.EQU                0
                                           
                                           ;  143H  LEDDATA1   Bits-------------------------------------
                                           DAT17			.EQU                7
                                           DAT16			.EQU                6
                                           DAT15			.EQU                5
                                           DAT14			.EQU                4
                                           DAT13			.EQU                3
                                           DAT12			.EQU                2
                                           DAT11			.EQU                1
                                           DAT10			.EQU                0
                                           _DAT17			.EQU                7
                                           _DAT16			.EQU                6
                                           _DAT15			.EQU                5
                                           _DAT14			.EQU                4
                                           _DAT13			.EQU                3
                                           _DAT12			.EQU                2
                                           _DAT11			.EQU                1
                                           _DAT10			.EQU                0
                                           
                                           ;  144H  LEDDATA2   Bits-------------------------------------
                                           DAT27			.EQU                7
                                           DAT26			.EQU                6
                                           DAT25			.EQU                5
                                           DAT24			.EQU                4
                                           DAT23			.EQU                3
                                           DAT22			.EQU                2
                                           DAT21			.EQU                1
                                           DAT20			.EQU                0
                                           _DAT27			.EQU                7
                                           _DAT26			.EQU                6
                                           _DAT25			.EQU                5
                                           _DAT24			.EQU                4
                                           _DAT23			.EQU                3
                                           _DAT22			.EQU                2
                                           _DAT21			.EQU                1
                                           _DAT20			.EQU                0
                                           
                                           ;  145H  LEDDATA3   Bits-------------------------------------
                                           DAT37			.EQU                7
                                           DAT36			.EQU                6
                                           DAT35			.EQU                5
                                           DAT34			.EQU                4
                                           DAT33			.EQU                3
                                           DAT32			.EQU                2
                                           DAT31			.EQU                1
                                           DAT30			.EQU                0
                                           _DAT37			.EQU                7
                                           _DAT36			.EQU                6
                                           _DAT35			.EQU                5
                                           _DAT34			.EQU                4
                                           _DAT33			.EQU                3
                                           _DAT32			.EQU                2
                                           _DAT31			.EQU                1
                                           _DAT30			.EQU                0
                                           
                                           ;  146H  LEDDATA4   Bits-------------------------------------
                                           DAT47			.EQU                7
                                           DAT46			.EQU                6
                                           DAT45			.EQU                5
                                           DAT44			.EQU                4
                                           DAT43			.EQU                3
                                           DAT42			.EQU                2
                                           DAT41			.EQU                1
                                           DAT40			.EQU                0
                                           _DAT47			.EQU                7
                                           _DAT46			.EQU                6
                                           _DAT45			.EQU                5
                                           _DAT44			.EQU                4
                                           _DAT43			.EQU                3
                                           _DAT42			.EQU                2
                                           _DAT41			.EQU                1
                                           _DAT40			.EQU                0
                                           
                                           ;  147H  LEDDATA5   Bits-------------------------------------
                                           DAT57			.EQU                7
                                           DAT56			.EQU                6
                                           DAT55			.EQU                5
                                           DAT54			.EQU                4
                                           DAT53			.EQU                3
                                           DAT52			.EQU                2
                                           DAT51			.EQU                1
                                           DAT50			.EQU                0
                                           _DAT57			.EQU                7
                                           _DAT56			.EQU                6
                                           _DAT55			.EQU                5
                                           _DAT54			.EQU                4
                                           _DAT53			.EQU                3
                                           _DAT52			.EQU                2
                                           _DAT51			.EQU                1
                                           _DAT50			.EQU                0
                                           
                                           ;  148H  LEDDATA6   Bits-------------------------------------
                                           DAT67			.EQU                7
                                           DAT66			.EQU                6
                                           DAT65			.EQU                5
                                           DAT64			.EQU                4
                                           DAT63			.EQU                3
                                           DAT62			.EQU                2
                                           DAT61			.EQU                1
                                           DAT60			.EQU                0
                                           _DAT67			.EQU                7
                                           _DAT66			.EQU                6
                                           _DAT65			.EQU                5
                                           _DAT64			.EQU                4
                                           _DAT63			.EQU                3
                                           _DAT62			.EQU                2
                                           _DAT61			.EQU                1
                                           _DAT60			.EQU                0
                                           
                                           ;  149H  LEDDATA7   Bits-------------------------------------
                                           DAT77			.EQU                7
                                           DAT76			.EQU                6
                                           DAT75			.EQU                5
                                           DAT74			.EQU                4
                                           DAT73			.EQU                3
                                           DAT72			.EQU                2
                                           DAT71			.EQU                1
                                           DAT70			.EQU                0
                                           _DAT77			.EQU                7
                                           _DAT76			.EQU                6
                                           _DAT75			.EQU                5
                                           _DAT74			.EQU                4
                                           _DAT73			.EQU                3
                                           _DAT72			.EQU                2
                                           _DAT71			.EQU                1
                                           _DAT70			.EQU                0
                                           
                                           ;  14AH  C1FILTCTL   Bits-------------------------------------
                                           INV1			.EQU                7
                                           WEN1			.EQU                6
                                           FEN1			.EQU                5
                                           F1CNT2			.EQU                2
                                           F1CNT1			.EQU                1
                                           F1CNT0			.EQU                0
                                           _INV1			.EQU                7
                                           _WEN1			.EQU                6
                                           _FEN1			.EQU                5
                                           _F1CNT2			.EQU                2
                                           _F1CNT1			.EQU                1
                                           _F1CNT0			.EQU                0
                                           
                                           ;  14BH  C1FILTPRE   Bits-------------------------------------
                                           FP17			.EQU                7
                                           FP16			.EQU                6
                                           FP15			.EQU                5
                                           FP14			.EQU                4
                                           FP13			.EQU                3
                                           FP12			.EQU                2
                                           FP11			.EQU                1
                                           FP10			.EQU                0
                                           _FP17			.EQU                7
                                           _FP16			.EQU                6
                                           _FP15			.EQU                5
                                           _FP14			.EQU                4
                                           _FP13			.EQU                3
                                           _FP12			.EQU                2
                                           _FP11			.EQU                1
                                           _FP10			.EQU                0
                                           
                                           ;  150H  LEDOMS1   Bits-------------------------------------
                                           LEDOM17			.EQU                7
                                           LEDOM16			.EQU                6
                                           LEDOM15			.EQU                5
                                           LEDOM14			.EQU                4
                                           LEDOM13			.EQU                3
                                           LEDOM12			.EQU                2
                                           LEDOM11			.EQU                1
                                           LEDOM10			.EQU                0
                                           _LEDOM17		.EQU                7
                                           _LEDOM16		.EQU                6
                                           _LEDOM15		.EQU                5
                                           _LEDOM14		.EQU                4
                                           _LEDOM13		.EQU                3
                                           _LEDOM12		.EQU                2
                                           _LEDOM11		.EQU                1
                                           _LEDOM10		.EQU                0
                                           
                                           ;  152H  CCPCTL   Bits-------------------------------------
                                           CCMOD3			.EQU                3
                                           CCMOD2			.EQU                2
                                           CCMOD1			.EQU                1
                                           CCMOD0			.EQU                0
                                           _CCMOD3			.EQU                3
                                           _CCMOD2			.EQU                2
                                           _CCMOD1			.EQU                1
                                           _CCMOD0			.EQU                0
                                           
                                           ;  155H  LEDODS0   Bits-------------------------------------
                                           LEDOD07			.EQU                7
                                           LEDOD06			.EQU                6
                                           LEDOD05			.EQU                5
                                           LEDOD04			.EQU                4
                                           LEDOD03			.EQU                3
                                           LEDOD02			.EQU                2
                                           LEDOD01			.EQU                1
                                           LEDOD00			.EQU                0
                                           _LEDOD07		.EQU                7
                                           _LEDOD06		.EQU                6
                                           _LEDOD05		.EQU                5
                                           _LEDOD04		.EQU                4
                                           _LEDOD03		.EQU                3
                                           _LEDOD02		.EQU                2
                                           _LEDOD01		.EQU                1
                                           _LEDOD00		.EQU                0
                                           
                                           ;  157H  LEDOMS0   Bits-------------------------------------
                                           LEDOM07			.EQU                7
                                           LEDOM06			.EQU                6
                                           LEDOM05			.EQU                5
                                           LEDOM04			.EQU                4
                                           LEDOM03			.EQU                3
                                           LEDOM02			.EQU                2
                                           LEDOM01			.EQU                1
                                           LEDOM00			.EQU                0
                                           _LEDOM07		.EQU                7
                                           _LEDOM06		.EQU                6
                                           _LEDOM05		.EQU                5
                                           _LEDOM04		.EQU                4
                                           _LEDOM03		.EQU                3
                                           _LEDOM02		.EQU                2
                                           _LEDOM01		.EQU                1
                                           _LEDOM00		.EQU                0
                                           
                                           ;  158H  LEDODS1   Bits-------------------------------------
                                           LEDOD17			.EQU                7
                                           LEDOD16			.EQU                6
                                           LEDOD15			.EQU                5
                                           LEDOD14			.EQU                4
                                           LEDOD13			.EQU                3
                                           LEDOD12			.EQU                2
                                           LEDOD11			.EQU                1
                                           LEDOD10			.EQU                0
                                           _LEDOD17		.EQU                7
                                           _LEDOD16		.EQU                6
                                           _LEDOD15		.EQU                5
                                           _LEDOD14		.EQU                4
                                           _LEDOD13		.EQU                3
                                           _LEDOD12		.EQU                2
                                           _LEDOD11		.EQU                1
                                           _LEDOD10		.EQU                0
                                           
                                           ;  15CH  LEDLUM   Bits-------------------------------------
                                           LEDBR			.EQU                7
                                           FRAMEF			.EQU                3
                                           LUM2			.EQU                2
                                           LUM1			.EQU                1
                                           LUM0			.EQU                0
                                           _LEDBR			.EQU                7
                                           _FRAMEF			.EQU                3
                                           _LUM2			.EQU                2
                                           _LUM1			.EQU                1
                                           _LUM0			.EQU                0
                                           
                                           ;  15DH  PWM5FC   Bits-------------------------------------
                                           FCA			.EQU                1
                                           FCB			.EQU                0
                                           _FCA			.EQU                1
                                           _FCB			.EQU                0
                                           
                                           ;  164H  T4CTL   Bits-------------------------------------
                                           T4REN			.EQU                7
                                           HSPEN			.EQU                6
                                           T4CKS1			.EQU                5
                                           T4CKS0			.EQU                4
                                           LSPEN			.EQU                3
                                           T4CS1			.EQU                2
                                           T4CS0			.EQU                1
                                           T4ON			.EQU                0
                                           _T4REN			.EQU                7
                                           _HSPEN			.EQU                6
                                           _T4CKS1			.EQU                5
                                           _T4CKS0			.EQU                4
                                           _LSPEN			.EQU                3
                                           _T4CS1			.EQU                2
                                           _T4CS0			.EQU                1
                                           _T4ON			.EQU                0
                                           ;************************************************************
                                           ;       Header file for the KungFu8 END
                                           ;       KF8A100EON
                                           ;       Microcontroller
                                           ;
                                           ;       Copyright 2012-2020 ChipON, All rights reserved
                                           ;************************************************************
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_FLASH_READ_ONE
                                           	.extern	_FLASH_READ_FUN
                                           	.extern	_FLASH_WRITE_ONE
                                           	.extern	_FLASH_WRITE_FUN
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_PCH_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_T3CTL_bits
                                           	.extern	_T3CTL1_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWM5PC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_CCPCTL_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_FLASH_BUFFER
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_T3CTL
                                           	.extern	_T3L
                                           	.extern	_PP5L
                                           	.extern	_T3CTL1
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_T3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWM5PC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIADD
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_CCRL
                                           	.extern	_CCPCTL
                                           	.extern	_CCRH
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	__hmulint
                                           	.extern	_startup
                                           	.extern	__gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Sys_Init
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           	.global	_test
                                           
                                           	.global I0R1
                                           	.global I0R7
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1R7
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata
                                           I0R1		.res 1
                                           I0R7		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1R7		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1000	.res	1
                                           UDL_main_1	.udata
                                           r0x1001	.res	1
                                           UDL_main_2	.udata
                                           r0x1002	.res	1
                                           UDL_main_3	.udata
                                           r0x1004	.res	1
                                           UDL_main_4	.udata
                                           r0x1003	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           
                                           ID_main_0	.code	0x1E58
                                           _test
001e58   b034     RRET	R0, #0x34           	RRET R0, #0x34
001e59   b012     RRET	R0, #0x12           	RRET R0, #0x12
                                           
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e010     MOVP	#0x10               	PAGESEL	init_imp
000002   ce5a     JMP	#0xe5a               	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
001e5a   e010     MOVP	#0x10               	PAGESEL	_startup
001e5b   d123     CALL	#0x123              	CALL	_startup
001e5c   e010     MOVP	#0x10               	PAGESEL	__gsinit_startup
001e5d   dfec     CALL	#0xfec              	CALL	__gsinit_startup
001e5e   e010     MOVP	#0x10               	PAGESEL	_main
001e5f   c000     JMP	#0                   	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           _00025_DS_
                                           ;	.line	98; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00027_DS_
                                           ;	.line	105; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _Sys_Init
                                           ;   __hmulint
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_ONE
                                           ;   __hmulint
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_ONE
                                           ;   _Sys_Init
                                           ;   __hmulint
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_ONE
                                           ;   __hmulint
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_ONE
                                           ;8 compiler assigned registers:
                                           ;   r0x1000
                                           ;   r0x1001
                                           ;   r0x1002
                                           ;   STK02
                                           ;   STK01
                                           ;   STK00
                                           ;   r0x1003
                                           ;   r0x1004
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	::->op : CALL
                                           ;	.line	51; "../main.c"	Sys_Init();
001000   e010     MOVP	#0x10               	PAGESEL	_Sys_Init
001001   dfe0     CALL	#0xfe0              	CALL	_Sys_Init
001002   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : =
                                           ;	.line	54; "../main.c"	for (i = 0; i < FLASH_BUFFER_MAX; i++)
001003   e100     MOVB	#0x00               	BANKSEL	r0x1000
001004   0384     CLR	0x84                 	CLR	r0x1000
                                           	BANKSEL	r0x1001
001005   0383     CLR	0x83                 	CLR	r0x1001
                                           ;	::->op : =
                                           	BANKSEL	r0x1002
001006   0382     CLR	0x82                 	CLR	r0x1002
                                           ;	::->op : LABEL
                                           ;	::->op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00006_DS_
001007   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	r0x1002
001008   3882     SUB	R0, 0x82             	SUB	R0, r0x1002
                                           ;comparing bytes at offset 0
001009   7003     JNB	0x3, 0               	JNB	PSW, 0
00100a   c029     JMP	#0x29                	JMP	_00009_DS_
                                           ;	::->op : *
                                           ;	.line	56; "../main.c"	FLASH_BUFFER[i] = temp;
00100b   9802     MOV	R0, #0x2             	MOV	R0,# 0x02
                                           	BANKSEL	STK02
00100c   51a4     MOV	0xa4, R0             	MOV	STK02, R0
00100d   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	STK01
00100e   51a5     MOV	0xa5, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x1002
00100f   0e82     MOVZ	R0, 0x82            	MOVZ	R0, r0x1002
                                           	BANKSEL	STK00
001010   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001011   9800     MOV	R0, #0               	MOV	R0,# 0x00
001012   e010     MOVP	#0x10               	PAGESEL	__hmulint
001013   d164     CALL	#0x164              	CALL	__hmulint
001014   e010     MOVP	#0x10               	PAGESEL	$
001015   e100     MOVB	#0x00               	BANKSEL	r0x1003
001016   5180     MOV	0x80, R0             	MOV	r0x1003, R0
                                           	BANKSEL	STK00
001017   50a6     MOV	R0, 0xa6             	MOV	R0, STK00
                                           	BANKSEL	r0x1004
001018   5181     MOV	0x81, R0             	MOV	r0x1004, R0
                                           ;	::->op : +
001019   98a7     MOV	R0, #0xa7            	MOV	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x1004
00101a   2181     ADD	0x81, R0             	ADD	r0x1004, R0
                                           ;	::->op :*  =
                                           	BANKSEL	r0x1000
00101b   0e84     MOVZ	R0, 0x84            	MOVZ	R0, r0x1000
                                           	BANKSEL	r0x1004
00101c   5281     MOV	R1, 0x81             	MOV	R1, r0x1004
                                           	BANKSEL	_FLASH_BUFFER
00101d   f741     ST	[R1], R0              	ST	[R1], R0
00101e   ff11     INC	R1                   	INC	R1
                                           	BANKSEL	r0x1001
00101f   0e83     MOVZ	R0, 0x83            	MOVZ	R0, r0x1001
                                           	BANKSEL	_FLASH_BUFFER
001020   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : +
                                           ;	.line	57; "../main.c"	temp += 0x1111;
001021   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
                                           	BANKSEL	r0x1000
001022   2184     ADD	0x84, R0             	ADD	r0x1000, R0
001023   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
001024   7003     JNB	0x3, 0               	JNB	PSW, 0
001025   9812     MOV	R0, #0x12            	MOV	R0,# 0x12
                                           	BANKSEL	r0x1001
001026   2183     ADD	0x83, R0             	ADD	r0x1001, R0
                                           ;	::->op : +
                                           ;	.line	54; "../main.c"	for (i = 0; i < FLASH_BUFFER_MAX; i++)
                                           	BANKSEL	r0x1002
001027   0b82     INC	0x82                 	INC	r0x1002
                                           ;	::->op : GOTO
001028   c007     JMP	#0x7                 	JMP	_00006_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           _00009_DS_
                                           ;	.line	61; "../main.c"	FLASH_WRITE_FUN(0x1E60,FLASH_BUFFER_MAX);
001029   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
00102a   51a5     MOV	0xa5, R0             	MOV	STK01, R0
00102b   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
                                           	BANKSEL	STK00
00102c   51a6     MOV	0xa6, R0             	MOV	STK00, R0
00102d   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
00102e   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_FUN
00102f   d088     CALL	#0x88               	CALL	_FLASH_WRITE_FUN
001030   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	62; "../main.c"	FLASH_WRITE_FUN(0x1E80,FLASH_BUFFER_MAX);
001031   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
001032   e100     MOVB	#0x00               	BANKSEL	STK01
001033   51a5     MOV	0xa5, R0             	MOV	STK01, R0
001034   9880     MOV	R0, #0x80            	MOV	R0,# 0x80
                                           	BANKSEL	STK00
001035   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001036   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001037   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_FUN
001038   d088     CALL	#0x88               	CALL	_FLASH_WRITE_FUN
001039   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	65; "../main.c"	temp=FLASH_READ_ONE(0x1E71);
00103a   9871     MOV	R0, #0x71            	MOV	R0,# 0x71
00103b   e100     MOVB	#0x00               	BANKSEL	STK00
00103c   51a6     MOV	0xa6, R0             	MOV	STK00, R0
00103d   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
00103e   e010     MOVP	#0x10               	PAGESEL	_FLASH_READ_ONE
00103f   d144     CALL	#0x144              	CALL	_FLASH_READ_ONE
001040   e010     MOVP	#0x10               	PAGESEL	$
001041   e100     MOVB	#0x00               	BANKSEL	r0x1001
001042   5183     MOV	0x83, R0             	MOV	r0x1001, R0
                                           	BANKSEL	STK00
001043   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1000
001044   5184     MOV	0x84, R0             	MOV	r0x1000, R0
                                           ;	::->op : =
                                           ;	.line	67; "../main.c"	for (i = 0; i < 16; i++)
                                           	BANKSEL	r0x1002
001045   0382     CLR	0x82                 	CLR	r0x1002
                                           ;	::->op : LABEL
                                           ;	::->op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00010_DS_
001046   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	r0x1002
001047   3882     SUB	R0, 0x82             	SUB	R0, r0x1002
                                           ;comparing bytes at offset 0
001048   7003     JNB	0x3, 0               	JNB	PSW, 0
001049   c062     JMP	#0x62                	JMP	_00013_DS_
                                           ;	::->op : *
                                           ;	.line	69; "../main.c"	FLASH_BUFFER[i] = 0x0000;
00104a   9802     MOV	R0, #0x2             	MOV	R0,# 0x02
                                           	BANKSEL	STK02
00104b   51a4     MOV	0xa4, R0             	MOV	STK02, R0
00104c   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	STK01
00104d   51a5     MOV	0xa5, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x1002
00104e   0e82     MOVZ	R0, 0x82            	MOVZ	R0, r0x1002
                                           	BANKSEL	STK00
00104f   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001050   9800     MOV	R0, #0               	MOV	R0,# 0x00
001051   e010     MOVP	#0x10               	PAGESEL	__hmulint
001052   d164     CALL	#0x164              	CALL	__hmulint
001053   e010     MOVP	#0x10               	PAGESEL	$
001054   e100     MOVB	#0x00               	BANKSEL	r0x1003
001055   5180     MOV	0x80, R0             	MOV	r0x1003, R0
                                           	BANKSEL	STK00
001056   50a6     MOV	R0, 0xa6             	MOV	R0, STK00
                                           	BANKSEL	r0x1004
001057   5181     MOV	0x81, R0             	MOV	r0x1004, R0
                                           ;	::->op : +
001058   98a7     MOV	R0, #0xa7            	MOV	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x1004
001059   2181     ADD	0x81, R0             	ADD	r0x1004, R0
                                           ;	::->op :*  =
00105a   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1004
00105b   5281     MOV	R1, 0x81             	MOV	R1, r0x1004
                                           	BANKSEL	_FLASH_BUFFER
00105c   f741     ST	[R1], R0              	ST	[R1], R0
00105d   ff11     INC	R1                   	INC	R1
00105e   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	_FLASH_BUFFER
00105f   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	::->op : +
                                           ;	.line	67; "../main.c"	for (i = 0; i < 16; i++)
                                           	BANKSEL	r0x1002
001060   0b82     INC	0x82                 	INC	r0x1002
                                           ;	::->op : GOTO
001061   c046     JMP	#0x46                	JMP	_00010_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           _00013_DS_
                                           ;	.line	72; "../main.c"	FLASH_WRITE_FUN(0x1EA0,16);
001062   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
001063   51a5     MOV	0xa5, R0             	MOV	STK01, R0
001064   98a0     MOV	R0, #0xa0            	MOV	R0,# 0xa0
                                           	BANKSEL	STK00
001065   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001066   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001067   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_FUN
001068   d088     CALL	#0x88               	CALL	_FLASH_WRITE_FUN
001069   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op :*  =
                                           ;	.line	74; "../main.c"	FLASH_BUFFER[5]=temp;
00106a   e100     MOVB	#0x00               	BANKSEL	r0x1000
00106b   0e84     MOVZ	R0, 0x84            	MOVZ	R0, r0x1000
                                           	BANKSEL	_FLASH_BUFFER
00106c   51b1     MOV	0xb1, R0             	MOV	 (_FLASH_BUFFER + 10), R0
                                           	BANKSEL	r0x1001
00106d   0e83     MOVZ	R0, 0x83            	MOVZ	R0, r0x1001
                                           	BANKSEL	_FLASH_BUFFER
00106e   51b2     MOV	0xb2, R0             	MOV	 (_FLASH_BUFFER + 11), R0
                                           ;	::->op :*  =
                                           ;	.line	75; "../main.c"	FLASH_BUFFER[6]=0xFF33; //ÑéÖ¤ ÓÃ 0x1FB6
00106f   9833     MOV	R0, #0x33            	MOV	R0,# 0x33
                                           	BANKSEL	_FLASH_BUFFER
001070   51b3     MOV	0xb3, R0             	MOV	 (_FLASH_BUFFER + 12), R0
001071   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	_FLASH_BUFFER
001072   51b4     MOV	0xb4, R0             	MOV	 (_FLASH_BUFFER + 13), R0
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	77; "../main.c"	FLASH_WRITE_FUN(0x1EB0,16);
001073   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
001074   51a5     MOV	0xa5, R0             	MOV	STK01, R0
001075   98b0     MOV	R0, #0xb0            	MOV	R0,# 0xb0
                                           	BANKSEL	STK00
001076   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001077   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001078   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_FUN
001079   d088     CALL	#0x88               	CALL	_FLASH_WRITE_FUN
00107a   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : SEND
                                           ;	::->op : SEND
                                           ;	::->op : CALL
                                           ;	.line	82; "../main.c"	FLASH_WRITE_ONE(0x1E69,0x55AA);
00107b   98aa     MOV	R0, #0xaa            	MOV	R0,# 0xaa
00107c   e100     MOVB	#0x00               	BANKSEL	STK02
00107d   51a4     MOV	0xa4, R0             	MOV	STK02, R0
00107e   9855     MOV	R0, #0x55            	MOV	R0,# 0x55
                                           	BANKSEL	STK01
00107f   51a5     MOV	0xa5, R0             	MOV	STK01, R0
001080   9869     MOV	R0, #0x69            	MOV	R0,# 0x69
                                           	BANKSEL	STK00
001081   51a6     MOV	0xa6, R0             	MOV	STK00, R0
001082   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001083   e010     MOVP	#0x10               	PAGESEL	_FLASH_WRITE_ONE
001084   d0c3     CALL	#0xc3               	CALL	_FLASH_WRITE_ONE
001085   e010     MOVP	#0x10               	PAGESEL	$
                                           ;	::->op : LABEL
                                           ;	::->op : GOTO
                                           _00004_DS_
                                           ;	.line	89; "../main.c"	while(1)
001086   c086     JMP	#0x86                	JMP	_00004_DS_
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
001087   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._Sys_Init	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	::->op : LABEL
                                           ;	::->op : FUNCTION
                                           _Sys_Init	;Function start
                                           ; 2 exit points
                                           ;	::->op : =
                                           ;	.line	34; "../main.c"	OSCCTL = 0x70;		//Ê±ÖÓÅäÖÃÎªÄÚ²¿16M
001fe0   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
001fe1   e100     MOVB	#0x00               	BANKSEL	_OSCCTL
001fe2   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	::->op : =
                                           ;	.line	35; "../main.c"	TR0=0;
                                           	BANKSEL	_TR0
001fe3   0325     CLR	0x25                 	CLR	_TR0
                                           ;	::->op : =
                                           ;	.line	36; "../main.c"	TR1=0;
                                           	BANKSEL	_TR1
001fe4   0327     CLR	0x27                 	CLR	_TR1
                                           ;	::->op : =
                                           ;	.line	37; "../main.c"	TR2=0;
                                           	BANKSEL	_TR2
001fe5   0326     CLR	0x26                 	CLR	_TR2
                                           ;	::->op : =
                                           ;	.line	38; "../main.c"	TR3=0;
                                           	BANKSEL	_TR3
001fe6   0349     CLR	0x49                 	CLR	_TR3
                                           ;	::->op : =
                                           ;	.line	39; "../main.c"	P0=0;
                                           	BANKSEL	_P0
001fe7   0305     CLR	0x5                  	CLR	_P0
                                           ;	::->op : =
                                           ;	.line	40; "../main.c"	P1=0;
                                           	BANKSEL	_P1
001fe8   0307     CLR	0x7                  	CLR	_P1
                                           ;	::->op : =
                                           ;	.line	41; "../main.c"	P2=0;
                                           	BANKSEL	_P2
001fe9   0306     CLR	0x6                  	CLR	_P2
                                           ;	::->op : =
                                           ;	.line	42; "../main.c"	P3=0;
                                           	BANKSEL	_P3
001fea   0308     CLR	0x8                  	CLR	_P3
                                           ;	::->op : LABEL
                                           ;	::->op : ENDFUNCTION
001feb   0008     CRET                     	CRET	
                                           ; exit point of _Sys_Init
                                           
                                           
                                           ;	code size estimation:
                                           ;	  141+   64 =   205 instructions (  538 byte)
                                           
                                           
                                           	.end
                                           .config
002007   1dd4     XOR	0xd4, R2            
002008   ffff     NOPZ                    
                                           func.__gsinit_startup
001fec   e010     MOVP	#0x10              
001fed   d17e     CALL	#0x17e             
001fee   e010     MOVP	#0x10              
001fef   0008     CRET                    
                                           func.__hmulint
001164   e101     MOVB	#0x01              
001165   0334     CLR	0x34                
001166   5130     MOV	0x30, R0            
001167   e100     MOVB	#0x00              
001168   50a6     MOV	R0, 0xa6            
001169   e101     MOVB	#0x01              
00116a   5131     MOV	0x31, R0            
00116b   e100     MOVB	#0x00              
00116c   50a5     MOV	R0, 0xa5            
00116d   e101     MOVB	#0x01              
00116e   5132     MOV	0x32, R0            
00116f   e100     MOVB	#0x00              
001170   50a4     MOV	R0, 0xa4            
001171   e101     MOVB	#0x01              
001172   5133     MOV	0x33, R0            
001173   6934     SET	0x34, 1             
001174   7834     JB	0x34, 0              
001175   c174     JMP	#0x174              
001176   0334     CLR	0x34                
001177   5038     MOV	R0, 0x38            
001178   e100     MOVB	#0x00              
001179   51a6     MOV	0xa6, R0            
00117a   e101     MOVB	#0x01              
00117b   5037     MOV	R0, 0x37            
00117c   0008     CRET                    
00117d   0008     CRET                    
                                           _sartup_A100EON
001123   e01f     MOVP	#0x1F              
001124   e100     MOVB	#0x00              
001125   dfff     CALL	#0xfff             
001126   5130     MOV	0x30, R0            
001127   ffff     NOPZ                    
001128   ffff     NOPZ                    
001129   dffe     CALL	#0xffe             
00112a   5137     MOV	0x37, R0            
00112b   ffff     NOPZ                    
00112c   ffff     NOPZ                    
00112d   dffd     CALL	#0xffd             
00112e   514c     MOV	0x4c, R0            
00112f   ffff     NOPZ                    
001130   ffff     NOPZ                    
001131   dffc     CALL	#0xffc             
001132   514d     MOV	0x4d, R0            
001133   ffff     NOPZ                    
001134   ffff     NOPZ                    
001135   dffb     CALL	#0xffb             
001136   512a     MOV	0x2a, R0            
001137   ffff     NOPZ                    
001138   e101     MOVB	#0x01              
001139   dffa     CALL	#0xffa             
00113a   5159     MOV	0x59, R0            
00113b   ffff     NOPZ                    
00113c   dff9     CALL	#0xff9             
00113d   515a     MOV	0x5a, R0            
00113e   ffff     NOPZ                    
00113f   dff8     CALL	#0xff8             
001140   5165     MOV	0x65, R0            
001141   ffff     NOPZ                    
001142   ffff     NOPZ                    
001143   0008     CRET                    
                                           .cinit
00117e   e100     MOVB	#0x00              
00117f   9880     MOV	R0, #0x80           
001180   9947     MOV	R1, #0x47           
001181   e010     MOVP	#0x10              
001182   d184     CALL	#0x184             
001183   0008     CRET                    
001184   020a     CLR	R2                  
001185   f750     ST	[R0], R2             
001186   ff10     INC	R0                  
001187   ff59     DECJZ	R1                
001188   c185     JMP	#0x185              
001189   0008     CRET                    
