gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 5-20-2016  14:52:14
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 09:33:53 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8V216
                                           	.radix dec
                                           	.include "KF8V216.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8V216 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           CM1CTL            .EQU                0x19
                                           AMPCTL            .EQU                0x1B
                                           VRECAL1           .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           VRECAL2           .EQU                0x2A
                                           VRECTL1           .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP4H              .EQU                0x42
                                           PWM4L1            .EQU                0x43
                                           PWM4H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           PP4L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM4L0            .EQU                0x55
                                           PWM4H0            .EQU                0x56
                                           PWM4CTL0          .EQU                0x57
                                           PWM4CTL1          .EQU                0x5B
                                           P4ASCTL           .EQU                0x5C
                                           PATRCTL           .EQU                0x5D
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL Bits-----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           PWM2ON             .EQU                1
                                           PWM1ON             .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _PWM2ON            .EQU                1
                                           _PWM1ON            .EQU                0
                                           
                                           ;CM1CTL Bits----------------------------------
                                           C1OE               .EQU                7
                                           C1INS              .EQU                6
                                           C1P                .EQU                2
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1OE              .EQU                7
                                           _C1INS             .EQU                6
                                           _C1P               .EQU                2
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;AMPCTL Bits----------------------------------
                                           CALIRD             .EQU                7
                                           CALIEN             .EQU                1
                                           AMPON              .EQU                0
                                           _CALIRD            .EQU                7
                                           _CALIEN            .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;VRECTL1 Bits---------------------------------
                                           VREOE              .EQU                3
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VREOE             .EQU                3
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR Bits-------------------------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCCALIEN          .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM1             .EQU                1
                                           ADCIM0             .EQU                0
                                           _ADCCALIEN         .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM1            .EQU                1
                                           _ADCIM0            .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR2              .EQU                2
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR2             .EQU                2
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;PWM4CTL0 Bits--------------------------------
                                           P4M1               .EQU                7
                                           P4M0               .EQU                6
                                           PWM4M3             .EQU                3
                                           PWM4M2             .EQU                2
                                           PWM4M1             .EQU                1
                                           PWM4M0             .EQU                0
                                           _P4M1              .EQU                7
                                           _P4M0              .EQU                6
                                           _PWM4M3            .EQU                3
                                           _PWM4M2            .EQU                2
                                           _PWM4M1            .EQU                1
                                           _PWM4M0            .EQU                0
                                           
                                           ;PWM4CTL1 Bits--------------------------------
                                           PRSEN              .EQU                7
                                           PDC6               .EQU                6
                                           PDC5               .EQU                5
                                           PDC4               .EQU                4
                                           PDC3               .EQU                3
                                           PDC2               .EQU                2
                                           PDC1               .EQU                1
                                           PDC0               .EQU                0
                                           _PRSEN             .EQU                7
                                           _PDC6              .EQU                6
                                           _PDC5              .EQU                5
                                           _PDC4              .EQU                4
                                           _PDC3              .EQU                3
                                           _PDC2              .EQU                2
                                           _PDC1              .EQU                1
                                           _PDC0              .EQU                0
                                           
                                           ;P4ASCTL Bits---------------------------------
                                           P4ASE              .EQU                7
                                           P4ASS2             .EQU                6
                                           P4ASS1             .EQU                5
                                           P4ASS0             .EQU                4
                                           P4SSAC1            .EQU                3
                                           P4SSAC0            .EQU                2
                                           P4SSBD1            .EQU                1
                                           P4SSBD0            .EQU                0
                                           _P4ASE             .EQU                7
                                           _P4ASS2            .EQU                6
                                           _P4ASS1            .EQU                5
                                           _P4ASS0            .EQU                4
                                           _P4SSAC1           .EQU                3
                                           _P4SSAC0           .EQU                2
                                           _P4SSBD1           .EQU                1
                                           _P4SSBD0           .EQU                0
                                           
                                           ;PATRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x690
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 14:52:14 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8V216
                                           	.radix dec
                                           	.include "KF8V216.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8V216 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           CM1CTL            .EQU                0x19
                                           AMPCTL            .EQU                0x1B
                                           VRECAL1           .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           VRECAL2           .EQU                0x2A
                                           VRECTL1           .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP4H              .EQU                0x42
                                           PWM4L1            .EQU                0x43
                                           PWM4H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           PP4L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM4L0            .EQU                0x55
                                           PWM4H0            .EQU                0x56
                                           PWM4CTL0          .EQU                0x57
                                           PWM4CTL1          .EQU                0x5B
                                           P4ASCTL           .EQU                0x5C
                                           PATRCTL           .EQU                0x5D
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL Bits-----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           PWM2ON             .EQU                1
                                           PWM1ON             .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _PWM2ON            .EQU                1
                                           _PWM1ON            .EQU                0
                                           
                                           ;CM1CTL Bits----------------------------------
                                           C1OE               .EQU                7
                                           C1INS              .EQU                6
                                           C1P                .EQU                2
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1OE              .EQU                7
                                           _C1INS             .EQU                6
                                           _C1P               .EQU                2
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;AMPCTL Bits----------------------------------
                                           CALIRD             .EQU                7
                                           CALIEN             .EQU                1
                                           AMPON              .EQU                0
                                           _CALIRD            .EQU                7
                                           _CALIEN            .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;VRECTL1 Bits---------------------------------
                                           VREOE              .EQU                3
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VREOE             .EQU                3
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR Bits-------------------------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCCALIEN          .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM1             .EQU                1
                                           ADCIM0             .EQU                0
                                           _ADCCALIEN         .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM1            .EQU                1
                                           _ADCIM0            .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR2              .EQU                2
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR2             .EQU                2
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;PWM4CTL0 Bits--------------------------------
                                           P4M1               .EQU                7
                                           P4M0               .EQU                6
                                           PWM4M3             .EQU                3
                                           PWM4M2             .EQU                2
                                           PWM4M1             .EQU                1
                                           PWM4M0             .EQU                0
                                           _P4M1              .EQU                7
                                           _P4M0              .EQU                6
                                           _PWM4M3            .EQU                3
                                           _PWM4M2            .EQU                2
                                           _PWM4M1            .EQU                1
                                           _PWM4M0            .EQU                0
                                           
                                           ;PWM4CTL1 Bits--------------------------------
                                           PRSEN              .EQU                7
                                           PDC6               .EQU                6
                                           PDC5               .EQU                5
                                           PDC4               .EQU                4
                                           PDC3               .EQU                3
                                           PDC2               .EQU                2
                                           PDC1               .EQU                1
                                           PDC0               .EQU                0
                                           _PRSEN             .EQU                7
                                           _PDC6              .EQU                6
                                           _PDC5              .EQU                5
                                           _PDC4              .EQU                4
                                           _PDC3              .EQU                3
                                           _PDC2              .EQU                2
                                           _PDC1              .EQU                1
                                           _PDC0              .EQU                0
                                           
                                           ;P4ASCTL Bits---------------------------------
                                           P4ASE              .EQU                7
                                           P4ASS2             .EQU                6
                                           P4ASS1             .EQU                5
                                           P4ASS0             .EQU                4
                                           P4SSAC1            .EQU                3
                                           P4SSAC0            .EQU                2
                                           P4SSBD1            .EQU                1
                                           P4SSBD0            .EQU                0
                                           _P4ASE             .EQU                7
                                           _P4ASS2            .EQU                6
                                           _P4ASS1            .EQU                5
                                           _P4ASS0            .EQU                4
                                           _P4SSAC1           .EQU                3
                                           _P4SSAC0           .EQU                2
                                           _P4SSBD1           .EQU                1
                                           _P4SSBD0           .EQU                0
                                           
                                           ;PATRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CM1CTL_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_VRECTL1_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_PWM4CTL0_bits
                                           	.extern	_PWM4CTL1_bits
                                           	.extern	_P4ASCTL_bits
                                           	.extern	_PATRCTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_CM1CTL
                                           	.extern	_AMPCTL
                                           	.extern	_VRECAL1
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECTL1
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP4H
                                           	.extern	_PWM4L1
                                           	.extern	_PWM4H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_PP4L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM4L0
                                           	.extern	_PWM4H0
                                           	.extern	_PWM4CTL0
                                           	.extern	_PWM4CTL1
                                           	.extern	_P4ASCTL
                                           	.extern	_PATRCTL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Delay_ms
                                           	.global	_init_mcu
                                           	.global	_init_pwm
                                           	.global	_pwm_function
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           
                                           	.global I0R1
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1002	.res	1
                                           UDL_main_1	.udata
                                           r0x1001	.res	1
                                           UDL_main_2	.udata
                                           r0x1003	.res	1
                                           UDL_main_3	.udata
                                           r0x1004	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           LDS_00000	.idata
                                           _pwm_function_direction_1_1
                                           	.db 0
                                           
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
                                           	PAGESEL	init_imp
000001   c085     JMP	#0x85                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
                                           	PAGESEL	_startup
000085   d01e     CALL	#0x1e               	CALL	_startup
                                           	PAGESEL	__sdcc_gsinit_startup
000086   d088     CALL	#0x88               	CALL	__sdcc_gsinit_startup
                                           	PAGESEL	_main
000087   c05c     JMP	#0x5c                	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           _00038_DS_
                                           ;	.line	132; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00040_DS_
                                           ;	.line	139; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;   _Delay_ms
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;   _Delay_ms
                                           ;1 compiler assigned register :
                                           ;   STK00
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	118; "../main.c"	init_mcu();
                                           	PAGESEL	_init_mcu
00005c   d06b     CALL	#0x6b               	CALL	_init_mcu
                                           	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	119; "../main.c"	init_pwm();
                                           	PAGESEL	_init_pwm
00005d   d04b     CALL	#0x4b               	CALL	_init_pwm
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	120; "../main.c"	Delay_ms(10);
00005e   980a     MOV	R0, #0xa             	MOV	R0,# 0x0a
00005f   6503     CLR	0x3, 5               	BANKSEL	STK00
000060   518f     MOV	0x8f, R0             	MOV	STK00, R0
000061   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_Delay_ms
000062   d002     CALL	#0x2                	CALL	_Delay_ms
                                           	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : CALL
                                           _00033_DS_
                                           ;	.line	123; "../main.c"	pwm_function();
                                           	PAGESEL	_pwm_function
000063   d037     CALL	#0x37               	CALL	_pwm_function
                                           	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	124; "../main.c"	Delay_ms(10);
000064   980a     MOV	R0, #0xa             	MOV	R0,# 0x0a
000065   6503     CLR	0x3, 5               	BANKSEL	STK00
000066   518f     MOV	0x8f, R0             	MOV	STK00, R0
000067   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	PAGESEL	_Delay_ms
000068   d002     CALL	#0x2                	CALL	_Delay_ms
                                           	PAGESEL	$
                                           ;	op : GOTO
000069   c063     JMP	#0x63                	JMP	_00033_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00006a   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._pwm_function	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _pwm_function	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _pwm_function	;Function start
                                           ; 2 exit points
                                           ;	op : IFX
                                           ;	.line	92; "../main.c"	if(direction)
000037   9800     MOV	R0, #0               	MOV	R0,# 0x00
000038   6503     CLR	0x3, 5               	BANKSEL	_pwm_function_direction_1_1
000039   3094     ORL	R0, 0x94             	ORL	R0, _pwm_function_direction_1_1
00003a   7203     JNB	0x3, 2               	JNB	PSW, 2
00003b   c043     JMP	#0x43                	JMP	_00023_DS_
                                           ;	op : +
                                           ;	.line	94; "../main.c"	PWM4L0++;
00003c   0b55     INC	0x55                 	INC	_PWM4L0
                                           ;	op : <
                                           ;unsigned compare: left < lit(0xFF=255), size=1
                                           ;	.line	95; "../main.c"	if(PWM4L0>=255)
00003d   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
00003e   3855     SUB	R0, 0x55             	SUB	R0, _PWM4L0
                                           ;comparing bytes at offset 0
00003f   7803     JB	0x3, 0                	JB	PSW, 0
000040   c04a     JMP	#0x4a                	JMP	_00025_DS_
                                           ;	op : =
                                           ;	.line	97; "../main.c"	direction=0;
                                           	BANKSEL	_pwm_function_direction_1_1
000041   0394     CLR	0x94                 	CLR	_pwm_function_direction_1_1
                                           ;	op : GOTO
000042   c04a     JMP	#0x4a                	JMP	_00025_DS_
                                           ;	op : LABEL
                                           ;	op : -
                                           _00023_DS_
                                           ;	.line	102; "../main.c"	PWM4L0--;
000043   0755     DEC	0x55                 	DEC	_PWM4L0
                                           ;	op : IFX
                                           ;	.line	103; "../main.c"	if(PWM4L0==0)
000044   9800     MOV	R0, #0               	MOV	R0,# 0x00
000045   3055     ORL	R0, 0x55             	ORL	R0, _PWM4L0
000046   7a03     JB	0x3, 2                	JB	PSW, 2
000047   c04a     JMP	#0x4a                	JMP	_00025_DS_
                                           ;	op : =
                                           ;	.line	105; "../main.c"	direction=1;
000048   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_pwm_function_direction_1_1
000049   5194     MOV	0x94, R0             	MOV	_pwm_function_direction_1_1, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00025_DS_
00004a   0008     CRET                     	CRET	
                                           ; exit point of _pwm_function
                                           
                                           
                                           
                                           func._init_pwm	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_pwm	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_pwm	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	65; "../main.c"	PWM4CTL1=0x00;	// ²»¿ªÆô×Ô¶¯Ê¹ÄÜ£¬ËÀÇø½ö¶Ô°ëÇÅÓÐÐ§¡£
00004b   035b     CLR	0x5b                 	CLR	_PWM4CTL1
                                           ;	op : =
                                           ;	.line	66; "../main.c"	P4ASCTL=0x00;	// ½ûÖ¹×Ô¶¯¹Ø±ÕÔ´£¬Ä¬ÈÏ¹Ø±Õ×´Ì¬Îª1¡£
00004c   035c     CLR	0x5c                 	CLR	_P4ASCTL
                                           ;	op : =
                                           ;	.line	67; "../main.c"	PATRCTL=0x1F;	// ¿ªÆô×ªÏòÍ¬²½£¬È«²¿Êä³ö£¬0x11 P3A 0x12 P3B  0x14 P3C 0x18 P3D
00004d   981f     MOV	R0, #0x1f            	MOV	R0,# 0x1f
00004e   515d     MOV	0x5d, R0             	MOV	_PATRCTL, R0
                                           ;	op : =
                                           ;	.line	69; "../main.c"	PP4H=0X00;
00004f   0342     CLR	0x42                 	CLR	_PP4H
                                           ;	op : =
                                           ;	.line	70; "../main.c"	PP4L=0XFF;		//T=(0X00FF+1)*(1/16MHz)*1=16us£¬F=1/T=62.5KHz
000050   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
000051   5152     MOV	0x52, R0             	MOV	_PP4L, R0
                                           ;	op : =
                                           ;	.line	72; "../main.c"	PWM4L0=0X80;	//³õÊ¼»¯Õ¼¿Õ±È0X0080/(0X00FF+1)=50%
000052   9880     MOV	R0, #0x80            	MOV	R0,# 0x80
000053   5155     MOV	0x55, R0             	MOV	_PWM4L0, R0
                                           ;	op : =
                                           ;	.line	73; "../main.c"	PWM4L1=0X00;
000054   0343     CLR	0x43                 	CLR	_PWM4L1
                                           ;	op : =
                                           ;	.line	76; "../main.c"	T2H=0;
000055   0341     CLR	0x41                 	CLR	_T2H
                                           ;	op : =
                                           ;	.line	77; "../main.c"	T2L=0;
000056   0311     CLR	0x11                 	CLR	_T2L
                                           ;	op : =
                                           ;	.line	78; "../main.c"	T2CTL=0X04;		// Æô¶¯T2£¬T2·ÖÆµ±È1
000057   9804     MOV	R0, #0x4             	MOV	R0,# 0x04
000058   5112     MOV	0x12, R0             	MOV	_T2CTL, R0
                                           ;	op : =
                                           ;	.line	80; "../main.c"	PWM4CTL0=0x0C;  // µ¥Êä³öÄ£Ê½£¬¿ªÆôPWM4£¬Ä¬ÈÏÓÐÐ§×´Ì¬¸ßµçÆ½¡£
000059   980c     MOV	R0, #0xc             	MOV	R0,# 0x0c
00005a   5157     MOV	0x57, R0             	MOV	_PWM4CTL0, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00005b   0008     CRET                     	CRET	
                                           ; exit point of _init_pwm
                                           
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	42; "../main.c"	OSCCTL = 0X70;      // 16MÊ±ÖÓ
00006b   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
00006c   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	45; "../main.c"	TR0 = 0x08;				//ÉèÖÃP03¶Ë¿ÚÎªÊäÈë£¬P0ÆäËûI/O¿ÚÎªÊä³ö
00006d   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
00006e   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	46; "../main.c"	TR1 = 0x00;				//ÉèÖÃP1¶Ë¿ÚÎªÊä³ö
00006f   0327     CLR	0x27                 	CLR	_TR1
                                           ;	op : =
                                           ;	.line	47; "../main.c"	TR2 = 0x00;				//ÉèÖÃP2¶Ë¿ÚÎªÊä³ö
000070   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	48; "../main.c"	P0 = 0;
000071   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	49; "../main.c"	P1 = 0;
000072   0307     CLR	0x7                  	CLR	_P1
                                           ;	op : =
                                           ;	.line	50; "../main.c"	P2 = 0;
000073   0306     CLR	0x6                  	CLR	_P2
                                           ;	op : =
                                           ;	.line	51; "../main.c"	P0LR = 0;				//P0¿ÚÊä³öµÍµçÆ½
000074   0345     CLR	0x45                 	CLR	_P0LR
                                           ;	op : =
                                           ;	.line	52; "../main.c"	P1LR = 0;				//P1¿ÚÊä³öµÍµçÆ½
000075   0347     CLR	0x47                 	CLR	_P1LR
                                           ;	op : =
                                           ;	.line	53; "../main.c"	P2LR = 0;				//P2¿ÚÊä³öµÍµçÆ½
000076   0346     CLR	0x46                 	CLR	_P2LR
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000077   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           
                                           func._Delay_ms	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x1001
                                           ;   STK00
                                           ;   r0x1002
                                           ;   r0x1003
                                           ;   r0x1004
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	23; "../main.c"	void Delay_ms(uint ms_data)
000002   6503     CLR	0x3, 5               	BANKSEL	r0x1001
000003   5191     MOV	0x91, R0             	MOV	r0x1001, R0
                                           	BANKSEL	STK00
000004   0e8f     MOVZ	R0, 0x8f            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1002
000005   5190     MOV	0x90, R0             	MOV	r0x1002, R0
                                           ;	op : =
                                           ;	op : LABEL
                                           ;	op : =
                                           _00004_DS_
                                           ;	.line	26; "../main.c"	while(ms_data--)
                                           	BANKSEL	r0x1002
000006   0e90     MOVZ	R0, 0x90            	MOVZ	R0, r0x1002
                                           	BANKSEL	r0x1003
000007   5192     MOV	0x92, R0             	MOV	r0x1003, R0
                                           	BANKSEL	r0x1001
000008   0e91     MOVZ	R0, 0x91            	MOVZ	R0, r0x1001
                                           	BANKSEL	r0x1004
000009   5193     MOV	0x93, R0             	MOV	r0x1004, R0
                                           ;	op : -
00000a   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x1002
00000b   2190     ADD	0x90, R0             	ADD	r0x1002, R0
00000c   7003     JNB	0x3, 0               	JNB	PSW, 0
00000d   c00f     JMP	#0xf                 	JMP	_00042_DS_
                                           	BANKSEL	r0x1001
00000e   0791     DEC	0x91                 	DEC	r0x1001
                                           ;	op : IFX
                                           _00042_DS_
                                           	BANKSEL	r0x1003
00000f   0e92     MOVZ	R0, 0x92            	MOVZ	R0, r0x1003
                                           	BANKSEL	r0x1004
000010   3093     ORL	R0, 0x93             	ORL	R0, r0x1004
000011   7203     JNB	0x3, 2               	JNB	PSW, 2
000012   c01d     JMP	#0x1d                	JMP	_00007_DS_
                                           ;	op : =
                                           ;	.line	29; "../main.c"	while(i--);
000013   987c     MOV	R0, #0x7c            	MOV	R0,# 0x7c
                                           	BANKSEL	r0x1003
000014   5192     MOV	0x92, R0             	MOV	r0x1003, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00001_DS_
                                           	BANKSEL	r0x1003
000015   0e92     MOVZ	R0, 0x92            	MOVZ	R0, r0x1003
                                           	BANKSEL	r0x1004
000016   5193     MOV	0x93, R0             	MOV	r0x1004, R0
                                           ;	op : -
                                           	BANKSEL	r0x1003
000017   0792     DEC	0x92                 	DEC	r0x1003
                                           ;	op : IFX
000018   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1004
000019   3093     ORL	R0, 0x93             	ORL	R0, r0x1004
00001a   7203     JNB	0x3, 2               	JNB	PSW, 2
00001b   c006     JMP	#0x6                 	JMP	_00004_DS_
                                           ;	op : GOTO
00001c   c015     JMP	#0x15                	JMP	_00001_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00007_DS_
00001d   0008     CRET                     	CRET	
                                           ; exit point of _Delay_ms
                                           
                                           
                                           ;	code size estimation:
                                           ;	  101+   21 =   122 instructions (  286 byte)
                                           
                                           
                                           	.end
                                           .config
002007   0690     DECR	0x90               
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
000088   d078     CALL	#0x78              
000089   0008     CRET                    
                                           .code
00001e   d7fa     CALL	#0x7fa             
00001f   512a     MOV	0x2a, R0            
000020   ffff     NOPZ                    
000021   ffff     NOPZ                    
000022   d7fb     CALL	#0x7fb             
000023   511c     MOV	0x1c, R0            
000024   ffff     NOPZ                    
000025   ffff     NOPZ                    
000026   d7fc     CALL	#0x7fc             
000027   514d     MOV	0x4d, R0            
000028   ffff     NOPZ                    
000029   ffff     NOPZ                    
00002a   d7fd     CALL	#0x7fd             
00002b   514c     MOV	0x4c, R0            
00002c   ffff     NOPZ                    
00002d   ffff     NOPZ                    
00002e   d7fe     CALL	#0x7fe             
00002f   5137     MOV	0x37, R0            
000030   ffff     NOPZ                    
000031   ffff     NOPZ                    
000032   d7ff     CALL	#0x7ff             
000033   5130     MOV	0x30, R0            
000034   ffff     NOPZ                    
000035   ffff     NOPZ                    
000036   0008     CRET                    
                                           .cinit
000078   6503     CLR	0x3, 5              
000079   9880     MOV	R0, #0x80           
00007a   9914     MOV	R1, #0x14           
00007b   0000     NOP                     
00007c   d07f     CALL	#0x7f              
00007d   0394     CLR	0x94                
00007e   0008     CRET                    
00007f   020a     CLR	R2                  
000080   f750     ST	[R0], R2             
000081   ff10     INC	R0                  
000082   ff59     DECJZ	R1                
000083   c080     JMP	#0x80               
000084   0008     CRET                    
