gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 6-6-2016  15:37:50
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Mon Jun 06 15:34:40 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8V216
                                           	.radix dec
                                           	.include "KF8V216.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8V216 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           CM1CTL            .EQU                0x19
                                           AMPCTL            .EQU                0x1B
                                           VRECAL1           .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           VRECAL2           .EQU                0x2A
                                           VRECTL1           .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP4H              .EQU                0x42
                                           PWM4L1            .EQU                0x43
                                           PWM4H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           PP4L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM4L0            .EQU                0x55
                                           PWM4H0            .EQU                0x56
                                           PWM4CTL0          .EQU                0x57
                                           PWM4CTL1          .EQU                0x5B
                                           P4ASCTL           .EQU                0x5C
                                           PATRCTL           .EQU                0x5D
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL Bits-----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           PWM2ON             .EQU                1
                                           PWM1ON             .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _PWM2ON            .EQU                1
                                           _PWM1ON            .EQU                0
                                           
                                           ;CM1CTL Bits----------------------------------
                                           C1OE               .EQU                7
                                           C1INS              .EQU                6
                                           C1P                .EQU                2
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1OE              .EQU                7
                                           _C1INS             .EQU                6
                                           _C1P               .EQU                2
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;AMPCTL Bits----------------------------------
                                           CALIRD             .EQU                7
                                           CALIEN             .EQU                1
                                           AMPON              .EQU                0
                                           _CALIRD            .EQU                7
                                           _CALIEN            .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;VRECTL1 Bits---------------------------------
                                           VREOE              .EQU                3
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VREOE             .EQU                3
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR Bits-------------------------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCCALIEN          .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM1             .EQU                1
                                           ADCIM0             .EQU                0
                                           _ADCCALIEN         .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM1            .EQU                1
                                           _ADCIM0            .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR2              .EQU                2
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR2             .EQU                2
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;PWM4CTL0 Bits--------------------------------
                                           P4M1               .EQU                7
                                           P4M0               .EQU                6
                                           PWM4M3             .EQU                3
                                           PWM4M2             .EQU                2
                                           PWM4M1             .EQU                1
                                           PWM4M0             .EQU                0
                                           _P4M1              .EQU                7
                                           _P4M0              .EQU                6
                                           _PWM4M3            .EQU                3
                                           _PWM4M2            .EQU                2
                                           _PWM4M1            .EQU                1
                                           _PWM4M0            .EQU                0
                                           
                                           ;PWM4CTL1 Bits--------------------------------
                                           PRSEN              .EQU                7
                                           PDC6               .EQU                6
                                           PDC5               .EQU                5
                                           PDC4               .EQU                4
                                           PDC3               .EQU                3
                                           PDC2               .EQU                2
                                           PDC1               .EQU                1
                                           PDC0               .EQU                0
                                           _PRSEN             .EQU                7
                                           _PDC6              .EQU                6
                                           _PDC5              .EQU                5
                                           _PDC4              .EQU                4
                                           _PDC3              .EQU                3
                                           _PDC2              .EQU                2
                                           _PDC1              .EQU                1
                                           _PDC0              .EQU                0
                                           
                                           ;P4ASCTL Bits---------------------------------
                                           P4ASE              .EQU                7
                                           P4ASS2             .EQU                6
                                           P4ASS1             .EQU                5
                                           P4ASS0             .EQU                4
                                           P4SSAC1            .EQU                3
                                           P4SSAC0            .EQU                2
                                           P4SSBD1            .EQU                1
                                           P4SSBD0            .EQU                0
                                           _P4ASE             .EQU                7
                                           _P4ASS2            .EQU                6
                                           _P4ASS1            .EQU                5
                                           _P4ASS0            .EQU                4
                                           _P4SSAC1           .EQU                3
                                           _P4SSAC0           .EQU                2
                                           _P4SSBD1           .EQU                1
                                           _P4SSBD0           .EQU                0
                                           
                                           ;PATRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x690
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Mon Jun 06 15:37:50 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8V216
                                           	.radix dec
                                           	.include "KF8V216.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8V216 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL             .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           CM1CTL            .EQU                0x19
                                           AMPCTL            .EQU                0x1B
                                           VRECAL1           .EQU                0x1C
                                           ANSEH             .EQU                0x1D
                                           ADCDATAH          .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           VRECAL2           .EQU                0x2A
                                           VRECTL1           .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR               .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           ADCDATAL          .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP4H              .EQU                0x42
                                           PWM4L1            .EQU                0x43
                                           PWM4H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           PP4L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM4L0            .EQU                0x55
                                           PWM4H0            .EQU                0x56
                                           PWM4CTL0          .EQU                0x57
                                           PWM4CTL1          .EQU                0x5B
                                           P4ASCTL           .EQU                0x5C
                                           PATRCTL           .EQU                0x5D
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           RP0                .EQU                5
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _RP0               .EQU                5
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL Bits-----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           PWM2ON             .EQU                1
                                           PWM1ON             .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _PWM2ON            .EQU                1
                                           _PWM1ON            .EQU                0
                                           
                                           ;CM1CTL Bits----------------------------------
                                           C1OE               .EQU                7
                                           C1INS              .EQU                6
                                           C1P                .EQU                2
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1OE              .EQU                7
                                           _C1INS             .EQU                6
                                           _C1P               .EQU                2
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;AMPCTL Bits----------------------------------
                                           CALIRD             .EQU                7
                                           CALIEN             .EQU                1
                                           AMPON              .EQU                0
                                           _CALIRD            .EQU                7
                                           _CALIEN            .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;VRECTL1 Bits---------------------------------
                                           VREOE              .EQU                3
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VREOE             .EQU                3
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CKOEN              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           _CKOEN             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR Bits-------------------------------------
                                           PUR5               .EQU                5
                                           PUR4               .EQU                4
                                           PUR2               .EQU                2
                                           PUR1               .EQU                1
                                           PUR0               .EQU                0
                                           _PUR5              .EQU                5
                                           _PUR4              .EQU                4
                                           _PUR2              .EQU                2
                                           _PUR1              .EQU                1
                                           _PUR0              .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCCALIEN          .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM1             .EQU                1
                                           ADCIM0             .EQU                0
                                           _ADCCALIEN         .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM1            .EQU                1
                                           _ADCIM0            .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR2              .EQU                2
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR2             .EQU                2
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;PWM4CTL0 Bits--------------------------------
                                           P4M1               .EQU                7
                                           P4M0               .EQU                6
                                           PWM4M3             .EQU                3
                                           PWM4M2             .EQU                2
                                           PWM4M1             .EQU                1
                                           PWM4M0             .EQU                0
                                           _P4M1              .EQU                7
                                           _P4M0              .EQU                6
                                           _PWM4M3            .EQU                3
                                           _PWM4M2            .EQU                2
                                           _PWM4M1            .EQU                1
                                           _PWM4M0            .EQU                0
                                           
                                           ;PWM4CTL1 Bits--------------------------------
                                           PRSEN              .EQU                7
                                           PDC6               .EQU                6
                                           PDC5               .EQU                5
                                           PDC4               .EQU                4
                                           PDC3               .EQU                3
                                           PDC2               .EQU                2
                                           PDC1               .EQU                1
                                           PDC0               .EQU                0
                                           _PRSEN             .EQU                7
                                           _PDC6              .EQU                6
                                           _PDC5              .EQU                5
                                           _PDC4              .EQU                4
                                           _PDC3              .EQU                3
                                           _PDC2              .EQU                2
                                           _PDC1              .EQU                1
                                           _PDC0              .EQU                0
                                           
                                           ;P4ASCTL Bits---------------------------------
                                           P4ASE              .EQU                7
                                           P4ASS2             .EQU                6
                                           P4ASS1             .EQU                5
                                           P4ASS0             .EQU                4
                                           P4SSAC1            .EQU                3
                                           P4SSAC0            .EQU                2
                                           P4SSBD1            .EQU                1
                                           P4SSBD0            .EQU                0
                                           _P4ASE             .EQU                7
                                           _P4ASS2            .EQU                6
                                           _P4ASS1            .EQU                5
                                           _P4ASS0            .EQU                4
                                           _P4SSAC1           .EQU                3
                                           _P4SSAC0           .EQU                2
                                           _P4SSBD1           .EQU                1
                                           _P4SSBD0           .EQU                0
                                           
                                           ;PATRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_CM1CTL_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_VRECTL1_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_PWM4CTL0_bits
                                           	.extern	_PWM4CTL1_bits
                                           	.extern	_P4ASCTL_bits
                                           	.extern	_PATRCTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_CM1CTL
                                           	.extern	_AMPCTL
                                           	.extern	_VRECAL1
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATAH
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECTL1
                                           	.extern	_EIE1
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_ADCDATAL
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP4H
                                           	.extern	_PWM4L1
                                           	.extern	_PWM4H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_PP4L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM4L0
                                           	.extern	_PWM4H0
                                           	.extern	_PWM4CTL0
                                           	.extern	_PWM4CTL1
                                           	.extern	_P4ASCTL
                                           	.extern	_PATRCTL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Init_fun
                                           	.global	_Delay
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           
                                           	.global I0R1
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1000	.res	1
                                           UDL_main_1	.udata
                                           r0x1001	.res	1
                                           UDL_main_2	.udata
                                           r0x1002	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
                                           	PAGESEL	init_imp
000001   c072     JMP	#0x72                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
                                           	PAGESEL	_startup
000072   d00b     CALL	#0xb                	CALL	_startup
                                           	PAGESEL	__sdcc_gsinit_startup
000073   d002     CALL	#0x2                	CALL	__sdcc_gsinit_startup
                                           	PAGESEL	_main
000074   c069     JMP	#0x69                	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           interrupt_0x04	.code	0x4
000004   f8c2     MOV	R2, R0               	MOV		R2,R0
000005   5603     MOV	R3, 0x3              	MOV		R3,PSW
000006   500a     MOV	R0, 0xa              	MOV		R0,PCH
000007   6503     CLR	0x3, 5               	BANKSEL	I0PCH
000008   5181     MOV	0x81, R0             	MOV		I0PCH,R0
000009   5380     MOV	0x80, R1             	MOV		I0R1,R1
                                           	PAGESEL	interrupt_service_routine_0x04
00000a   c04e     JMP	#0x4e                	JMP		interrupt_service_routine_0x04
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           ;	.line	116; "../main.c"	if (INT2IF)
00004e   7d0c     JB	0xc, 5                	JB	_EIF1_bits, 5
00004f   c056     JMP	#0x56                	JMP	_00028_DS_
                                           ;	op : =
                                           ;	.line	118; "../main.c"	INT2IF = 0;                 // ÇåÖÐ¶Ï±êÖ¾
000050   650c     CLR	0xc, 5               	CLR	_EIF1_bits, 5
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	op : !
                                           ;	op : =
                                           ;	.line	119; "../main.c"	LED1 = !LED1;               // ¸ü¸Ä D3 ÏÔÊ¾×´Ì¬
000051   7c47     JB	0x47, 4               	JB	_P1LR_bits, 4
000052   c055     JMP	#0x55                	JMP	_00031_DS_
000053   6447     CLR	0x47, 4              	CLR	_P1LR_bits, 4
000054   c056     JMP	#0x56                	JMP	_00028_DS_
                                           _00031_DS_
000055   6c47     SET	0x47, 4              	SET	_P1LR_bits, 4
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00028_DS_
000056   6503     CLR	0x3, 5               	BANKSEL	I0R1
000057   5280     MOV	R1, 0x80             	MOV	R1, I0R1
                                           	BANKSEL	I0PCH
000058   5081     MOV	R0, 0x81             	MOV	R0, I0PCH
000059   510a     MOV	0xa, R0              	MOV	PCH, R0
00005a   5703     MOV	0x3, R3              	MOV	PSW, R3
00005b   f8d0     MOV	R0, R2               	MOV	R0, R2
00005c   0009     IRET                     	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00033_DS_
                                           ;	.line	128; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _Init_fun
                                           ;   _Delay
                                           ;   _Init_fun
                                           ;   _Delay
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	87; "../main.c"	Init_fun();
                                           	PAGESEL	_Init_fun
000069   d024     CALL	#0x24               	CALL	_Init_fun
                                           	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	op : !
                                           ;	op : =
                                           _00019_DS_
                                           ;	.line	91; "../main.c"	P1LR1 = !P1LR1;                 //  ¸Ä±äP11¿ÚµçÆ½
00006a   7947     JB	0x47, 1               	JB	_P1LR_bits, 1
00006b   c06e     JMP	#0x6e                	JMP	_00024_DS_
00006c   6147     CLR	0x47, 1              	CLR	_P1LR_bits, 1
00006d   c06f     JMP	#0x6f                	JMP	_00025_DS_
                                           _00024_DS_
00006e   6947     SET	0x47, 1              	SET	_P1LR_bits, 1
                                           ;	op : CALL
                                           _00025_DS_
                                           ;	.line	92; "../main.c"	Delay();
                                           	PAGESEL	_Delay
00006f   d03a     CALL	#0x3a               	CALL	_Delay
                                           	PAGESEL	$
                                           ;	op : GOTO
000070   c06a     JMP	#0x6a                	JMP	_00019_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000071   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._Delay	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Delay	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;3 compiler assigned registers:
                                           ;   r0x1000
                                           ;   r0x1001
                                           ;   r0x1002
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Delay	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	81; "../main.c"	for (i = 0;i < 200;i++)
00003a   6503     CLR	0x3, 5               	BANKSEL	r0x1000
00003b   0390     CLR	0x90                 	CLR	r0x1000
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0xC8=200), size=1
                                           _00006_DS_
00003c   98c8     MOV	R0, #0xc8            	MOV	R0,# 0xc8
                                           	BANKSEL	r0x1000
00003d   3890     SUB	R0, 0x90             	SUB	R0, r0x1000
                                           ;comparing bytes at offset 0
00003e   7003     JNB	0x3, 0               	JNB	PSW, 0
00003f   c04d     JMP	#0x4d                	JMP	_00010_DS_
                                           ;	op : =
                                           ;	.line	82; "../main.c"	for (j = 0;j < 200;j++);
000040   98c8     MOV	R0, #0xc8            	MOV	R0,# 0xc8
                                           	BANKSEL	r0x1001
000041   5191     MOV	0x91, R0             	MOV	r0x1001, R0
                                           ;	op : LABEL
                                           ;	op : CAST
                                           _00005_DS_
                                           	BANKSEL	r0x1001
000042   0e91     MOVZ	R0, 0x91            	MOVZ	R0, r0x1001
                                           	BANKSEL	r0x1002
000043   5192     MOV	0x92, R0             	MOV	r0x1002, R0
                                           ;	op : -
                                           	BANKSEL	r0x1002
000044   0792     DEC	0x92                 	DEC	r0x1002
                                           ;	op : CAST
                                           	BANKSEL	r0x1002
000045   0e92     MOVZ	R0, 0x92            	MOVZ	R0, r0x1002
                                           	BANKSEL	r0x1001
000046   5191     MOV	0x91, R0             	MOV	r0x1001, R0
                                           ;	op : IFX
000047   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1001
000048   3091     ORL	R0, 0x91             	ORL	R0, r0x1001
000049   7a03     JB	0x3, 2                	JB	PSW, 2
00004a   c042     JMP	#0x42                	JMP	_00005_DS_
                                           ;	op : +
                                           ;	.line	81; "../main.c"	for (i = 0;i < 200;i++)
                                           	BANKSEL	r0x1000
00004b   0b90     INC	0x90                 	INC	r0x1000
                                           ;	op : GOTO
00004c   c03c     JMP	#0x3c                	JMP	_00006_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00010_DS_
00004d   0008     CRET                     	CRET	
                                           ; exit point of _Delay
                                           
                                           
                                           
                                           func._Init_fun	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Init_fun	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Init_fun	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	28; "../main.c"	OSCCTL = 0x60;                           //ÉèÖÃÏµÍ³Ê±ÖÓÎª8M
000024   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
000025   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	31; "../main.c"	TR0 = 0x0c;				                 //ÉèÖÃP03 P02(INT0) ¶Ë¿ÚÖ»ÄÜÉèÖÃÎªÊäÈë
000026   980c     MOV	R0, #0xc             	MOV	R0,# 0x0c
000027   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	32; "../main.c"	TR1 = 0x0c;				                 //P12(INT1)/P13(INT2)¿ÚÎªÍâ²¿ÖÐ¶ÏÒý½Å£¬ÐèÅäÖÃÎªÊý×ÖÊäÈë¿ÚÉèÖÃP1¶Ë¿ÚÎªÊä³ö
000028   980c     MOV	R0, #0xc             	MOV	R0,# 0x0c
000029   5127     MOV	0x27, R0             	MOV	_TR1, R0
                                           ;	op : =
                                           ;	.line	33; "../main.c"	TR2 = 0x00;				                 //ÉèÖÃP2¶Ë¿ÚÎªÊä³ö
00002a   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	35; "../main.c"	P0 = 0x00;
00002b   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	36; "../main.c"	P1 = 0x00;
00002c   0307     CLR	0x7                  	CLR	_P1
                                           ;	op : =
                                           ;	.line	37; "../main.c"	P2 = 0x00;
00002d   0306     CLR	0x6                  	CLR	_P2
                                           ;	op : =
                                           ;	.line	39; "../main.c"	P0LR = 0;
00002e   0345     CLR	0x45                 	CLR	_P0LR
                                           ;	op : =
                                           ;	.line	40; "../main.c"	P1LR = 0;
00002f   0347     CLR	0x47                 	CLR	_P1LR
                                           ;	op : =
                                           ;	.line	41; "../main.c"	P2LR = 0;
000030   0346     CLR	0x46                 	CLR	_P2LR
                                           ;	op : =
                                           ;	.line	43; "../main.c"	ANSEL = 0;                               //ÅäÖÃP12¿ÚÎªÊý×Ö¿Ú
000031   0331     CLR	0x31                 	CLR	_ANSEL
                                           ;	op : =
                                           ;	.line	44; "../main.c"	ANSEH = 0;
000032   031d     CLR	0x1d                 	CLR	_ANSEH
                                           ;	op : =
                                           ;	.line	61; "../main.c"	INT2IF = 0;   //  ÇåÖÐ¶Ï±êÖ¾Î»
000033   650c     CLR	0xc, 5               	CLR	_EIF1_bits, 5
                                           ;	op : =
                                           ;	.line	62; "../main.c"	INT2SE = 0;   //  0 £ºÏÂ½µÑØ             1£ºÉÏÉýÑØ
000034   6715     CLR	0x15, 7              	CLR	_PWMCTL_bits, 7
                                           ;	op : =
                                           ;	.line	63; "../main.c"	INT2IE = 1;   //  Ê¹ÄÜÖÐ¶Ï
000035   6d2c     SET	0x2c, 5              	SET	_EIE1_bits, 5
                                           ;	op : =
                                           ;	.line	64; "../main.c"	PUIE = 1;     //  INT2 ÊôÓÚÍâ²¿ÖÐ¶Ï
000036   6e0b     SET	0xb, 6               	SET	_INTCTL_bits, 6
                                           ;	op : =
                                           ;	.line	66; "../main.c"	PCTL = 0;     // ½ûÖ¹ÖÐ¶ÏÓÅÏÈ¼¶
000037   032e     CLR	0x2e                 	CLR	_PCTL
                                           ;	op : =
                                           ;	.line	67; "../main.c"	AIE = 1;      // Ê¹ÄÜ×ÜÖÐ¶Ï
000038   6f0b     SET	0xb, 7               	SET	_INTCTL_bits, 7
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000039   0008     CRET                     	CRET	
                                           ; exit point of _Init_fun
                                           
                                           
                                           ;	code size estimation:
                                           ;	   69+   12 =    81 instructions (  186 byte)
                                           
                                           
                                           	.end
                                           .config
002007   0690     DECR	0x90               
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
000002   d05d     CALL	#0x5d              
000003   0008     CRET                    
                                           .code
00000b   d7fa     CALL	#0x7fa             
00000c   512a     MOV	0x2a, R0            
00000d   ffff     NOPZ                    
00000e   ffff     NOPZ                    
00000f   d7fb     CALL	#0x7fb             
000010   511c     MOV	0x1c, R0            
000011   ffff     NOPZ                    
000012   ffff     NOPZ                    
000013   d7fc     CALL	#0x7fc             
000014   514d     MOV	0x4d, R0            
000015   ffff     NOPZ                    
000016   ffff     NOPZ                    
000017   d7fd     CALL	#0x7fd             
000018   514c     MOV	0x4c, R0            
000019   ffff     NOPZ                    
00001a   ffff     NOPZ                    
00001b   d7fe     CALL	#0x7fe             
00001c   5137     MOV	0x37, R0            
00001d   ffff     NOPZ                    
00001e   ffff     NOPZ                    
00001f   d7ff     CALL	#0x7ff             
000020   5130     MOV	0x30, R0            
000021   ffff     NOPZ                    
000022   ffff     NOPZ                    
000023   0008     CRET                    
                                           .cinit
00005d   6503     CLR	0x3, 5              
00005e   9880     MOV	R0, #0x80           
00005f   9913     MOV	R1, #0x13           
000060   0000     NOP                     
000061   d063     CALL	#0x63              
000062   0008     CRET                    
000063   020a     CLR	R2                  
000064   f750     ST	[R0], R2             
000065   ff10     INC	R0                  
000066   ff59     DECJZ	R1                
000067   c064     JMP	#0x64               
000068   0008     CRET                    
