gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 5-20-2016  14:54:19
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 14:35:06 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x3fd4
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 14:54:19 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_ADCINTCTL_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWMPC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_ADCDATA1H
                                           	.extern	_ADCDATA1L
                                           	.extern	_PP5L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_ADCINTCTL
                                           	.extern	_ADCDATA2H
                                           	.extern	_ADCDATA2L
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_ADCDATA3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_ADCDATA3L
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWMPC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Delay_ms
                                           	.global	_init_mcu
                                           	.global	_init_pwm
                                           	.global	_pwm_function
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           
                                           	.global I0R1
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1001	.res	1
                                           UDL_main_1	.udata
                                           r0x1000	.res	1
                                           UDL_main_2	.udata
                                           r0x1002	.res	1
                                           UDL_main_3	.udata
                                           r0x1003	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e010     MOVP	0x10                	PAGESEL	init_imp
000002   c08b     JMP	#0x8b                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
00108b   e010     MOVP	0x10                	PAGESEL	_startup
00108c   d000     CALL	#0                  	CALL	_startup
00108d   e010     MOVP	0x10                	PAGESEL	__sdcc_gsinit_startup
00108e   d091     CALL	#0x91               	CALL	__sdcc_gsinit_startup
00108f   e010     MOVP	0x10                	PAGESEL	_main
001090   c040     JMP	#0x40                	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           _00026_DS_
                                           ;	.line	121; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00028_DS_
                                           ;	.line	128; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;   _Delay_ms
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;   _Delay_ms
                                           ;1 compiler assigned register :
                                           ;   STK00
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	106; "../main.c"	init_mcu();
001040   e010     MOVP	0x10                	PAGESEL	_init_mcu
001041   d06e     CALL	#0x6e               	CALL	_init_mcu
001042   e010     MOVP	0x10                	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	107; "../main.c"	init_pwm();
001043   e010     MOVP	0x10                	PAGESEL	_init_pwm
001044   d059     CALL	#0x59               	CALL	_init_pwm
001045   e010     MOVP	0x10                	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	108; "../main.c"	Delay_ms(10);
001046   980a     MOV	R0, #0xa             	MOV	R0,# 0x0a
001047   e100     MOVB	0                   	BANKSEL	STK00
001048   5191     MOV	0x91, R0             	MOV	STK00, R0
001049   9800     MOV	R0, #0               	MOV	R0,# 0x00
00104a   e010     MOVP	0x10                	PAGESEL	_Delay_ms
00104b   d024     CALL	#0x24               	CALL	_Delay_ms
00104c   e010     MOVP	0x10                	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : CALL
                                           _00021_DS_
                                           ;	.line	112; "../main.c"	pwm_function();
00104d   e010     MOVP	0x10                	PAGESEL	_pwm_function
00104e   d095     CALL	#0x95               	CALL	_pwm_function
00104f   e010     MOVP	0x10                	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	113; "../main.c"	Delay_ms(10);
001050   980a     MOV	R0, #0xa             	MOV	R0,# 0x0a
001051   e100     MOVB	0                   	BANKSEL	STK00
001052   5191     MOV	0x91, R0             	MOV	STK00, R0
001053   9800     MOV	R0, #0               	MOV	R0,# 0x00
001054   e010     MOVP	0x10                	PAGESEL	_Delay_ms
001055   d024     CALL	#0x24               	CALL	_Delay_ms
001056   e010     MOVP	0x10                	PAGESEL	$
                                           ;	op : GOTO
001057   c04d     JMP	#0x4d                	JMP	_00021_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
001058   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._pwm_function	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _pwm_function	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _pwm_function	;Function start
                                           ; 2 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ;	.line	96; "../main.c"	}
001095   0008     CRET                     	CRET	
                                           ; exit point of _pwm_function
                                           
                                           
                                           
                                           func._init_pwm	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_pwm	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_pwm	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	72; "../main.c"	P5ASCTL		= 0b00000000;			//ÉèÖÃPWM5¹Ø±ÕÊ±ºòPWM¿ÚÊä³öµçÆ½		ÕâÀïÎªÄ¬ÈÏÉèÖÃ£¬¹Ø±ÕPWMÊ±ºò¶¼Êä³ö0
001059   e100     MOVB	0                   	BANKSEL	_P5ASCTL
00105a   035c     CLR	0x5c                 	CLR	_P5ASCTL
                                           ;	op : =
                                           ;	.line	73; "../main.c"	PWM5CTL2	= 0b00000001;			//PWMÖÜÆÚ×Ô¶¯Ìî³ä¸üÐÂ
00105b   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
00105c   e101     MOVB	0x1                 	BANKSEL	_PWM5CTL2
00105d   511c     MOV	0x1c, R0             	MOV	_PWM5CTL2, R0
                                           ;	op : =
                                           ;	.line	75; "../main.c"	PWM5CTL0	= 0b00001100; 			//µ¥Êä³öPWM¸ßµçÆ½ÓÐÐ§
00105e   980c     MOV	R0, #0xc             	MOV	R0,# 0x0c
00105f   e100     MOVB	0                   	BANKSEL	_PWM5CTL0
001060   5157     MOV	0x57, R0             	MOV	_PWM5CTL0, R0
                                           ;	op : =
                                           ;	.line	76; "../main.c"	PSTRCTL		= 0b00010001;			//PWMµ¥ÏîÊä³öÊ±ºò£¬ºÍÈ«ÇÅÊä³öÊ±ºò£¬PWMÐÅºÅ¿ØÖÆÊÇ·ñÊä³öµ½ÏàÓ¦IOÉÏ£¬ PSTRCTL£¨3:0£©·Ö±ðÎªP5D P5C P5B P5A,P5A=1Ôò£¬PWMÊä³öµ½P5A¿Ú£¬ÆäËûÎªÉèÖÃÎª1Êä³öµ½ÆäËû¿Ú
001061   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
                                           	BANKSEL	_PSTRCTL
001062   515d     MOV	0x5d, R0             	MOV	_PSTRCTL, R0
                                           ;	op : =
                                           ;	.line	77; "../main.c"	PP5H		= 0;					//¸ßÎ»
                                           	BANKSEL	_PP5H
001063   0342     CLR	0x42                 	CLR	_PP5H
                                           ;	op : =
                                           ;	.line	78; "../main.c"	PP5L		= 40;					//ÉèÖÃPWMÖÜÆÚ  ÖÜÆÚÊ±¼äÎªPP5+1½øÐÐ¼ÆËã
001064   9828     MOV	R0, #0x28            	MOV	R0,# 0x28
                                           	BANKSEL	_PP5L
001065   5152     MOV	0x52, R0             	MOV	_PP5L, R0
                                           ;	op : =
                                           ;	.line	79; "../main.c"	PWM5L1		= 0;					//¸ßÎ»
                                           	BANKSEL	_PWM5L1
001066   0356     CLR	0x56                 	CLR	_PWM5L1
                                           ;	op : =
                                           ;	.line	80; "../main.c"	PWM5L0		= 20;					//ÉèÖÃPWMÕ¼¿Õ±È
001067   9814     MOV	R0, #0x14            	MOV	R0,# 0x14
                                           	BANKSEL	_PWM5L0
001068   5155     MOV	0x55, R0             	MOV	_PWM5L0, R0
                                           ;	op : =
                                           ;	.line	81; "../main.c"	T2H			= 0;
                                           	BANKSEL	_T2H
001069   0341     CLR	0x41                 	CLR	_T2H
                                           ;	op : =
                                           ;	.line	82; "../main.c"	T2L			= 0;					//PWMÊ±ÖÓÔ´ T2Ïà¹ØÉèÖÃ
                                           	BANKSEL	_T2L
00106a   0311     CLR	0x11                 	CLR	_T2L
                                           ;	op : =
                                           ;	.line	83; "../main.c"	T2CTL0		= 0b00000000;
                                           	BANKSEL	_T2CTL0
00106b   0312     CLR	0x12                 	CLR	_T2CTL0
                                           ;	op : =
                                           ;	.line	84; "../main.c"	T2ON		= 1;
                                           	BANKSEL	_T2CTL0_bits
00106c   6a12     SET	0x12, 2              	SET	_T2CTL0_bits, 2
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00106d   0008     CRET                     	CRET	
                                           ; exit point of _init_pwm
                                           
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	45; "../main.c"	OSCCTL = 0x70;          //ÉèÖÃÎª16M
00106e   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
00106f   e100     MOVB	0                   	BANKSEL	_OSCCTL
001070   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	48; "../main.c"	TR0 = 0x08;				//ÉèÖÃP03¶Ë¿ÚÎªÊäÈë£¬P0ÆäËûI/O¿ÚÎªÊä³ö
001071   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	_TR0
001072   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	49; "../main.c"	TR1 = 0x00;				//ÉèÖÃP1¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR1
001073   0327     CLR	0x27                 	CLR	_TR1
                                           ;	op : =
                                           ;	.line	50; "../main.c"	TR2 = 0x00;				//ÉèÖÃP2¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR2
001074   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	51; "../main.c"	TR3 = 0x00;				//ÉèÖÃP3¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR3
001075   0349     CLR	0x49                 	CLR	_TR3
                                           ;	op : =
                                           ;	.line	52; "../main.c"	P0 = 0;
                                           	BANKSEL	_P0
001076   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	53; "../main.c"	P1 = 0;
                                           	BANKSEL	_P1
001077   0307     CLR	0x7                  	CLR	_P1
                                           ;	op : =
                                           ;	.line	54; "../main.c"	P2 = 0;
                                           	BANKSEL	_P2
001078   0306     CLR	0x6                  	CLR	_P2
                                           ;	op : =
                                           ;	.line	55; "../main.c"	P3 = 0;
                                           	BANKSEL	_P3
001079   0308     CLR	0x8                  	CLR	_P3
                                           ;	op : =
                                           ;	.line	56; "../main.c"	P0LR = 0;				//P0¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P0LR
00107a   0345     CLR	0x45                 	CLR	_P0LR
                                           ;	op : =
                                           ;	.line	57; "../main.c"	P1LR = 0;				//P1¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P1LR
00107b   0347     CLR	0x47                 	CLR	_P1LR
                                           ;	op : =
                                           ;	.line	58; "../main.c"	P2LR = 0;				//P2¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P2LR
00107c   0346     CLR	0x46                 	CLR	_P2LR
                                           ;	op : =
                                           ;	.line	59; "../main.c"	P3LR = 0;				//P3¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P3LR
00107d   0348     CLR	0x48                 	CLR	_P3LR
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00107e   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           
                                           func._Delay_ms	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x1000
                                           ;   STK00
                                           ;   r0x1001
                                           ;   r0x1002
                                           ;   r0x1003
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	26; "../main.c"	void Delay_ms(uint ms_data)
001024   e100     MOVB	0                   	BANKSEL	r0x1000
001025   5193     MOV	0x93, R0             	MOV	r0x1000, R0
                                           	BANKSEL	STK00
001026   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1001
001027   5192     MOV	0x92, R0             	MOV	r0x1001, R0
                                           ;	op : =
                                           ;	op : LABEL
                                           ;	op : =
                                           _00004_DS_
                                           ;	.line	29; "../main.c"	while(ms_data--)
                                           	BANKSEL	r0x1001
001028   0e92     MOVZ	R0, 0x92            	MOVZ	R0, r0x1001
                                           	BANKSEL	r0x1002
001029   5194     MOV	0x94, R0             	MOV	r0x1002, R0
                                           	BANKSEL	r0x1000
00102a   0e93     MOVZ	R0, 0x93            	MOVZ	R0, r0x1000
                                           	BANKSEL	r0x1003
00102b   5195     MOV	0x95, R0             	MOV	r0x1003, R0
                                           ;	op : -
00102c   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x1001
00102d   2192     ADD	0x92, R0             	ADD	r0x1001, R0
00102e   7003     JNB	0x3, 0               	JNB	PSW, 0
00102f   c031     JMP	#0x31                	JMP	_00030_DS_
                                           	BANKSEL	r0x1000
001030   0793     DEC	0x93                 	DEC	r0x1000
                                           ;	op : IFX
                                           _00030_DS_
                                           	BANKSEL	r0x1002
001031   0e94     MOVZ	R0, 0x94            	MOVZ	R0, r0x1002
                                           	BANKSEL	r0x1003
001032   3095     ORL	R0, 0x95             	ORL	R0, r0x1003
001033   7203     JNB	0x3, 2               	JNB	PSW, 2
001034   c03f     JMP	#0x3f                	JMP	_00007_DS_
                                           ;	op : =
                                           ;	.line	32; "../main.c"	while(i--);
001035   987c     MOV	R0, #0x7c            	MOV	R0,# 0x7c
                                           	BANKSEL	r0x1002
001036   5194     MOV	0x94, R0             	MOV	r0x1002, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00001_DS_
                                           	BANKSEL	r0x1002
001037   0e94     MOVZ	R0, 0x94            	MOVZ	R0, r0x1002
                                           	BANKSEL	r0x1003
001038   5195     MOV	0x95, R0             	MOV	r0x1003, R0
                                           ;	op : -
                                           	BANKSEL	r0x1002
001039   0794     DEC	0x94                 	DEC	r0x1002
                                           ;	op : IFX
00103a   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1003
00103b   3095     ORL	R0, 0x95             	ORL	R0, r0x1003
00103c   7203     JNB	0x3, 2               	JNB	PSW, 2
00103d   c028     JMP	#0x28                	JMP	_00004_DS_
                                           ;	op : GOTO
00103e   c037     JMP	#0x37                	JMP	_00001_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00007_DS_
00103f   0008     CRET                     	CRET	
                                           ; exit point of _Delay_ms
                                           
                                           
                                           ;	code size estimation:
                                           ;	   87+   43 =   130 instructions (  346 byte)
                                           
                                           
                                           	.end
                                           .config
002007   3fd4     SUB	0xd4, R3            
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
001091   e010     MOVP	0x10               
001092   d07f     CALL	#0x7f              
001093   e010     MOVP	0x10               
001094   0008     CRET                    
                                           .code
001000   e01f     MOVP	0x1f               
001001   e100     MOVB	0                  
001002   dfff     CALL	#0xfff             
001003   5130     MOV	0x30, R0            
001004   ffff     NOPZ                    
001005   ffff     NOPZ                    
001006   dffe     CALL	#0xffe             
001007   5137     MOV	0x37, R0            
001008   ffff     NOPZ                    
001009   ffff     NOPZ                    
00100a   dffd     CALL	#0xffd             
00100b   514c     MOV	0x4c, R0            
00100c   ffff     NOPZ                    
00100d   ffff     NOPZ                    
00100e   dffc     CALL	#0xffc             
00100f   514d     MOV	0x4d, R0            
001010   ffff     NOPZ                    
001011   ffff     NOPZ                    
001012   dffb     CALL	#0xffb             
001013   512a     MOV	0x2a, R0            
001014   ffff     NOPZ                    
001015   ffff     NOPZ                    
001016   e101     MOVB	0x1                
001017   dffa     CALL	#0xffa             
001018   5159     MOV	0x59, R0            
001019   ffff     NOPZ                    
00101a   ffff     NOPZ                    
00101b   dff9     CALL	#0xff9             
00101c   515a     MOV	0x5a, R0            
00101d   ffff     NOPZ                    
00101e   ffff     NOPZ                    
00101f   dff8     CALL	#0xff8             
001020   5165     MOV	0x65, R0            
001021   ffff     NOPZ                    
001022   ffff     NOPZ                    
001023   0008     CRET                    
                                           .cinit
00107f   e100     MOVB	0                  
001080   9880     MOV	R0, #0x80           
001081   9916     MOV	R1, #0x16           
001082   e010     MOVP	0x10               
001083   d085     CALL	#0x85              
001084   0008     CRET                    
001085   020a     CLR	R2                  
001086   f750     ST	[R0], R2             
001087   ff10     INC	R0                  
001088   ff59     DECJZ	R1                
001089   c086     JMP	#0x86               
00108a   0008     CRET                    
