gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 12-25-2015  14:49:22
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Sep 24 2015 15:22:16) (MSVC)
                                           ; This file was generated Fri Dec 25 14:49:21 2015
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x1f94
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Sep 24 2015 15:22:16) (MSVC)
                                           ; This file was generated Fri Dec 25 14:49:22 2015
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_ADCINTCTL_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWMPC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_ADCDATA1H
                                           	.extern	_ADCDATA1L
                                           	.extern	_PP5L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_ADCINTCTL
                                           	.extern	_ADCDATA2H
                                           	.extern	_ADCDATA2L
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_ADCDATA3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_ADCDATA3L
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWMPC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_init_mcu
                                           	.global	_led_init
                                           	.global	_Start_for_led
                                           	.global	_Stop_for_led
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           	.global	_L_1
                                           	.global	_L_2
                                           	.global	_L_3
                                           	.global	_L_4
                                           	.global	_timer
                                           	.global	_work_flag
                                           	.global	_ARR_List
                                           
                                           	.global I0R1
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_main_0	.udata
                                           _L_1	.res	1
                                           
                                           UD_main_1	.udata
                                           _L_2	.res	1
                                           
                                           UD_main_2	.udata
                                           _L_3	.res	1
                                           
                                           UD_main_3	.udata
                                           _L_4	.res	1
                                           
                                           UD_main_4	.udata
                                           _timer	.res	2
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1019	.res	1
                                           UDL_main_1	.udata
                                           r0x101A	.res	1
                                           UDL_main_2	.udata
                                           r0x101B	.res	1
                                           UDL_main_3	.udata
                                           r0x101C	.res	1
                                           UDL_main_4	.udata
                                           r0x101D	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           
                                           ID_main_0	.idata
                                           _work_flag
                                           	.db	0x01
                                           
                                           
                                           ID_main_1	.idata
                                           _ARR_List
                                           	.db	0xc0
                                           	.db	0xf9
                                           	.db	0xa4
                                           	.db	0xb0
                                           	.db	0x99
                                           	.db	0x92
                                           	.db	0x82
                                           	.db	0xf8
                                           	.db	0x80
                                           	.db	0x90
                                           	.db	0x88
                                           	.db	0x83
                                           	.db	0xa7
                                           	.db	0xa1
                                           	.db	0x86
                                           	.db	0x8e
                                           	.db	0xbf
                                           	.db	0xff
                                           
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e001     MOVP	0x1                 	PAGESEL	init_imp
000002   c145     JMP	#0x145               	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
000145   e000     MOVP	0                   	PAGESEL	_startup
000146   d0d6     CALL	#0xd6               	CALL	_startup
000147   e001     MOVP	0x1                 	PAGESEL	__sdcc_gsinit_startup
000148   d14b     CALL	#0x14b              	CALL	__sdcc_gsinit_startup
000149   e000     MOVP	0                   	PAGESEL	_main
00014a   c00f     JMP	#0xf                 	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           interrupt_0x04	.code	0x4
000004   f8c2     MOV	R2, R0               	MOV		R2,R0
000005   5617     MOV	R3, 0x17             	MOV		R3,BANK
000006   5003     MOV	R0, 0x3              	MOV		R0,PSW
000007   e100     MOVB	0                   	BANKSEL	I0PSW
000008   5181     MOV	0x81, R0             	MOV		I0PSW,R0
000009   500a     MOV	R0, 0xa              	MOV		R0,PCH
00000a   e100     MOVB	0                   	BANKSEL	I0PCH
00000b   5182     MOV	0x82, R0             	MOV		I0PCH,R0
00000c   5380     MOV	0x80, R1             	MOV		I0R1,R1
00000d   e000     MOVP	0                   	PAGESEL	interrupt_service_routine_0x04
00000e   c0a2     JMP	#0xa2                	JMP		interrupt_service_routine_0x04
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           ;	.line	187; "../main.c"	if(T0IF)
0000a2   e100     MOVB	0                   	BANKSEL	_INTCTL_bits
0000a3   7a0b     JB	0xb, 2                	JB	_INTCTL_bits, 2
0000a4   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           ;	op : =
                                           ;	.line	189; "../main.c"	T0IF=0;
                                           	BANKSEL	_INTCTL_bits
0000a5   620b     CLR	0xb, 2               	CLR	_INTCTL_bits, 2
                                           ;	op : =
                                           ;	.line	190; "../main.c"	T0=0x64;
0000a6   9864     MOV	R0, #0x64            	MOV	R0,# 0x64
                                           	BANKSEL	_T0
0000a7   5101     MOV	0x1, R0              	MOV	_T0, R0
                                           ;	op : +
                                           ;	.line	192; "../main.c"	timer++;
                                           	BANKSEL	_timer
0000a8   0ba4     INC	0xa4                 	INC	_timer
0000a9   7a03     JB	0x3, 2                	JB	PSW, 2
0000aa   c0ac     JMP	#0xac                	JMP	_00052_DS_
                                           	BANKSEL	_timer
0000ab   0ba5     INC	0xa5                 	INC	(_timer + 1)
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/3)
                                           ;unsigned compare: left >= lit(0x51=81), size=2
                                           _00052_DS_
                                           ;	.line	193; "../main.c"	if(timer>80)	// ¼Ó¿ìÂý¿ØÖÆ
0000ac   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	_timer
0000ad   38a5     SUB	R0, 0xa5             	SUB	R0, (_timer + 1)
                                           ;comparing bytes at offset 1
0000ae   7a03     JB	0x3, 2                	JB	PSW, 2
0000af   c0b2     JMP	#0xb2                	JMP	_00047_DS_
0000b0   9851     MOV	R0, #0x51            	MOV	R0,# 0x51
                                           	BANKSEL	_timer
0000b1   38a4     SUB	R0, 0xa4             	SUB	R0, _timer
                                           _00047_DS_
0000b2   7803     JB	0x3, 0                	JB	PSW, 0
0000b3   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           ;	op : =
                                           ;	.line	195; "../main.c"	timer=0;
                                           	BANKSEL	_timer
0000b4   03a4     CLR	0xa4                 	CLR	_timer
                                           	BANKSEL	_timer
0000b5   03a5     CLR	0xa5                 	CLR	(_timer + 1)
                                           ;	op : +
                                           ;	.line	197; "../main.c"	L_4++;
                                           	BANKSEL	_L_4
0000b6   0ba9     INC	0xa9                 	INC	_L_4
                                           ;	op : EQ_OP
                                           ;	.line	198; "../main.c"	if(L_4==10)
                                           	BANKSEL	_L_4
0000b7   0ea9     MOVZ	R0, 0xa9            	MOVZ	R0, _L_4
0000b8   a80a     XOR	R0, #0xa             	XOR	R0,# 0x0a
0000b9   7a03     JB	0x3, 2                	JB	PSW, 2
0000ba   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           ;	op : =
                                           ;	.line	200; "../main.c"	L_4=0;
                                           	BANKSEL	_L_4
0000bb   03a9     CLR	0xa9                 	CLR	_L_4
                                           ;	op : +
                                           ;	.line	201; "../main.c"	L_3++;
                                           	BANKSEL	_L_3
0000bc   0ba8     INC	0xa8                 	INC	_L_3
                                           ;	op : EQ_OP
                                           ;	.line	202; "../main.c"	if(L_3==10)
                                           	BANKSEL	_L_3
0000bd   0ea8     MOVZ	R0, 0xa8            	MOVZ	R0, _L_3
0000be   a80a     XOR	R0, #0xa             	XOR	R0,# 0x0a
0000bf   7a03     JB	0x3, 2                	JB	PSW, 2
0000c0   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           ;	op : =
                                           ;	.line	204; "../main.c"	L_3=0;
                                           	BANKSEL	_L_3
0000c1   03a8     CLR	0xa8                 	CLR	_L_3
                                           ;	op : +
                                           ;	.line	205; "../main.c"	L_2++;
                                           	BANKSEL	_L_2
0000c2   0ba7     INC	0xa7                 	INC	_L_2
                                           ;	op : EQ_OP
                                           ;	.line	206; "../main.c"	if(L_2==10)
                                           	BANKSEL	_L_2
0000c3   0ea7     MOVZ	R0, 0xa7            	MOVZ	R0, _L_2
0000c4   a80a     XOR	R0, #0xa             	XOR	R0,# 0x0a
0000c5   7a03     JB	0x3, 2                	JB	PSW, 2
0000c6   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           ;	op : =
                                           ;	.line	208; "../main.c"	L_2=0;
                                           	BANKSEL	_L_2
0000c7   03a7     CLR	0xa7                 	CLR	_L_2
                                           ;	op : +
                                           ;	.line	209; "../main.c"	L_1++;
                                           	BANKSEL	_L_1
0000c8   0ba6     INC	0xa6                 	INC	_L_1
                                           ;	op : EQ_OP
                                           ;	.line	210; "../main.c"	if(L_1==10)
                                           	BANKSEL	_L_1
0000c9   0ea6     MOVZ	R0, 0xa6            	MOVZ	R0, _L_1
                                           ;	.line	212; "../main.c"	L_1=0;
0000ca   a80a     XOR	R0, #0xa             	XOR	R0,# 0x0a
0000cb   7a03     JB	0x3, 2                	JB	PSW, 2
0000cc   c0ce     JMP	#0xce                	JMP	_00053_DS_
                                           	BANKSEL	_L_1
0000cd   03a6     CLR	0xa6                 	CLR	_L_1
                                           _00053_DS_
                                           	BANKSEL	I0R1
0000ce   5280     MOV	R1, 0x80             	MOV	R1, I0R1
                                           	BANKSEL	I0PCH
0000cf   5082     MOV	R0, 0x82             	MOV	R0, I0PCH
0000d0   510a     MOV	0xa, R0              	MOV	PCH, R0
                                           	BANKSEL	I0PSW
0000d1   5081     MOV	R0, 0x81             	MOV	R0, I0PSW
0000d2   5103     MOV	0x3, R0              	MOV	PSW, R0
0000d3   5717     MOV	0x17, R3             	MOV	BANK, R3
0000d4   f8d0     MOV	R0, R2               	MOV	R0, R2
0000d5   0009     IRET                     	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00048_DS_
                                           ;	.line	226; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _led_init
                                           ;   _Start_for_led
                                           ;   _Start_for_led
                                           ;   _Stop_for_led
                                           ;   _init_mcu
                                           ;   _led_init
                                           ;   _Start_for_led
                                           ;   _Start_for_led
                                           ;   _Stop_for_led
                                           ;5 compiler assigned registers:
                                           ;   r0x1019
                                           ;   r0x101A
                                           ;   r0x101B
                                           ;   r0x101C
                                           ;   r0x101D
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	146; "../main.c"	unsigned int timeA=0,timeB=0;
00000f   e100     MOVB	0                   	BANKSEL	r0x1019
000010   03aa     CLR	0xaa                 	CLR	r0x1019
                                           	BANKSEL	r0x101A
000011   03ab     CLR	0xab                 	CLR	r0x101A
                                           ;	op : =
                                           	BANKSEL	r0x101B
000012   03ac     CLR	0xac                 	CLR	r0x101B
                                           	BANKSEL	r0x101C
000013   03ad     CLR	0xad                 	CLR	r0x101C
                                           ;	op : CALL
                                           ;	.line	148; "../main.c"	init_mcu();
000014   e001     MOVP	0x1                 	PAGESEL	_init_mcu
000015   d12d     CALL	#0x12d              	CALL	_init_mcu
000016   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	149; "../main.c"	led_init();
000017   e000     MOVP	0                   	PAGESEL	_led_init
000018   d0fa     CALL	#0xfa               	CALL	_led_init
000019   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	150; "../main.c"	Start_for_led();// ÓÅÏÈLEDÏÔÊ¾
00001a   e001     MOVP	0x1                 	PAGESEL	_Start_for_led
00001b   d118     CALL	#0x118              	CALL	_Start_for_led
00001c   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : =
                                           ;	.line	151; "../main.c"	P1LR2=0;
00001d   e100     MOVB	0                   	BANKSEL	_P1LR_bits
00001e   6247     CLR	0x47, 2              	CLR	_P1LR_bits, 2
                                           ;	op : LABEL
                                           ;	op : +
                                           _00017_DS_
                                           ;	.line	154; "../main.c"	LEDDATA3=ARR_List[L_1];
                                           	BANKSEL	_L_1
00001f   50a6     MOV	R0, 0xa6             	MOV	R0, _L_1
000020   8092     ADD	R0, #0x92            	ADD	R0,# (_ARR_List + 0)
                                           	BANKSEL	r0x101D
000021   51ae     MOV	0xae, R0             	MOV	r0x101D, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x101D
000022   52ae     MOV	R1, 0xae             	MOV	R1, r0x101D
                                           	BANKSEL	_ARR_List
000023   f708     LD	R0, [R1]              	LD	R0, [R1]
000024   e101     MOVB	0x1                 	BANKSEL	_LEDDATA3
000025   5145     MOV	0x45, R0             	MOV	_LEDDATA3, R0
                                           ;	op : +
                                           ;	.line	155; "../main.c"	LEDDATA2=ARR_List[L_2];
000026   e100     MOVB	0                   	BANKSEL	_L_2
000027   50a7     MOV	R0, 0xa7             	MOV	R0, _L_2
000028   8092     ADD	R0, #0x92            	ADD	R0,# (_ARR_List + 0)
                                           	BANKSEL	r0x101D
000029   51ae     MOV	0xae, R0             	MOV	r0x101D, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x101D
00002a   52ae     MOV	R1, 0xae             	MOV	R1, r0x101D
                                           	BANKSEL	_ARR_List
00002b   f708     LD	R0, [R1]              	LD	R0, [R1]
00002c   e101     MOVB	0x1                 	BANKSEL	_LEDDATA2
00002d   5144     MOV	0x44, R0             	MOV	_LEDDATA2, R0
                                           ;	op : +
                                           ;	.line	156; "../main.c"	LEDDATA1=ARR_List[L_3];
00002e   e100     MOVB	0                   	BANKSEL	_L_3
00002f   50a8     MOV	R0, 0xa8             	MOV	R0, _L_3
000030   8092     ADD	R0, #0x92            	ADD	R0,# (_ARR_List + 0)
                                           	BANKSEL	r0x101D
000031   51ae     MOV	0xae, R0             	MOV	r0x101D, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x101D
000032   52ae     MOV	R1, 0xae             	MOV	R1, r0x101D
                                           	BANKSEL	_ARR_List
000033   f708     LD	R0, [R1]              	LD	R0, [R1]
000034   e101     MOVB	0x1                 	BANKSEL	_LEDDATA1
000035   5143     MOV	0x43, R0             	MOV	_LEDDATA1, R0
                                           ;	op : +
                                           ;	.line	157; "../main.c"	LEDDATA0=ARR_List[L_4];
000036   e100     MOVB	0                   	BANKSEL	_L_4
000037   50a9     MOV	R0, 0xa9             	MOV	R0, _L_4
000038   8092     ADD	R0, #0x92            	ADD	R0,# (_ARR_List + 0)
                                           	BANKSEL	r0x101D
000039   51ae     MOV	0xae, R0             	MOV	r0x101D, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           	BANKSEL	r0x101D
00003a   52ae     MOV	R1, 0xae             	MOV	R1, r0x101D
                                           	BANKSEL	_ARR_List
00003b   f708     LD	R0, [R1]              	LD	R0, [R1]
00003c   e101     MOVB	0x1                 	BANKSEL	_LEDDATA0
00003d   5142     MOV	0x42, R0             	MOV	_LEDDATA0, R0
                                           ;	op : +
                                           ;	.line	160; "../main.c"	timeA++;
00003e   e100     MOVB	0                   	BANKSEL	r0x1019
00003f   0baa     INC	0xaa                 	INC	r0x1019
000040   7a03     JB	0x3, 2                	JB	PSW, 2
000041   c043     JMP	#0x43                	JMP	_00050_DS_
                                           	BANKSEL	r0x101A
000042   0bab     INC	0xab                 	INC	r0x101A
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;unsigned compare: left >= lit(0x4E21=20001), size=2
                                           _00050_DS_
                                           ;	.line	161; "../main.c"	if(timeA>20000)
000043   984e     MOV	R0, #0x4e            	MOV	R0,# 0x4e
                                           	BANKSEL	r0x101A
000044   38ab     SUB	R0, 0xab             	SUB	R0, r0x101A
                                           ;comparing bytes at offset 1
000045   7a03     JB	0x3, 2                	JB	PSW, 2
000046   c049     JMP	#0x49                	JMP	_00025_DS_
000047   9821     MOV	R0, #0x21            	MOV	R0,# 0x21
                                           	BANKSEL	r0x1019
000048   38aa     SUB	R0, 0xaa             	SUB	R0, r0x1019
                                           _00025_DS_
000049   7803     JB	0x3, 0                	JB	PSW, 0
00004a   c01f     JMP	#0x1f                	JMP	_00017_DS_
                                           ;	op : =
                                           ;	.line	163; "../main.c"	timeA=0;
                                           	BANKSEL	r0x1019
00004b   03aa     CLR	0xaa                 	CLR	r0x1019
                                           	BANKSEL	r0x101A
00004c   03ab     CLR	0xab                 	CLR	r0x101A
                                           ;	op : +
                                           ;	.line	164; "../main.c"	timeB++;
                                           	BANKSEL	r0x101B
00004d   0bac     INC	0xac                 	INC	r0x101B
00004e   7a03     JB	0x3, 2                	JB	PSW, 2
00004f   c051     JMP	#0x51                	JMP	_00051_DS_
                                           	BANKSEL	r0x101C
000050   0bad     INC	0xad                 	INC	r0x101C
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;unsigned compare: left >= lit(0x6=6), size=2
                                           _00051_DS_
                                           ;	.line	165; "../main.c"	if(timeB>5)
000051   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x101C
000052   38ad     SUB	R0, 0xad             	SUB	R0, r0x101C
                                           ;comparing bytes at offset 1
000053   7a03     JB	0x3, 2                	JB	PSW, 2
000054   c057     JMP	#0x57                	JMP	_00026_DS_
000055   9806     MOV	R0, #0x6             	MOV	R0,# 0x06
                                           	BANKSEL	r0x101B
000056   38ac     SUB	R0, 0xac             	SUB	R0, r0x101B
                                           _00026_DS_
000057   7803     JB	0x3, 0                	JB	PSW, 0
000058   c01f     JMP	#0x1f                	JMP	_00017_DS_
                                           ;	op : =
                                           ;	.line	167; "../main.c"	timeB=0;
                                           	BANKSEL	r0x101B
000059   03ac     CLR	0xac                 	CLR	r0x101B
                                           	BANKSEL	r0x101C
00005a   03ad     CLR	0xad                 	CLR	r0x101C
                                           ;	op : IFX
                                           ;	.line	168; "../main.c"	if(!work_flag)
00005b   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	_work_flag
00005c   30af     ORL	R0, 0xaf             	ORL	R0, _work_flag
00005d   7a03     JB	0x3, 2                	JB	PSW, 2
00005e   c065     JMP	#0x65                	JMP	_00010_DS_
                                           ;	op : CALL
                                           ;	.line	170; "../main.c"	Start_for_led();
00005f   e001     MOVP	0x1                 	PAGESEL	_Start_for_led
000060   d118     CALL	#0x118              	CALL	_Start_for_led
000061   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : =
                                           ;	.line	171; "../main.c"	P1LR2=0;
000062   e100     MOVB	0                   	BANKSEL	_P1LR_bits
000063   6247     CLR	0x47, 2              	CLR	_P1LR_bits, 2
                                           ;	op : GOTO
000064   c01f     JMP	#0x1f                	JMP	_00017_DS_
                                           ;	op : LABEL
                                           ;	op : CALL
                                           _00010_DS_
                                           ;	.line	175; "../main.c"	Stop_for_led();
000065   e001     MOVP	0x1                 	PAGESEL	_Stop_for_led
000066   d13e     CALL	#0x13e              	CALL	_Stop_for_led
000067   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : =
                                           ;	.line	176; "../main.c"	P1LR2=1;
000068   e100     MOVB	0                   	BANKSEL	_P1LR_bits
000069   6a47     SET	0x47, 2              	SET	_P1LR_bits, 2
                                           ;	op : GOTO
00006a   c01f     JMP	#0x1f                	JMP	_00017_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00006b   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._Stop_for_led	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Stop_for_led	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Stop_for_led	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	139; "../main.c"	T0IE=0;
00013e   e100     MOVB	0                   	BANKSEL	_INTCTL_bits
00013f   650b     CLR	0xb, 5               	CLR	_INTCTL_bits, 5
                                           ;	op : =
                                           ;	.line	140; "../main.c"	LEDCTL=0x00;
000140   e101     MOVB	0x1                 	BANKSEL	_LEDCTL
000141   0340     CLR	0x40                 	CLR	_LEDCTL
                                           ;	op : =
                                           ;	.line	141; "../main.c"	work_flag=0;
000142   e100     MOVB	0                   	BANKSEL	_work_flag
000143   03af     CLR	0xaf                 	CLR	_work_flag
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000144   0008     CRET                     	CRET	
                                           ; exit point of _Stop_for_led
                                           
                                           
                                           
                                           func._Start_for_led	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Start_for_led	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Start_for_led	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	119; "../main.c"	L_1=9;
000118   9809     MOV	R0, #0x9             	MOV	R0,# 0x09
000119   e100     MOVB	0                   	BANKSEL	_L_1
00011a   51a6     MOV	0xa6, R0             	MOV	_L_1, R0
                                           ;	op : =
                                           ;	.line	120; "../main.c"	L_2=9;
00011b   9809     MOV	R0, #0x9             	MOV	R0,# 0x09
                                           	BANKSEL	_L_2
00011c   51a7     MOV	0xa7, R0             	MOV	_L_2, R0
                                           ;	op : =
                                           ;	.line	121; "../main.c"	L_3=8;
00011d   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	_L_3
00011e   51a8     MOV	0xa8, R0             	MOV	_L_3, R0
                                           ;	op : =
                                           ;	.line	122; "../main.c"	L_4=7;
00011f   9807     MOV	R0, #0x7             	MOV	R0,# 0x07
                                           	BANKSEL	_L_4
000120   51a9     MOV	0xa9, R0             	MOV	_L_4, R0
                                           ;	op : =
                                           ;	.line	123; "../main.c"	timer=0;
                                           	BANKSEL	_timer
000121   03a4     CLR	0xa4                 	CLR	_timer
                                           	BANKSEL	_timer
000122   03a5     CLR	0xa5                 	CLR	(_timer + 1)
                                           ;	op : =
                                           ;	.line	125; "../main.c"	LEDCTL=LED_WORK_MODE;
000123   988c     MOV	R0, #0x8c            	MOV	R0,# 0x8c
000124   e101     MOVB	0x1                 	BANKSEL	_LEDCTL
000125   5140     MOV	0x40, R0             	MOV	_LEDCTL, R0
                                           ;	op : =
                                           ;	.line	127; "../main.c"	T0=0x64;
000126   9864     MOV	R0, #0x64            	MOV	R0,# 0x64
000127   e100     MOVB	0                   	BANKSEL	_T0
000128   5101     MOV	0x1, R0              	MOV	_T0, R0
                                           ;	op : =
                                           ;	.line	128; "../main.c"	T0IE=1;
                                           	BANKSEL	_INTCTL_bits
000129   6d0b     SET	0xb, 5               	SET	_INTCTL_bits, 5
                                           ;	op : =
                                           ;	.line	129; "../main.c"	work_flag=1;
00012a   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_work_flag
00012b   51af     MOV	0xaf, R0             	MOV	_work_flag, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00012c   0008     CRET                     	CRET	
                                           ; exit point of _Start_for_led
                                           
                                           
                                           
                                           func._led_init	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _led_init	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _led_init	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	87; "../main.c"	LEDOMS0=0x00;			//LED-COMx¶ËÊä³öÄ£Ê½ÉèÖÃÎ»
0000fa   e101     MOVB	0x1                 	BANKSEL	_LEDOMS0
0000fb   0357     CLR	0x57                 	CLR	_LEDOMS0
                                           ;	op : =
                                           ;	.line	88; "../main.c"	LEDOMS1=0x00;			//LED-SEGx¶ËÊä³öÄ£Ê½ÉèÖÃÎ»
                                           	BANKSEL	_LEDOMS1
0000fc   0350     CLR	0x50                 	CLR	_LEDOMS1
                                           ;	op : =
                                           ;	.line	90; "../main.c"	LEDODS0=0xFF;			//LED-COMx¶Ë¿ªÂ©·½Ê½Ñ¡ÔñÎ»
0000fd   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	_LEDODS0
0000fe   5155     MOV	0x55, R0             	MOV	_LEDODS0, R0
                                           ;	op : =
                                           ;	.line	91; "../main.c"	LEDODS1=0xFF;			//LED-SEGx¶Ë¿ªÂ©·½Ê½Ñ¡ÔñÎ»
0000ff   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	_LEDODS1
000100   5158     MOV	0x58, R0             	MOV	_LEDODS1, R0
                                           ;	op : =
                                           ;	.line	94; "../main.c"	LEDLUM=0x01;
000101   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
                                           	BANKSEL	_LEDLUM
000102   515c     MOV	0x5c, R0             	MOV	_LEDLUM, R0
                                           ;	op : =
                                           ;	.line	100; "../main.c"	LEDPRE=0x72;
000103   9872     MOV	R0, #0x72            	MOV	R0,# 0x72
                                           	BANKSEL	_LEDPRE
000104   5141     MOV	0x41, R0             	MOV	_LEDPRE, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	102; "../main.c"	LEDDATA3=ARR_List[10];								//Ç§Î»
000105   e100     MOVB	0                   	BANKSEL	_ARR_List
000106   0e9c     MOVZ	R0, 0x9c            	MOVZ	R0,  (_ARR_List + 10)
000107   e101     MOVB	0x1                 	BANKSEL	_LEDDATA3
000108   5145     MOV	0x45, R0             	MOV	_LEDDATA3, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	103; "../main.c"	LEDDATA2=ARR_List[11];		 						//°ÙÎ»
000109   e100     MOVB	0                   	BANKSEL	_ARR_List
00010a   0e9d     MOVZ	R0, 0x9d            	MOVZ	R0,  (_ARR_List + 11)
00010b   e101     MOVB	0x1                 	BANKSEL	_LEDDATA2
00010c   5144     MOV	0x44, R0             	MOV	_LEDDATA2, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	104; "../main.c"	LEDDATA1=ARR_List[12];					 			//Ê®Î»
00010d   e100     MOVB	0                   	BANKSEL	_ARR_List
00010e   0e9e     MOVZ	R0, 0x9e            	MOVZ	R0,  (_ARR_List + 12)
00010f   e101     MOVB	0x1                 	BANKSEL	_LEDDATA1
000110   5143     MOV	0x43, R0             	MOV	_LEDDATA1, R0
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	.line	105; "../main.c"	LEDDATA0=ARR_List[13];  //   0 ÁÁ 1Ãð£¬Óë¹²Òõ¹²ÑôÎÞ¹Ø 	//¸öÎ»
000111   e100     MOVB	0                   	BANKSEL	_ARR_List
000112   0e9f     MOVZ	R0, 0x9f            	MOVZ	R0,  (_ARR_List + 13)
000113   e101     MOVB	0x1                 	BANKSEL	_LEDDATA0
000114   5142     MOV	0x42, R0             	MOV	_LEDDATA0, R0
                                           ;	op : =
                                           ;	.line	107; "../main.c"	LEDCTL=LED_WORK_MODE;  // Ä¬ÈÏ¿ªÆô ÏÔÊ¾  ABCD
000115   988c     MOV	R0, #0x8c            	MOV	R0,# 0x8c
                                           	BANKSEL	_LEDCTL
000116   5140     MOV	0x40, R0             	MOV	_LEDCTL, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000117   0008     CRET                     	CRET	
                                           ; exit point of _led_init
                                           
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	61; "../main.c"	OSCCTL = 0x60;           //8M
00012d   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
00012e   e100     MOVB	0                   	BANKSEL	_OSCCTL
00012f   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	64; "../main.c"	TR0 = 0x04;
000130   9804     MOV	R0, #0x4             	MOV	R0,# 0x04
                                           	BANKSEL	_TR0
000131   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	65; "../main.c"	TR1 = 0x00;
                                           	BANKSEL	_TR1
000132   0327     CLR	0x27                 	CLR	_TR1
                                           ;	op : =
                                           ;	.line	66; "../main.c"	TR2 = 0x00;
                                           	BANKSEL	_TR2
000133   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	67; "../main.c"	TR3 = 0x00;  	// LEDÊä³ö
                                           	BANKSEL	_TR3
000134   0349     CLR	0x49                 	CLR	_TR3
                                           ;	op : =
                                           ;	.line	69; "../main.c"	P0LR = 0X1B;	// COM ¶Ë¸ßµçÆ½
000135   981b     MOV	R0, #0x1b            	MOV	R0,# 0x1b
                                           	BANKSEL	_P0LR
000136   5145     MOV	0x45, R0             	MOV	_P0LR, R0
                                           ;	op : =
                                           ;	.line	70; "../main.c"	P1LR = 0X00;
                                           	BANKSEL	_P1LR
000137   0347     CLR	0x47                 	CLR	_P1LR
                                           ;	op : =
                                           ;	.line	71; "../main.c"	P2LR = 0X00;
                                           	BANKSEL	_P2LR
000138   0346     CLR	0x46                 	CLR	_P2LR
                                           ;	op : =
                                           ;	.line	72; "../main.c"	P3LR = 0X00;
                                           	BANKSEL	_P3LR
000139   0348     CLR	0x48                 	CLR	_P3LR
                                           ;	op : =
                                           ;	.line	74; "../main.c"	OPTR=0x44;		//Ê¹ÄÜÉÏÀ­£¬T0¼ÆÊ±Ä£Ê½£¬µÈ´ýÆô¶¯
00013a   9844     MOV	R0, #0x44            	MOV	R0,# 0x44
                                           	BANKSEL	_OPTR
00013b   5121     MOV	0x21, R0             	MOV	_OPTR, R0
                                           ;	op : =
                                           ;	.line	76; "../main.c"	AIE=1;
                                           	BANKSEL	_INTCTL_bits
00013c   6f0b     SET	0xb, 7               	SET	_INTCTL_bits, 7
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00013d   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           ;	code size estimation:
                                           ;	  192+  103 =   295 instructions (  796 byte)
                                           
                                           
                                           	.end
                                           .config
002007   1f94     XOR	0x94, R3            
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
00014b   e000     MOVP	0                  
00014c   d06c     CALL	#0x6c              
00014d   e001     MOVP	0x1                
00014e   0008     CRET                    
                                           .code
0000d6   e01f     MOVP	0x1f               
0000d7   e100     MOVB	0                  
0000d8   dfff     CALL	#0xfff             
0000d9   5130     MOV	0x30, R0            
0000da   ffff     NOPZ                    
0000db   ffff     NOPZ                    
0000dc   dffe     CALL	#0xffe             
0000dd   5137     MOV	0x37, R0            
0000de   ffff     NOPZ                    
0000df   ffff     NOPZ                    
0000e0   dffd     CALL	#0xffd             
0000e1   514c     MOV	0x4c, R0            
0000e2   ffff     NOPZ                    
0000e3   ffff     NOPZ                    
0000e4   dffc     CALL	#0xffc             
0000e5   514d     MOV	0x4d, R0            
0000e6   ffff     NOPZ                    
0000e7   ffff     NOPZ                    
0000e8   dffb     CALL	#0xffb             
0000e9   512a     MOV	0x2a, R0            
0000ea   ffff     NOPZ                    
0000eb   ffff     NOPZ                    
0000ec   e101     MOVB	0x1                
0000ed   dffa     CALL	#0xffa             
0000ee   5159     MOV	0x59, R0            
0000ef   ffff     NOPZ                    
0000f0   ffff     NOPZ                    
0000f1   dff9     CALL	#0xff9             
0000f2   515a     MOV	0x5a, R0            
0000f3   ffff     NOPZ                    
0000f4   ffff     NOPZ                    
0000f5   dff8     CALL	#0xff8             
0000f6   5165     MOV	0x65, R0            
0000f7   ffff     NOPZ                    
0000f8   ffff     NOPZ                    
0000f9   0008     CRET                    
                                           .cinit
00006c   e100     MOVB	0                  
00006d   9880     MOV	R0, #0x80           
00006e   9912     MOV	R1, #0x12           
00006f   e000     MOVP	0                  
000070   d09c     CALL	#0x9c              
000071   98c0     MOV	R0, #0xc0           
000072   5192     MOV	0x92, R0            
000073   98a4     MOV	R0, #0xa4           
000074   990b     MOV	R1, #0xb            
000075   e000     MOVP	0                  
000076   d09c     CALL	#0x9c              
000077   98f9     MOV	R0, #0xf9           
000078   5193     MOV	0x93, R0            
000079   98a4     MOV	R0, #0xa4           
00007a   5194     MOV	0x94, R0            
00007b   98b0     MOV	R0, #0xb0           
00007c   5195     MOV	0x95, R0            
00007d   9899     MOV	R0, #0x99           
00007e   5196     MOV	0x96, R0            
00007f   9892     MOV	R0, #0x92           
000080   5197     MOV	0x97, R0            
000081   9882     MOV	R0, #0x82           
000082   5198     MOV	0x98, R0            
000083   98f8     MOV	R0, #0xf8           
000084   5199     MOV	0x99, R0            
000085   9880     MOV	R0, #0x80           
000086   519a     MOV	0x9a, R0            
000087   9890     MOV	R0, #0x90           
000088   519b     MOV	0x9b, R0            
000089   9888     MOV	R0, #0x88           
00008a   519c     MOV	0x9c, R0            
00008b   9883     MOV	R0, #0x83           
00008c   519d     MOV	0x9d, R0            
00008d   98a7     MOV	R0, #0xa7           
00008e   519e     MOV	0x9e, R0            
00008f   98a1     MOV	R0, #0xa1           
000090   519f     MOV	0x9f, R0            
000091   9886     MOV	R0, #0x86           
000092   51a0     MOV	0xa0, R0            
000093   988e     MOV	R0, #0x8e           
000094   51a1     MOV	0xa1, R0            
000095   98bf     MOV	R0, #0xbf           
000096   51a2     MOV	0xa2, R0            
000097   98ff     MOV	R0, #0xff           
000098   51a3     MOV	0xa3, R0            
000099   9801     MOV	R0, #0x1            
00009a   51af     MOV	0xaf, R0            
00009b   0008     CRET                    
00009c   020a     CLR	R2                  
00009d   f750     ST	[R0], R2             
00009e   ff10     INC	R0                  
00009f   ff59     DECJZ	R1                
0000a0   c09d     JMP	#0x9d               
0000a1   0008     CRET                    
