gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 5-29-2016  19:48:38
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Sun May 29 19:48:32 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x5c4
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Sun May 29 19:48:35 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_ADCINTCTL_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWMPC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_ADCDATA1H
                                           	.extern	_ADCDATA1L
                                           	.extern	_PP5L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_ADCINTCTL
                                           	.extern	_ADCDATA2H
                                           	.extern	_ADCDATA2L
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_ADCDATA3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_ADCDATA3L
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWMPC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_FLASH_WRITE_ONE
                                           	.global	_FLASH_WRITE_FUN
                                           	.global	_FLASH_READ_FUN
                                           	.global	_FLASH_READ_ONE
                                           	.global	_init_mcu
                                           	.global	_main
                                           	.global	_FLASH_BUFFER
                                           	.global	_FLASH_READ_BUF
                                           
                                           	.global I0R1
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_main_0	.udata
                                           _FLASH_BUFFER	.res	64
                                           
                                           UD_main_1	.udata
                                           _FLASH_READ_BUF	.res	2
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1053	.res	1
                                           UDL_main_1	.udata
                                           r0x1054	.res	1
                                           UDL_main_2	.udata
                                           r0x1055	.res	1
                                           UDL_main_3	.udata
                                           r0x1056	.res	1
                                           UDL_main_4	.udata
                                           r0x1050	.res	1
                                           UDL_main_5	.udata
                                           r0x1051	.res	1
                                           UDL_main_6	.udata
                                           r0x1043	.res	1
                                           UDL_main_7	.udata
                                           r0x1042	.res	1
                                           UDL_main_8	.udata
                                           r0x1044	.res	1
                                           UDL_main_9	.udata
                                           r0x1048	.res	1
                                           UDL_main_10	.udata
                                           r0x1047	.res	1
                                           UDL_main_11	.udata
                                           r0x104A	.res	1
                                           UDL_main_12	.udata
                                           r0x1049	.res	1
                                           UDL_main_13	.udata
                                           r0x104B	.res	1
                                           UDL_main_14	.udata
                                           r0x104C	.res	1
                                           UDL_main_15	.udata
                                           r0x104D	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e010     MOVP	0x10                	PAGESEL	init_imp
000002   c068     JMP	#0x68                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
001068   e01f     MOVP	0x1f                	PAGESEL	_startup
001069   dfd2     CALL	#0xfd2              	CALL	_startup
00106a   e010     MOVP	0x10                	PAGESEL	__sdcc_gsinit_startup
00106b   d06e     CALL	#0x6e               	CALL	__sdcc_gsinit_startup
00106c   e01e     MOVP	0x1e                	PAGESEL	_main
00106d   cee0     JMP	#0xee0               	JMP		_main
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_ONE
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_ONE
                                           ;   _init_mcu
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_ONE
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_WRITE_ONE
                                           ;7 compiler assigned registers:
                                           ;   r0x1053
                                           ;   r0x1054
                                           ;   r0x1055
                                           ;   r0x1056
                                           ;   STK01
                                           ;   STK00
                                           ;   STK02
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	56; "../main.c"	init_mcu();
001ee0   e010     MOVP	0x10                	PAGESEL	_init_mcu
001ee1   d04f     CALL	#0x4f               	CALL	_init_mcu
001ee2   e01e     MOVP	0x1e                	PAGESEL	$
                                           ;	op : =
                                           ;	.line	58; "../main.c"	for (i = 0; i < FLASH_BUFFER_MAX; i++)
001ee3   e100     MOVB	0                   	BANKSEL	r0x1053
001ee4   03d4     CLR	0xd4                 	CLR	r0x1053
                                           	BANKSEL	r0x1054
001ee5   03d5     CLR	0xd5                 	CLR	r0x1054
                                           ;	op : =
                                           	BANKSEL	r0x1055
001ee6   03d6     CLR	0xd6                 	CLR	r0x1055
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x20=32), size=1
                                           _00008_DS_
001ee7   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
                                           	BANKSEL	r0x1055
001ee8   38d6     SUB	R0, 0xd6             	SUB	R0, r0x1055
                                           ;comparing bytes at offset 0
001ee9   7003     JNB	0x3, 0               	JNB	PSW, 0
001eea   cefe     JMP	#0xefe               	JMP	_00011_DS_
                                           ;	op : LEFT_OP
                                           ;	.line	60; "../main.c"	FLASH_BUFFER[i] = temp;
001eeb   6003     CLR	0x3, 0               	CLR	PSW, 0
                                           	BANKSEL	r0x1055
001eec   12d6     RLCR	0xd6                	RLCR	r0x1055
                                           	BANKSEL	r0x1056
001eed   51d7     MOV	0xd7, R0             	MOV	r0x1056, R0
                                           ;	op : +
001eee   9892     MOV	R0, #0x92            	MOV	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x1056
001eef   21d7     ADD	0xd7, R0             	ADD	r0x1056, R0
                                           ;	op : =
                                           	BANKSEL	r0x1053
001ef0   0ed4     MOVZ	R0, 0xd4            	MOVZ	R0, r0x1053
                                           	BANKSEL	r0x1056
001ef1   52d7     MOV	R1, 0xd7             	MOV	R1, r0x1056
                                           	BANKSEL	_FLASH_BUFFER
001ef2   f741     ST	[R1], R0              	ST	[R1], R0
001ef3   ff11     INC	R1                   	INC	R1
                                           	BANKSEL	r0x1054
001ef4   0ed5     MOVZ	R0, 0xd5            	MOVZ	R0, r0x1054
                                           	BANKSEL	_FLASH_BUFFER
001ef5   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	op : +
                                           ;	.line	61; "../main.c"	temp += 0x1111;
001ef6   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
                                           	BANKSEL	r0x1053
001ef7   21d4     ADD	0xd4, R0             	ADD	r0x1053, R0
001ef8   9811     MOV	R0, #0x11            	MOV	R0,# 0x11
001ef9   7003     JNB	0x3, 0               	JNB	PSW, 0
001efa   9812     MOV	R0, #0x12            	MOV	R0,# 0x12
                                           	BANKSEL	r0x1054
001efb   21d5     ADD	0xd5, R0             	ADD	r0x1054, R0
                                           ;	op : +
                                           ;	.line	58; "../main.c"	for (i = 0; i < FLASH_BUFFER_MAX; i++)
                                           	BANKSEL	r0x1055
001efc   0bd6     INC	0xd6                 	INC	r0x1055
                                           ;	op : GOTO
001efd   cee7     JMP	#0xee7               	JMP	_00008_DS_
                                           ;	op : LABEL
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
                                           _00011_DS_
                                           ;	.line	65; "../main.c"	FLASH_WRITE_FUN(0x1E60,FLASH_BUFFER_MAX);
001efe   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
                                           	BANKSEL	STK01
001eff   5190     MOV	0x90, R0             	MOV	STK01, R0
001f00   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
001f01   5191     MOV	0x91, R0             	MOV	STK00, R0
001f02   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f03   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_FUN
001f04   df66     CALL	#0xf66              	CALL	_FLASH_WRITE_FUN
001f05   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	66; "../main.c"	FLASH_WRITE_FUN(0x1E80,FLASH_BUFFER_MAX);
001f06   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
001f07   e100     MOVB	0                   	BANKSEL	STK01
001f08   5190     MOV	0x90, R0             	MOV	STK01, R0
001f09   9880     MOV	R0, #0x80            	MOV	R0,# 0x80
001f0a   5191     MOV	0x91, R0             	MOV	STK00, R0
001f0b   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f0c   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_FUN
001f0d   df66     CALL	#0xf66              	CALL	_FLASH_WRITE_FUN
001f0e   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	71; "../main.c"	temp=FLASH_READ_ONE(0x1E71);
001f0f   9871     MOV	R0, #0x71            	MOV	R0,# 0x71
001f10   e100     MOVB	0                   	BANKSEL	STK00
001f11   5191     MOV	0x91, R0             	MOV	STK00, R0
001f12   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f13   e010     MOVP	0x10                	PAGESEL	_FLASH_READ_ONE
001f14   d02f     CALL	#0x2f               	CALL	_FLASH_READ_ONE
001f15   e01f     MOVP	0x1f                	PAGESEL	$
001f16   e100     MOVB	0                   	BANKSEL	r0x1054
001f17   51d5     MOV	0xd5, R0             	MOV	r0x1054, R0
                                           	BANKSEL	STK00
001f18   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1053
001f19   51d4     MOV	0xd4, R0             	MOV	r0x1053, R0
                                           ;	op : =
                                           ;	.line	73; "../main.c"	for (i = 0; i < 16; i++)
                                           	BANKSEL	r0x1055
001f1a   03d6     CLR	0xd6                 	CLR	r0x1055
                                           ;	op : LABEL
                                           ;	op : <
                                           ;unsigned compare: left < lit(0x10=16), size=1
                                           _00012_DS_
001f1b   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	r0x1055
001f1c   38d6     SUB	R0, 0xd6             	SUB	R0, r0x1055
                                           ;comparing bytes at offset 0
001f1d   7003     JNB	0x3, 0               	JNB	PSW, 0
001f1e   cf2c     JMP	#0xf2c               	JMP	_00015_DS_
                                           ;	op : LEFT_OP
                                           ;	.line	75; "../main.c"	FLASH_BUFFER[i] = 0x0000;
001f1f   6003     CLR	0x3, 0               	CLR	PSW, 0
                                           	BANKSEL	r0x1055
001f20   12d6     RLCR	0xd6                	RLCR	r0x1055
                                           	BANKSEL	r0x1056
001f21   51d7     MOV	0xd7, R0             	MOV	r0x1056, R0
                                           ;	op : +
001f22   9892     MOV	R0, #0x92            	MOV	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x1056
001f23   21d7     ADD	0xd7, R0             	ADD	r0x1056, R0
                                           ;	op : =
001f24   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1056
001f25   52d7     MOV	R1, 0xd7             	MOV	R1, r0x1056
                                           	BANKSEL	_FLASH_BUFFER
001f26   f741     ST	[R1], R0              	ST	[R1], R0
001f27   ff11     INC	R1                   	INC	R1
001f28   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	_FLASH_BUFFER
001f29   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	op : +
                                           ;	.line	73; "../main.c"	for (i = 0; i < 16; i++)
                                           	BANKSEL	r0x1055
001f2a   0bd6     INC	0xd6                 	INC	r0x1055
                                           ;	op : GOTO
001f2b   cf1b     JMP	#0xf1b               	JMP	_00012_DS_
                                           ;	op : LABEL
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
                                           _00015_DS_
                                           ;	.line	78; "../main.c"	FLASH_WRITE_FUN(0x1EA0,16);
001f2c   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
001f2d   5190     MOV	0x90, R0             	MOV	STK01, R0
001f2e   98a0     MOV	R0, #0xa0            	MOV	R0,# 0xa0
001f2f   5191     MOV	0x91, R0             	MOV	STK00, R0
001f30   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f31   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_FUN
001f32   df66     CALL	#0xf66              	CALL	_FLASH_WRITE_FUN
001f33   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : =
                                           ;d:\svn\workspace\compiler\chipon16target\gen.c:8828: size=0/2, offset=0, AOP_TYPE(res)=7
                                           ;	.line	80; "../main.c"	FLASH_BUFFER[5]=temp;
001f34   e100     MOVB	0                   	BANKSEL	r0x1053
001f35   0ed4     MOVZ	R0, 0xd4            	MOVZ	R0, r0x1053
                                           	BANKSEL	_FLASH_BUFFER
001f36   519c     MOV	0x9c, R0             	MOV	 (_FLASH_BUFFER + 10), R0
                                           ;d:\svn\workspace\compiler\chipon16target\gen.c:8828: size=1/2, offset=1, AOP_TYPE(res)=7
                                           	BANKSEL	r0x1054
001f37   0ed5     MOVZ	R0, 0xd5            	MOVZ	R0, r0x1054
                                           	BANKSEL	_FLASH_BUFFER
001f38   519d     MOV	0x9d, R0             	MOV	 (_FLASH_BUFFER + 11), R0
                                           ;	op : =
                                           ;d:\svn\workspace\compiler\chipon16target\gen.c:8828: size=0/2, offset=0, AOP_TYPE(res)=7
                                           ;	.line	81; "../main.c"	FLASH_BUFFER[6]=0xFF33; //ÑéÖ¤ ÓÃ 0x1FB6
001f39   9833     MOV	R0, #0x33            	MOV	R0,# 0x33
                                           	BANKSEL	_FLASH_BUFFER
001f3a   519e     MOV	0x9e, R0             	MOV	 (_FLASH_BUFFER + 12), R0
                                           ;d:\svn\workspace\compiler\chipon16target\gen.c:8828: size=1/2, offset=1, AOP_TYPE(res)=7
001f3b   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	_FLASH_BUFFER
001f3c   519f     MOV	0x9f, R0             	MOV	 (_FLASH_BUFFER + 13), R0
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	83; "../main.c"	FLASH_WRITE_FUN(0x1EB0,16);
001f3d   9810     MOV	R0, #0x10            	MOV	R0,# 0x10
                                           	BANKSEL	STK01
001f3e   5190     MOV	0x90, R0             	MOV	STK01, R0
001f3f   98b0     MOV	R0, #0xb0            	MOV	R0,# 0xb0
001f40   5191     MOV	0x91, R0             	MOV	STK00, R0
001f41   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f42   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_FUN
001f43   df66     CALL	#0xf66              	CALL	_FLASH_WRITE_FUN
001f44   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	88; "../main.c"	FLASH_WRITE_ONE(0x1E69,0x55AA);
001f45   98aa     MOV	R0, #0xaa            	MOV	R0,# 0xaa
001f46   e100     MOVB	0                   	BANKSEL	STK02
001f47   518f     MOV	0x8f, R0             	MOV	STK02, R0
001f48   9855     MOV	R0, #0x55            	MOV	R0,# 0x55
001f49   5190     MOV	0x90, R0             	MOV	STK01, R0
001f4a   9869     MOV	R0, #0x69            	MOV	R0,# 0x69
001f4b   5191     MOV	0x91, R0             	MOV	STK00, R0
001f4c   981e     MOV	R0, #0x1e            	MOV	R0,# 0x1e
001f4d   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_ONE
001f4e   dfa1     CALL	#0xfa1              	CALL	_FLASH_WRITE_ONE
001f4f   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : +
                                           _00006_DS_
                                           ;	.line	99; "../main.c"	temp++;
001f50   e100     MOVB	0                   	BANKSEL	r0x1053
001f51   0bd4     INC	0xd4                 	INC	r0x1053
001f52   7a03     JB	0x3, 2                	JB	PSW, 2
001f53   cf55     JMP	#0xf55               	JMP	_00051_DS_
                                           	BANKSEL	r0x1054
001f54   0bd5     INC	0xd5                 	INC	r0x1054
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/2)
                                           ;unsigned compare: left >= lit(0x7531=30001), size=2
                                           _00051_DS_
                                           ;	.line	100; "../main.c"	if(temp>30000)
001f55   9875     MOV	R0, #0x75            	MOV	R0,# 0x75
                                           	BANKSEL	r0x1054
001f56   38d5     SUB	R0, 0xd5             	SUB	R0, r0x1054
                                           ;comparing bytes at offset 1
001f57   7a03     JB	0x3, 2                	JB	PSW, 2
001f58   cf5b     JMP	#0xf5b               	JMP	_00028_DS_
001f59   9831     MOV	R0, #0x31            	MOV	R0,# 0x31
                                           	BANKSEL	r0x1053
001f5a   38d4     SUB	R0, 0xd4             	SUB	R0, r0x1053
                                           _00028_DS_
001f5b   7803     JB	0x3, 0                	JB	PSW, 0
001f5c   cf50     JMP	#0xf50               	JMP	_00006_DS_
                                           ;	op : =
                                           ;	.line	102; "../main.c"	temp=0;
                                           	BANKSEL	r0x1053
001f5d   03d4     CLR	0xd4                 	CLR	r0x1053
                                           	BANKSEL	r0x1054
001f5e   03d5     CLR	0xd5                 	CLR	r0x1054
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ;	op : !
                                           ;	op : =
                                           ;	.line	103; "../main.c"	LED = !LED;
                                           	BANKSEL	_P1LR_bits
001f5f   7a47     JB	0x47, 2               	JB	_P1LR_bits, 2
001f60   cf63     JMP	#0xf63               	JMP	_00029_DS_
                                           	BANKSEL	_P1LR_bits
001f61   6247     CLR	0x47, 2              	CLR	_P1LR_bits, 2
001f62   cf64     JMP	#0xf64               	JMP	_00030_DS_
                                           _00029_DS_
                                           	BANKSEL	_P1LR_bits
001f63   6a47     SET	0x47, 2              	SET	_P1LR_bits, 2
                                           ;	op : GOTO
                                           _00030_DS_
001f64   cf50     JMP	#0xf50               	JMP	_00006_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
001f65   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._FLASH_WRITE_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _FLASH_READ_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;   _FLASH_READ_FUN
                                           ;   _FLASH_WRITE_FUN
                                           ;11 compiler assigned registers:
                                           ;   r0x1047
                                           ;   STK00
                                           ;   r0x1048
                                           ;   STK01
                                           ;   r0x1049
                                           ;   STK02
                                           ;   r0x104A
                                           ;   r0x104B
                                           ;   r0x104C
                                           ;   r0x104D
                                           ;   r0x104E
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _FLASH_WRITE_ONE	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
001fa1   e100     MOVB	0                   	BANKSEL	r0x104C
001fa2   51e2     MOV	0xe2, R0             	MOV	r0x104C, R0
                                           ;	.line	490; "../main.c"	void FLASH_WRITE_ONE(unsigned int address,unsigned int value)
                                           	BANKSEL	r0x1047
001fa3   51de     MOV	0xde, R0             	MOV	r0x1047, R0
                                           	BANKSEL	STK00
001fa4   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1048
001fa5   51dd     MOV	0xdd, R0             	MOV	r0x1048, R0
                                           ;	op : RECEIVE
                                           	BANKSEL	STK01
001fa6   0e90     MOVZ	R0, 0x90            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1049
001fa7   51e0     MOV	0xe0, R0             	MOV	r0x1049, R0
                                           	BANKSEL	STK02
001fa8   0e8f     MOVZ	R0, 0x8f            	MOVZ	R0, STK02
                                           	BANKSEL	r0x104A
001fa9   51df     MOV	0xdf, R0             	MOV	r0x104A, R0
                                           ;	op : BITWISEAND
                                           ;	.line	493; "../main.c"	FLASH_READ_FUN(address&0xFFE0,FLASH_BUFFER_MAX);
001faa   98e0     MOV	R0, #0xe0            	MOV	R0,# 0xe0
                                           	BANKSEL	r0x1048
001fab   28dd     AND	R0, 0xdd             	AND	R0, r0x1048
                                           	BANKSEL	r0x104B
001fac   51e1     MOV	0xe1, R0             	MOV	r0x104B, R0
                                           ;;106	MOVZ	R0, r0x1047
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
001fad   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
                                           	BANKSEL	STK01
001fae   5190     MOV	0x90, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x104B
001faf   0ee1     MOVZ	R0, 0xe1            	MOVZ	R0, r0x104B
                                           	BANKSEL	STK00
001fb0   5191     MOV	0x91, R0             	MOV	STK00, R0
                                           	BANKSEL	r0x104C
001fb1   0ee2     MOVZ	R0, 0xe2            	MOVZ	R0, r0x104C
001fb2   e010     MOVP	0x10                	PAGESEL	_FLASH_READ_FUN
001fb3   d000     CALL	#0                  	CALL	_FLASH_READ_FUN
001fb4   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : BITWISEAND
                                           ;	.line	495; "../main.c"	FLASH_BUFFER[address&0x1F] = value;
001fb5   981f     MOV	R0, #0x1f            	MOV	R0,# 0x1f
001fb6   e100     MOVB	0                   	BANKSEL	r0x1048
001fb7   28dd     AND	R0, 0xdd             	AND	R0, r0x1048
                                           	BANKSEL	r0x104B
001fb8   51e1     MOV	0xe1, R0             	MOV	r0x104B, R0
                                           	BANKSEL	r0x104C
001fb9   03e2     CLR	0xe2                 	CLR	r0x104C
                                           ;	op : LEFT_OP
001fba   6003     CLR	0x3, 0               	CLR	PSW, 0
                                           	BANKSEL	r0x104B
001fbb   12e1     RLCR	0xe1                	RLCR	r0x104B
                                           	BANKSEL	r0x104D
001fbc   51e3     MOV	0xe3, R0             	MOV	r0x104D, R0
                                           	BANKSEL	r0x104C
001fbd   12e2     RLCR	0xe2                	RLCR	r0x104C
                                           ;;1	MOV	r0x104E, R0
                                           ;	op : +
                                           	BANKSEL	r0x104D
001fbe   50e3     MOV	R0, 0xe3             	MOV	R0, r0x104D
001fbf   8092     ADD	R0, #0x92            	ADD	R0,# (_FLASH_BUFFER + 0)
                                           	BANKSEL	r0x104B
001fc0   51e1     MOV	0xe1, R0             	MOV	r0x104B, R0
                                           ;	op : =
                                           	BANKSEL	r0x104A
001fc1   0edf     MOVZ	R0, 0xdf            	MOVZ	R0, r0x104A
                                           	BANKSEL	r0x104B
001fc2   52e1     MOV	R1, 0xe1             	MOV	R1, r0x104B
                                           	BANKSEL	_FLASH_BUFFER
001fc3   f741     ST	[R1], R0              	ST	[R1], R0
001fc4   ff11     INC	R1                   	INC	R1
                                           	BANKSEL	r0x1049
001fc5   0ee0     MOVZ	R0, 0xe0            	MOVZ	R0, r0x1049
                                           	BANKSEL	_FLASH_BUFFER
001fc6   f741     ST	[R1], R0              	ST	[R1], R0
                                           ;	op : BITWISEAND
                                           ;	.line	497; "../main.c"	FLASH_WRITE_FUN(address&0xFFE0,FLASH_BUFFER_MAX);
001fc7   98e0     MOV	R0, #0xe0            	MOV	R0,# 0xe0
                                           	BANKSEL	r0x1048
001fc8   29dd     AND	0xdd, R0             	AND	r0x1048, R0
                                           ;	op : SEND
                                           ;	op : SEND
                                           ;	op : CALL
001fc9   9820     MOV	R0, #0x20            	MOV	R0,# 0x20
                                           	BANKSEL	STK01
001fca   5190     MOV	0x90, R0             	MOV	STK01, R0
                                           	BANKSEL	r0x1048
001fcb   0edd     MOVZ	R0, 0xdd            	MOVZ	R0, r0x1048
                                           	BANKSEL	STK00
001fcc   5191     MOV	0x91, R0             	MOV	STK00, R0
                                           	BANKSEL	r0x1047
001fcd   0ede     MOVZ	R0, 0xde            	MOVZ	R0, r0x1047
001fce   e01f     MOVP	0x1f                	PAGESEL	_FLASH_WRITE_FUN
001fcf   df66     CALL	#0xf66              	CALL	_FLASH_WRITE_FUN
001fd0   e01f     MOVP	0x1f                	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
001fd1   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_WRITE_ONE
                                           
                                           
                                           
                                           func._FLASH_WRITE_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;7 compiler assigned registers:
                                           ;   r0x1042
                                           ;   STK00
                                           ;   r0x1043
                                           ;   STK01
                                           ;   r0x1044
                                           ;   r0x1045
                                           ;   r0x1046
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _FLASH_WRITE_FUN	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	336; "../main.c"	void FLASH_WRITE_FUN(unsigned int address,unsigned char length)
001f66   e100     MOVB	0                   	BANKSEL	r0x1042
001f67   51db     MOV	0xdb, R0             	MOV	r0x1042, R0
                                           	BANKSEL	STK00
001f68   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1043
001f69   51da     MOV	0xda, R0             	MOV	r0x1043, R0
                                           ;	op : RECEIVE
                                           	BANKSEL	STK01
001f6a   0e90     MOVZ	R0, 0x90            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1044
001f6b   51dc     MOV	0xdc, R0             	MOV	r0x1044, R0
                                           ;	op : RIGHT_OP
                                           ;;105	MOVZ	R0, r0x1042
                                           ;;103	MOV	r0x1045, R0
                                           ;;1	CLR	r0x1046
                                           ;	op : CAST
                                           ;;104	MOVZ	R0, r0x1045
                                           ;	.line	340; "../main.c"	NVMADDRH=(unsigned char) (address>>8);
                                           	BANKSEL	r0x1042
001f6c   0edb     MOVZ	R0, 0xdb            	MOVZ	R0, r0x1042
                                           	BANKSEL	_NVMADDRH
001f6d   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	op : CAST
                                           ;	.line	341; "../main.c"	NVMADDRL=address;
                                           	BANKSEL	r0x1043
001f6e   0eda     MOVZ	R0, 0xda            	MOVZ	R0, r0x1043
                                           	BANKSEL	_NVMADDRL
001f6f   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
001f70   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
001f71   660b     CLR	0xb, 6               	CLR _INTCTL,_PUIE
001f72   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001f73   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
001f74   cf72     JMP	#0xf72               	JMP $-2
                                           	;
001f75   9830     MOV	R0, #0x30            	MOV R0,#0x30
001f76   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
001f77   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
001f78   9b92     MOV	R3, #0x92            	MOV R3,#_FLASH_BUFFER
                                           	
                                           ;	op : =
                                           ;	.line	360; "../main.c"	while(length--)		// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1044
001f79   0edc     MOVZ	R0, 0xdc            	MOVZ	R0, r0x1044
                                           	BANKSEL	r0x1043
001f7a   51da     MOV	0xda, R0             	MOV	r0x1043, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00041_DS_
                                           	BANKSEL	r0x1043
001f7b   0eda     MOVZ	R0, 0xda            	MOVZ	R0, r0x1043
                                           	BANKSEL	r0x1042
001f7c   51db     MOV	0xdb, R0             	MOV	r0x1042, R0
                                           ;	op : -
                                           	BANKSEL	r0x1043
001f7d   07da     DEC	0xda                 	DEC	r0x1043
                                           ;	op : IFX
001f7e   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1042
001f7f   30db     ORL	R0, 0xdb             	ORL	R0, r0x1042
001f80   7203     JNB	0x3, 2               	JNB	PSW, 2
001f81   cf9d     JMP	#0xf9d               	JMP	_00043_DS_
                                           ;	op : INLINEASM
                                           	;
                                           	BANKSEL _FLASH_BUFFER
001f82   f71e     LD	R6, [R3]              	LD R6,[R3]
001f83   ff13     INC	R3                   	INC R3
001f84   f71f     LD	R7, [R3]              	LD R7,[R3]
001f85   ff13     INC	R3                   	INC R3
                                           	BANKSEL _NVMDATAH
001f86   5f38     MOV	0x38, R7             	MOV _NVMDATAH,R7
001f87   5d39     MOV	0x39, R6             	MOV _NVMDATAL,R6
                                           	;
001f88   9d84     MOV	R5, #0x84            	MOV R5 ,#0x84
001f89   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001f8a   9d69     MOV	R5, #0x69            	MOV R5,#0x69
001f8b   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
001f8c   9d96     MOV	R5, #0x96            	MOV R5,#0x96
001f8d   5b3d     MOV	0x3d, R5             	MOV _NVMCTL1,R5
001f8e   693c     SET	0x3c, 1              	SET _NVMCTL0 , 1 ;
001f8f   ffff     NOPZ                     	NOPZ
001f90   ffff     NOPZ                     	NOPZ
001f91   ffff     NOPZ                     	NOPZ
001f92   ffff     NOPZ                     	NOPZ
001f93   ffff     NOPZ                     	NOPZ
001f94   ffff     NOPZ                     	NOPZ ;
001f95   ffff     NOPZ                     	NOPZ
001f96   ffff     NOPZ                     	NOPZ
001f97   ffff     NOPZ                     	NOPZ
001f98   ffff     NOPZ                     	NOPZ
001f99   9d80     MOV	R5, #0x80            	MOV R5,#0X80
001f9a   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
                                           	;
                                           	BANKSEL _NVMADDRL
001f9b   0b3b     INC	0x3b                 	INC _NVMADDRL
                                           	
                                           ;	op : GOTO
001f9c   cf7b     JMP	#0xf7b               	JMP	_00041_DS_
                                           ;	op : LABEL
                                           ;	op : INLINEASM
                                           _00043_DS_
                                           	;
                                           	BANKSEL _OSCCTL
001f9d   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
001f9e   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
001f9f   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
001fa0   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_WRITE_FUN
                                           
                                           
                                           
                                           func._FLASH_READ_FUN	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;7 compiler assigned registers:
                                           ;   r0x1042
                                           ;   STK00
                                           ;   r0x1043
                                           ;   STK01
                                           ;   r0x1044
                                           ;   r0x1045
                                           ;   r0x1046
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _FLASH_READ_FUN	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	206; "../main.c"	void FLASH_READ_FUN(unsigned int address,unsigned char length)
001000   e100     MOVB	0                   	BANKSEL	r0x1042
001001   51db     MOV	0xdb, R0             	MOV	r0x1042, R0
                                           	BANKSEL	STK00
001002   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1043
001003   51da     MOV	0xda, R0             	MOV	r0x1043, R0
                                           ;	op : RECEIVE
                                           	BANKSEL	STK01
001004   0e90     MOVZ	R0, 0x90            	MOVZ	R0, STK01
                                           	BANKSEL	r0x1044
001005   51dc     MOV	0xdc, R0             	MOV	r0x1044, R0
                                           ;	op : RIGHT_OP
                                           ;;102	MOVZ	R0, r0x1042
                                           ;;100	MOV	r0x1045, R0
                                           ;;1	CLR	r0x1046
                                           ;	op : CAST
                                           ;;101	MOVZ	R0, r0x1045
                                           ;	.line	210; "../main.c"	NVMADDRH=(unsigned char) (address>>8);
                                           	BANKSEL	r0x1042
001006   0edb     MOVZ	R0, 0xdb            	MOVZ	R0, r0x1042
                                           	BANKSEL	_NVMADDRH
001007   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	op : CAST
                                           ;	.line	211; "../main.c"	NVMADDRL=address;
                                           	BANKSEL	r0x1043
001008   0eda     MOVZ	R0, 0xda            	MOVZ	R0, r0x1043
                                           	BANKSEL	_NVMADDRL
001009   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
00100a   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
00100b   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
00100c   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
00100d   c00b     JMP	#0xb                 	JMP $-2
                                           	;
00100e   9830     MOV	R0, #0x30            	MOV R0,#0x30
00100f   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
001010   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
001011   9b92     MOV	R3, #0x92            	MOV R3,#_FLASH_BUFFER
                                           	
                                           ;	op : =
                                           ;	.line	229; "../main.c"	while(length--)	// ½öÊ¹ÓÃR0£¬²»¸Ä±äR1
                                           	BANKSEL	r0x1044
001012   0edc     MOVZ	R0, 0xdc            	MOVZ	R0, r0x1044
                                           	BANKSEL	r0x1043
001013   51da     MOV	0xda, R0             	MOV	r0x1043, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00033_DS_
                                           	BANKSEL	r0x1043
001014   0eda     MOVZ	R0, 0xda            	MOVZ	R0, r0x1043
                                           	BANKSEL	r0x1042
001015   51db     MOV	0xdb, R0             	MOV	r0x1042, R0
                                           ;	op : -
                                           	BANKSEL	r0x1043
001016   07da     DEC	0xda                 	DEC	r0x1043
                                           ;	op : IFX
001017   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1042
001018   30db     ORL	R0, 0xdb             	ORL	R0, r0x1042
001019   7203     JNB	0x3, 2               	JNB	PSW, 2
00101a   c02b     JMP	#0x2b                	JMP	_00035_DS_
                                           ;	op : INLINEASM
                                           	;
                                           	BANKSEL _NVMCTL0
00101b   9d81     MOV	R5, #0x81            	MOV R5,#0x81
00101c   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
00101d   ffff     NOPZ                     	NOPZ
00101e   ffff     NOPZ                     	NOPZ
00101f   ffff     NOPZ                     	NOPZ ;
001020   ffff     NOPZ                     	NOPZ
                                           	;
                                           	BANKSEL _NVMDATAL
001021   5c39     MOV	R6, 0x39             	MOV R6,_NVMDATAL
001022   5e38     MOV	R7, 0x38             	MOV R7,_NVMDATAH
                                           	BANKSEL _FLASH_BUFFER
001023   f773     ST	[R3], R6              	ST [R3],R6
001024   ff13     INC	R3                   	INC R3
001025   f77b     ST	[R3], R7              	ST [R3],R7
001026   ff13     INC	R3                   	INC R3
                                           	;
                                           	BANKSEL _NVMADDRL
001027   0b3b     INC	0x3b                 	INC _NVMADDRL
001028   7203     JNB	0x3, 2               	JNB _PSW,_Z
001029   0b3a     INC	0x3a                 	INC _NVMADDRH
                                           	
                                           ;	op : GOTO
00102a   c014     JMP	#0x14                	JMP	_00033_DS_
                                           ;	op : LABEL
                                           ;	op : INLINEASM
                                           _00035_DS_
                                           	;
                                           	BANKSEL _OSCCTL
00102b   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
00102c   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
00102d   330b     ORL	0xb, R1              	ORL _INTCTL,R1
                                           	
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00102e   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_READ_FUN
                                           
                                           
                                           
                                           func._FLASH_READ_ONE	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _FLASH_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x104F
                                           ;   STK00
                                           ;   r0x1050
                                           ;   r0x1051
                                           ;   r0x1052
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _FLASH_READ_ONE	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
00102f   e100     MOVB	0                   	BANKSEL	r0x1051
001030   51d9     MOV	0xd9, R0             	MOV	r0x1051, R0
                                           ;;1	MOV	r0x104F, R0
                                           ;	.line	114; "../main.c"	unsigned int FLASH_READ_ONE(unsigned int address)
                                           	BANKSEL	STK00
001031   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1050
001032   51d8     MOV	0xd8, R0             	MOV	r0x1050, R0
                                           ;	op : RIGHT_OP
                                           ;;99	MOVZ	R0, r0x104F
                                           ;;1	CLR	r0x1052
                                           ;	op : CAST
                                           ;	.line	120; "../main.c"	NVMADDRH=(unsigned char)(address>>8);
                                           	BANKSEL	r0x1051
001033   0ed9     MOVZ	R0, 0xd9            	MOVZ	R0, r0x1051
                                           	BANKSEL	_NVMADDRH
001034   513a     MOV	0x3a, R0             	MOV	_NVMADDRH, R0
                                           ;	op : CAST
                                           ;	.line	121; "../main.c"	NVMADDRL=(unsigned char)address;
                                           	BANKSEL	r0x1050
001035   0ed8     MOVZ	R0, 0xd8            	MOVZ	R0, r0x1050
                                           	BANKSEL	_NVMADDRL
001036   513b     MOV	0x3b, R0             	MOV	_NVMADDRL, R0
                                           ;	op : INLINEASM
                                           	;
                                           	BANKSEL _INTCTL
001037   520b     MOV	R1, 0xb              	MOV R1,_INTCTL
                                           	;
001038   670b     CLR	0xb, 7               	CLR _INTCTL,_AIE
001039   770b     JNB	0xb, 7               	JNB _INTCTL,_AIE
00103a   c038     JMP	#0x38                	JMP $-2
                                           	;
00103b   9830     MOV	R0, #0x30            	MOV R0,#0x30
00103c   542f     MOV	R2, 0x2f             	MOV R2,_OSCCTL
00103d   512f     MOV	0x2f, R0             	MOV _OSCCTL,R0
                                           	;
                                           	BANKSEL _NVMCTL0
00103e   9d81     MOV	R5, #0x81            	MOV R5,#0x81
00103f   5b3c     MOV	0x3c, R5             	MOV _NVMCTL0,R5
001040   ffff     NOPZ                     	NOPZ
001041   ffff     NOPZ                     	NOPZ
001042   ffff     NOPZ                     	NOPZ
001043   ffff     NOPZ                     	NOPZ
                                           	;
001044   552f     MOV	0x2f, R2             	MOV _OSCCTL,R2
001045   89c0     AND	R1, #0xc0            	AND R1,#0xC0 ;
001046   330b     ORL	0xb, R1              	ORL INTCTL,R1
                                           	;
                                           	BANKSEL _NVMDATAL
001047   5c39     MOV	R6, 0x39             	MOV R6,_NVMDATAL
001048   5e38     MOV	R7, 0x38             	MOV R7,_NVMDATAH
                                           	BANKSEL _FLASH_READ_BUF
001049   5dd2     MOV	0xd2, R6             	MOV (_FLASH_READ_BUF),R6
00104a   5fd3     MOV	0xd3, R7             	MOV (_FLASH_READ_BUF+1),R7
                                           	
                                           ;	op : RETURN
                                           ;	.line	154; "../main.c"	return 	FLASH_READ_BUF;
                                           	BANKSEL	_FLASH_READ_BUF
00104b   0ed2     MOVZ	R0, 0xd2            	MOVZ	R0, _FLASH_READ_BUF
                                           	BANKSEL	STK00
00104c   5191     MOV	0x91, R0             	MOV	STK00, R0
                                           	BANKSEL	_FLASH_READ_BUF
00104d   0ed3     MOVZ	R0, 0xd3            	MOVZ	R0, (_FLASH_READ_BUF + 1)
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00104e   0008     CRET                     	CRET	
                                           ; exit point of _FLASH_READ_ONE
                                           
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	42; "../main.c"	OSCCTL = 0x60;                           //ÉèÖÃÎª8M
00104f   9860     MOV	R0, #0x60            	MOV	R0,# 0x60
001050   e100     MOVB	0                   	BANKSEL	_OSCCTL
001051   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	44; "../main.c"	TR0 = 0x04;				                 //ÉèÖÃP0¶Ë¿Ú 	1100 1111
001052   9804     MOV	R0, #0x4             	MOV	R0,# 0x04
                                           	BANKSEL	_TR0
001053   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	45; "../main.c"	TR1 = 0x00;				                 //ÉèÖÃP1¶Ë¿Ú	0000 0000
                                           	BANKSEL	_TR1
001054   0327     CLR	0x27                 	CLR	_TR1
                                           ;	op : =
                                           ;	.line	46; "../main.c"	TR2 = 0x00;				                 //ÉèÖÃP2¶Ë¿Ú	0011 1111
                                           	BANKSEL	_TR2
001055   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	47; "../main.c"	P0 = 0x00;
                                           	BANKSEL	_P0
001056   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	48; "../main.c"	P1 = 0x80;			//P1.6 P1.7 Ö¸Ê¾ÔËÐÐ½áÊøµÆ
001057   9880     MOV	R0, #0x80            	MOV	R0,# 0x80
                                           	BANKSEL	_P1
001058   5107     MOV	0x7, R0              	MOV	_P1, R0
                                           ;	op : =
                                           ;	.line	49; "../main.c"	P2 = 0xF0;
001059   98f0     MOV	R0, #0xf0            	MOV	R0,# 0xf0
                                           	BANKSEL	_P2
00105a   5106     MOV	0x6, R0              	MOV	_P2, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00105b   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           ;	code size estimation:
                                           ;	  237+  127 =   364 instructions (  982 byte)
                                           
                                           
                                           	.end
                                           .config
002007   05c4     CPL	0xc4                
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
00106e   e010     MOVP	0x10               
00106f   d05c     CALL	#0x5c              
001070   e010     MOVP	0x10               
001071   0008     CRET                    
                                           .code
001fd2   e01f     MOVP	0x1f               
001fd3   e100     MOVB	0                  
001fd4   dfff     CALL	#0xfff             
001fd5   5130     MOV	0x30, R0            
001fd6   ffff     NOPZ                    
001fd7   ffff     NOPZ                    
001fd8   dffe     CALL	#0xffe             
001fd9   5137     MOV	0x37, R0            
001fda   ffff     NOPZ                    
001fdb   ffff     NOPZ                    
001fdc   dffd     CALL	#0xffd             
001fdd   514c     MOV	0x4c, R0            
001fde   ffff     NOPZ                    
001fdf   ffff     NOPZ                    
001fe0   dffc     CALL	#0xffc             
001fe1   514d     MOV	0x4d, R0            
001fe2   ffff     NOPZ                    
001fe3   ffff     NOPZ                    
001fe4   dffb     CALL	#0xffb             
001fe5   512a     MOV	0x2a, R0            
001fe6   ffff     NOPZ                    
001fe7   ffff     NOPZ                    
001fe8   e101     MOVB	0x1                
001fe9   dffa     CALL	#0xffa             
001fea   5159     MOV	0x59, R0            
001feb   ffff     NOPZ                    
001fec   ffff     NOPZ                    
001fed   dff9     CALL	#0xff9             
001fee   515a     MOV	0x5a, R0            
001fef   ffff     NOPZ                    
001ff0   ffff     NOPZ                    
001ff1   dff8     CALL	#0xff8             
001ff2   5165     MOV	0x65, R0            
001ff3   ffff     NOPZ                    
001ff4   ffff     NOPZ                    
001ff5   0008     CRET                    
                                           .cinit
00105c   e100     MOVB	0                  
00105d   9880     MOV	R0, #0x80           
00105e   9964     MOV	R1, #0x64           
00105f   e010     MOVP	0x10               
001060   d062     CALL	#0x62              
001061   0008     CRET                    
001062   020a     CLR	R2                  
001063   f750     ST	[R0], R2             
001064   ff10     INC	R0                  
001065   ff59     DECJZ	R1                
001066   c063     JMP	#0x63               
001067   0008     CRET                    
