gplink-1.1.0
Copyright (c) 1998-2005 gputils project
Listing File Generated: 5-20-2016  15:08:13
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 15:05:26 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../config_set.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; config word(s)
                                           ;--------------------------------------------------------
                                           	__config 0x3f94
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           
                                           	.extern I0R1
                                           	.extern I0PSW
                                           	.extern I0PCH
                                           	.extern I1R1
                                           	.extern I1PSW
                                           	.extern I1PCH
                                           	.extern STK11
                                           	.extern STK10
                                           	.extern STK09
                                           	.extern STK08
                                           	.extern STK07
                                           	.extern STK06
                                           	.extern STK05
                                           	.extern STK04
                                           	.extern STK03
                                           	.extern STK02
                                           	.extern STK01
                                           	.extern STK00
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           
                                           ;	code size estimation:
                                           ;	    0+    0 =     0 instructions (    0 byte)
                                           
                                           
                                           	.end
                                           ;--------------------------------------------------------
                                           ; File Created by ChiponCC : aolisn inc.
                                           ; Version 3.0.4#6752 (Nov 19 2015 16:48:50) (MSVC)
                                           ; This file was generated Fri May 20 15:08:13 2016
                                           ;--------------------------------------------------------
                                           ; chipon port for the 16-bit core
                                           ;--------------------------------------------------------
                                           ;	.file	"../main.c"
                                           	.list	p=KF8F4156
                                           	.radix dec
                                           	.include "KF8F4156.inc"
                                           
                                           ;************************************************************ 
                                           ;       Header file for the KungFu8 
                                           ;       KF8F4156 
                                           ;       Microcontroller
                                           ; 
                                           ;       Copyright 2012-2013 ChipON, All rights reserved
                                           ;************************************************************ 
                                            
                                           T0                .EQU                0x01
                                           PCL               .EQU                0x02
                                           PSW               .EQU                0x03
                                           P0                .EQU                0x05
                                           P2                .EQU                0x06
                                           P1                .EQU                0x07
                                           P3                .EQU                0x08
                                           PCH               .EQU                0x0A
                                           INTCTL            .EQU                0x0B
                                           EIF1              .EQU                0x0C
                                           EIF2              .EQU                0x0D
                                           T1L               .EQU                0x0E
                                           T1H               .EQU                0x0F
                                           T1CTL             .EQU                0x10
                                           T2L               .EQU                0x11
                                           T2CTL0            .EQU                0x12
                                           PWM1L             .EQU                0x13
                                           PWM1H             .EQU                0x14
                                           PWMCTL            .EQU                0x15
                                           PP1               .EQU                0x16
                                           BANK              .EQU                0x17
                                           ADSCANCTL         .EQU                0x18
                                           C1CTL             .EQU                0x19
                                           VDACS             .EQU                0x1A
                                           AMPCTL            .EQU                0x1B
                                           ANSEH             .EQU                0x1D
                                           ADCDATA0H         .EQU                0x1E
                                           ADCCTL0           .EQU                0x1F
                                           AMPDT             .EQU                0x20
                                           OPTR              .EQU                0x21
                                           IP0               .EQU                0x22
                                           IP1               .EQU                0x23
                                           IP2               .EQU                0x24
                                           TR0               .EQU                0x25
                                           TR2               .EQU                0x26
                                           TR1               .EQU                0x27
                                           OSCSTA            .EQU                0x28
                                           IP3               .EQU                0x29
                                           VRECAL1           .EQU                0x2A
                                           VRECTL            .EQU                0x2B
                                           EIE1              .EQU                0x2C
                                           EIE2              .EQU                0x2D
                                           PCTL              .EQU                0x2E
                                           OSCCTL            .EQU                0x2F
                                           OSCCAL0           .EQU                0x30
                                           ANSEL             .EQU                0x31
                                           PP2               .EQU                0x32
                                           PWM2L             .EQU                0x33
                                           PWM2H             .EQU                0x34
                                           PUR0              .EQU                0x35
                                           IOCL              .EQU                0x36
                                           OSCCAL1           .EQU                0x37
                                           NVMDATAH          .EQU                0x38
                                           NVMDATAL          .EQU                0x39
                                           NVMADDRH          .EQU                0x3A
                                           NVMADDRL          .EQU                0x3B
                                           NVMCTL0           .EQU                0x3C
                                           NVMCTL1           .EQU                0x3D
                                           ADCDATA0L         .EQU                0x3E
                                           ADCCTL1           .EQU                0x3F
                                           T2CCRH            .EQU                0x40
                                           T2H               .EQU                0x41
                                           PP5H              .EQU                0x42
                                           PWM5H0            .EQU                0x43
                                           PWM5H1            .EQU                0x44
                                           P0LR              .EQU                0x45
                                           P2LR              .EQU                0x46
                                           P1LR              .EQU                0x47
                                           P3LR              .EQU                0x48
                                           TR3               .EQU                0x49
                                           EIE3              .EQU                0x4A
                                           EIF3              .EQU                0x4B
                                           OSCCAL2           .EQU                0x4C
                                           OSCCAL3           .EQU                0x4D
                                           ADCDATA1H         .EQU                0x50
                                           ADCDATA1L         .EQU                0x51
                                           PP5L              .EQU                0x52
                                           T2CCRL            .EQU                0x54
                                           PWM5L0            .EQU                0x55
                                           PWM5L1            .EQU                0x56
                                           PWM5CTL0          .EQU                0x57
                                           ADCINTCTL         .EQU                0x58
                                           ADCDATA2H         .EQU                0x59
                                           ADCDATA2L         .EQU                0x5A
                                           PWM5CTL1          .EQU                0x5B
                                           P5ASCTL           .EQU                0x5C
                                           PSTRCTL           .EQU                0x5D
                                           ADCDATA3H         .EQU                0x5E
                                           PUR1              .EQU                0x60
                                           PUR2              .EQU                0x61
                                           INTEDGCTL         .EQU                0x67
                                           ADCDATA3L         .EQU                0x6A
                                           VBIASCTL          .EQU                0x6B
                                           VBIAS1EN          .EQU                0x6C
                                           VBIAS2EN          .EQU                0x6D
                                           PWM5OC            .EQU                0x10E
                                           T2CTL1            .EQU                0x10F
                                           VDAC              .EQU                0x112
                                           PWM5CTL2          .EQU                0x11C
                                           PWMPC             .EQU                0x11D
                                           RSCTL             .EQU                0x120
                                           TXSDR             .EQU                0x121
                                           RXSDR             .EQU                0x122
                                           BRCTL             .EQU                0x123
                                           TSCTL             .EQU                0x124
                                           EUBRGL            .EQU                0x125
                                           EUBRGH            .EQU                0x126
                                           SSCICTL0          .EQU                0x128
                                           SSCICTL1          .EQU                0x12A
                                           SSCISTA           .EQU                0x12B
                                           SSCIBUFR          .EQU                0x12C
                                           SSCIMSK           .EQU                0x12E
                                           SSCIADD           .EQU                0x12E
                                           WDTPS             .EQU                0x12F
                                           MULAH             .EQU                0x130
                                           MULAL             .EQU                0x131
                                           MULBH             .EQU                0x132
                                           MULBL             .EQU                0x133
                                           MULCTL            .EQU                0x134
                                           MULRES3           .EQU                0x135
                                           MULRES2           .EQU                0x136
                                           MULRES1           .EQU                0x137
                                           MULRES0           .EQU                0x138
                                           DIVCTL            .EQU                0x139
                                           DIVAH             .EQU                0x13A
                                           DIVAL             .EQU                0x13B
                                           DIVB              .EQU                0x13C
                                           DIVQH             .EQU                0x13D
                                           DIVQL             .EQU                0x13E
                                           DIVR              .EQU                0x13F
                                           LEDCTL            .EQU                0x140
                                           LEDPRE            .EQU                0x141
                                           LEDDATA0          .EQU                0x142
                                           LEDDATA1          .EQU                0x143
                                           LEDDATA2          .EQU                0x144
                                           LEDDATA3          .EQU                0x145
                                           LEDDATA4          .EQU                0x146
                                           LEDDATA5          .EQU                0x147
                                           LEDDATA6          .EQU                0x148
                                           LEDDATA7          .EQU                0x149
                                           C1FILTCTL         .EQU                0x14A
                                           C1FILTPRE         .EQU                0x14B
                                           LEDOMS1           .EQU                0x150
                                           LEDODS0           .EQU                0x155
                                           LEDOMS0           .EQU                0x157
                                           LEDODS1           .EQU                0x158
                                           VRECAL2           .EQU                0x159
                                           VRECAL3           .EQU                0x15A
                                           LEDLUM            .EQU                0x15C
                                           PWM5FC            .EQU                0x15D
                                           T4L               .EQU                0x160
                                           T4H               .EQU                0x161
                                           T4REL             .EQU                0x162
                                           T4REH             .EQU                0x163
                                           T4CTL             .EQU                0x164
                                           RC32KCAL          .EQU                0x165
                                            
                                            
                                           
                                           ;PSW Bits-------------------------------------
                                           TO                 .EQU                4
                                           PD                 .EQU                3
                                           Z                  .EQU                2
                                           DC                 .EQU                1
                                           CY                 .EQU                0
                                           _TO                .EQU                4
                                           _PD                .EQU                3
                                           _Z                 .EQU                2
                                           _DC                .EQU                1
                                           _CY                .EQU                0
                                           
                                           ;P0 Bits--------------------------------------
                                           P05                .EQU                5
                                           P04                .EQU                4
                                           P03                .EQU                3
                                           P02                .EQU                2
                                           P01                .EQU                1
                                           P00                .EQU                0
                                           _P05               .EQU                5
                                           _P04               .EQU                4
                                           _P03               .EQU                3
                                           _P02               .EQU                2
                                           _P01               .EQU                1
                                           _P00               .EQU                0
                                           
                                           ;P2 Bits--------------------------------------
                                           P27                .EQU                7
                                           P26                .EQU                6
                                           P25                .EQU                5
                                           P24                .EQU                4
                                           P23                .EQU                3
                                           P22                .EQU                2
                                           P21                .EQU                1
                                           P20                .EQU                0
                                           _P27               .EQU                7
                                           _P26               .EQU                6
                                           _P25               .EQU                5
                                           _P24               .EQU                4
                                           _P23               .EQU                3
                                           _P22               .EQU                2
                                           _P21               .EQU                1
                                           _P20               .EQU                0
                                           
                                           ;P1 Bits--------------------------------------
                                           P17                .EQU                7
                                           P16                .EQU                6
                                           P15                .EQU                5
                                           P14                .EQU                4
                                           P13                .EQU                3
                                           P12                .EQU                2
                                           P11                .EQU                1
                                           P10                .EQU                0
                                           _P17               .EQU                7
                                           _P16               .EQU                6
                                           _P15               .EQU                5
                                           _P14               .EQU                4
                                           _P13               .EQU                3
                                           _P12               .EQU                2
                                           _P11               .EQU                1
                                           _P10               .EQU                0
                                           
                                           ;P3 Bits--------------------------------------
                                           P37                .EQU                7
                                           P36                .EQU                6
                                           P35                .EQU                5
                                           P34                .EQU                4
                                           P33                .EQU                3
                                           P32                .EQU                2
                                           P31                .EQU                1
                                           P30                .EQU                0
                                           _P37               .EQU                7
                                           _P36               .EQU                6
                                           _P35               .EQU                5
                                           _P34               .EQU                4
                                           _P33               .EQU                3
                                           _P32               .EQU                2
                                           _P31               .EQU                1
                                           _P30               .EQU                0
                                           
                                           ;INTCTL Bits----------------------------------
                                           AIE                .EQU                7
                                           AIEH               .EQU                7
                                           PUIE               .EQU                6
                                           AIEL               .EQU                6
                                           T0IE               .EQU                5
                                           INT0IE             .EQU                4
                                           P0IE               .EQU                3
                                           T0IF               .EQU                2
                                           INT0IF             .EQU                1
                                           P0IF               .EQU                0
                                           _AIE               .EQU                7
                                           _AIEH              .EQU                7
                                           _PUIE              .EQU                6
                                           _AIEL              .EQU                6
                                           _T0IE              .EQU                5
                                           _INT0IE            .EQU                4
                                           _P0IE              .EQU                3
                                           _T0IF              .EQU                2
                                           _INT0IF            .EQU                1
                                           _P0IF              .EQU                0
                                           
                                           ;EIF1 Bits------------------------------------
                                           EEIF               .EQU                7
                                           ADIF               .EQU                6
                                           INT2IF             .EQU                5
                                           INT1IF             .EQU                4
                                           C1IF               .EQU                3
                                           PWM2IF             .EQU                2
                                           T2IF               .EQU                1
                                           T1IF               .EQU                0
                                           _EEIF              .EQU                7
                                           _ADIF              .EQU                6
                                           _INT2IF            .EQU                5
                                           _INT1IF            .EQU                4
                                           _C1IF              .EQU                3
                                           _PWM2IF            .EQU                2
                                           _T2IF              .EQU                1
                                           _T1IF              .EQU                0
                                           
                                           ;EIF2 Bits------------------------------------
                                           RCIF               .EQU                5
                                           TXIF               .EQU                4
                                           CCPIF              .EQU                2
                                           BCLIF              .EQU                1
                                           SSCIIF             .EQU                0
                                           _RCIF              .EQU                5
                                           _TXIF              .EQU                4
                                           _CCPIF             .EQU                2
                                           _BCLIF             .EQU                1
                                           _SSCIIF            .EQU                0
                                           
                                           ;T1CTL Bits-----------------------------------
                                           T1RLD              .EQU                7
                                           T1GC               .EQU                6
                                           T1CKS1             .EQU                5
                                           T1CKS0             .EQU                4
                                           T1OSCEN            .EQU                3
                                           T1SY               .EQU                2
                                           T1CS               .EQU                1
                                           T1ON               .EQU                0
                                           _T1RLD             .EQU                7
                                           _T1GC              .EQU                6
                                           _T1CKS1            .EQU                5
                                           _T1CKS0            .EQU                4
                                           _T1OSCEN           .EQU                3
                                           _T1SY              .EQU                2
                                           _T1CS              .EQU                1
                                           _T1ON              .EQU                0
                                           
                                           ;T2CTL0 Bits----------------------------------
                                           T2CKBS3            .EQU                6
                                           T2CKBS2            .EQU                5
                                           T2CKBS1            .EQU                4
                                           T2CKBS0            .EQU                3
                                           T2ON               .EQU                2
                                           T2CKPS1            .EQU                1
                                           T2CKPS0            .EQU                0
                                           _T2CKBS3           .EQU                6
                                           _T2CKBS2           .EQU                5
                                           _T2CKBS1           .EQU                4
                                           _T2CKBS0           .EQU                3
                                           _T2ON              .EQU                2
                                           _T2CKPS1           .EQU                1
                                           _T2CKPS0           .EQU                0
                                           
                                           ;PWMCTL Bits----------------------------------
                                           PWM2ON             .EQU                4
                                           PWM1ON             .EQU                0
                                           _PWM2ON            .EQU                4
                                           _PWM1ON            .EQU                0
                                           
                                           ;BANK Bits------------------------------------
                                           PR3                .EQU                3
                                           PR2                .EQU                2
                                           PR1                .EQU                1
                                           PR0                .EQU                0
                                           _PR3               .EQU                3
                                           _PR2               .EQU                2
                                           _PR1               .EQU                1
                                           _PR0               .EQU                0
                                           
                                           ;ADSCANCTL Bits-------------------------------
                                           ADSCANEN           .EQU                7
                                           SMOD1              .EQU                6
                                           SMOD0              .EQU                5
                                           STIM4              .EQU                4
                                           STIM3              .EQU                3
                                           STIM2              .EQU                2
                                           STIM1              .EQU                1
                                           STIM0              .EQU                0
                                           _ADSCANEN          .EQU                7
                                           _SMOD1             .EQU                6
                                           _SMOD0             .EQU                5
                                           _STIM4             .EQU                4
                                           _STIM3             .EQU                3
                                           _STIM2             .EQU                2
                                           _STIM1             .EQU                1
                                           _STIM0             .EQU                0
                                           
                                           ;C1CTL Bits-----------------------------------
                                           C1MOD2             .EQU                6
                                           C1MOD1             .EQU                5
                                           C1MOD0             .EQU                4
                                           C1OUT              .EQU                1
                                           C1EN               .EQU                0
                                           _C1MOD2            .EQU                6
                                           _C1MOD1            .EQU                5
                                           _C1MOD0            .EQU                4
                                           _C1OUT             .EQU                1
                                           _C1EN              .EQU                0
                                           
                                           ;VDACS Bits-----------------------------------
                                           VCEN               .EQU                6
                                           _VCEN              .EQU                6
                                           
                                           ;AMPCTL Bits----------------------------------
                                           AMPCALD            .EQU                7
                                           INPS1              .EQU                5
                                           INPS0              .EQU                4
                                           AMPCALEN           .EQU                1
                                           AMPON              .EQU                0
                                           _AMPCALD           .EQU                7
                                           _INPS1             .EQU                5
                                           _INPS0             .EQU                4
                                           _AMPCALEN          .EQU                1
                                           _AMPON             .EQU                0
                                           
                                           ;ANSEH Bits-----------------------------------
                                           ANS13              .EQU                5
                                           ANS12              .EQU                4
                                           ANS11              .EQU                3
                                           ANS10              .EQU                2
                                           ANS9               .EQU                1
                                           ANS8               .EQU                0
                                           _ANS13             .EQU                5
                                           _ANS12             .EQU                4
                                           _ANS11             .EQU                3
                                           _ANS10             .EQU                2
                                           _ANS9              .EQU                1
                                           _ANS8              .EQU                0
                                           
                                           ;ADCCTL0 Bits---------------------------------
                                           ADLR               .EQU                7
                                           T2CCRON            .EQU                6
                                           CHS3               .EQU                5
                                           CHS2               .EQU                4
                                           CHS1               .EQU                3
                                           CHS0               .EQU                2
                                           START              .EQU                1
                                           ADEN               .EQU                0
                                           _ADLR              .EQU                7
                                           _T2CCRON           .EQU                6
                                           _CHS3              .EQU                5
                                           _CHS2              .EQU                4
                                           _CHS1              .EQU                3
                                           _CHS0              .EQU                2
                                           _START             .EQU                1
                                           _ADEN              .EQU                0
                                           
                                           ;AMPDT Bits-----------------------------------
                                           AMPDT7             .EQU                7
                                           AMPDT6             .EQU                6
                                           AMPDT5             .EQU                5
                                           AMPDT4             .EQU                4
                                           AMPDT3             .EQU                3
                                           AMPDT2             .EQU                2
                                           AMPDT1             .EQU                1
                                           AMPDT0             .EQU                0
                                           _AMPDT7            .EQU                7
                                           _AMPDT6            .EQU                6
                                           _AMPDT5            .EQU                5
                                           _AMPDT4            .EQU                4
                                           _AMPDT3            .EQU                3
                                           _AMPDT2            .EQU                2
                                           _AMPDT1            .EQU                1
                                           _AMPDT0            .EQU                0
                                           
                                           ;OPTR Bits------------------------------------
                                           PUPH               .EQU                7
                                           INT0SE             .EQU                6
                                           T0CS               .EQU                5
                                           T0SE               .EQU                4
                                           PSA                .EQU                3
                                           PS2                .EQU                2
                                           PS1                .EQU                1
                                           PS0                .EQU                0
                                           _PUPH              .EQU                7
                                           _INT0SE            .EQU                6
                                           _T0CS              .EQU                5
                                           _T0SE              .EQU                4
                                           _PSA               .EQU                3
                                           _PS2               .EQU                2
                                           _PS1               .EQU                1
                                           _PS0               .EQU                0
                                           
                                           ;IP0 Bits-------------------------------------
                                           PT0                .EQU                2
                                           PINT0              .EQU                1
                                           PP0                .EQU                0
                                           _PT0               .EQU                2
                                           _PINT0             .EQU                1
                                           _PP0               .EQU                0
                                           
                                           ;IP1 Bits-------------------------------------
                                           PEE                .EQU                7
                                           PADC               .EQU                6
                                           PINT2              .EQU                5
                                           PINT1              .EQU                4
                                           PC1                .EQU                3
                                           PPWM2              .EQU                2
                                           PT2                .EQU                1
                                           PT1                .EQU                0
                                           _PEE               .EQU                7
                                           _PADC              .EQU                6
                                           _PINT2             .EQU                5
                                           _PINT1             .EQU                4
                                           _PC1               .EQU                3
                                           _PPWM2             .EQU                2
                                           _PT2               .EQU                1
                                           _PT1               .EQU                0
                                           
                                           ;IP2 Bits-------------------------------------
                                           PRC                .EQU                5
                                           PTX                .EQU                4
                                           PCCP               .EQU                2
                                           PBCL               .EQU                1
                                           PSSCI              .EQU                0
                                           _PRC               .EQU                5
                                           _PTX               .EQU                4
                                           _PCCP              .EQU                2
                                           _PBCL              .EQU                1
                                           _PSSCI             .EQU                0
                                           
                                           ;TR0 Bits-------------------------------------
                                           TR05               .EQU                5
                                           TR04               .EQU                4
                                           TR03               .EQU                3
                                           TR02               .EQU                2
                                           TR01               .EQU                1
                                           TR00               .EQU                0
                                           _TR05              .EQU                5
                                           _TR04              .EQU                4
                                           _TR03              .EQU                3
                                           _TR02              .EQU                2
                                           _TR01              .EQU                1
                                           _TR00              .EQU                0
                                           
                                           ;TR2 Bits-------------------------------------
                                           TR27               .EQU                7
                                           TR26               .EQU                6
                                           TR25               .EQU                5
                                           TR24               .EQU                4
                                           TR23               .EQU                3
                                           TR22               .EQU                2
                                           TR21               .EQU                1
                                           TR20               .EQU                0
                                           _TR27              .EQU                7
                                           _TR26              .EQU                6
                                           _TR25              .EQU                5
                                           _TR24              .EQU                4
                                           _TR23              .EQU                3
                                           _TR22              .EQU                2
                                           _TR21              .EQU                1
                                           _TR20              .EQU                0
                                           
                                           ;TR1 Bits-------------------------------------
                                           TR17               .EQU                7
                                           TR16               .EQU                6
                                           TR15               .EQU                5
                                           TR14               .EQU                4
                                           TR13               .EQU                3
                                           TR12               .EQU                2
                                           TR11               .EQU                1
                                           TR10               .EQU                0
                                           _TR17              .EQU                7
                                           _TR16              .EQU                6
                                           _TR15              .EQU                5
                                           _TR14              .EQU                4
                                           _TR13              .EQU                3
                                           _TR12              .EQU                2
                                           _TR11              .EQU                1
                                           _TR10              .EQU                0
                                           
                                           ;OSCSTA Bits----------------------------------
                                           OSTS               .EQU                6
                                           HTS                .EQU                5
                                           LTS                .EQU                4
                                           SCF1               .EQU                1
                                           SCF0               .EQU                0
                                           _OSTS              .EQU                6
                                           _HTS               .EQU                5
                                           _LTS               .EQU                4
                                           _SCF1              .EQU                1
                                           _SCF0              .EQU                0
                                           
                                           ;IP3 Bits-------------------------------------
                                           PT4                .EQU                7
                                           POSCFAIL           .EQU                5
                                           _PT4               .EQU                7
                                           _POSCFAIL          .EQU                5
                                           
                                           ;VRECTL Bits----------------------------------
                                           VRESEL1            .EQU                7
                                           VRESEL0            .EQU                6
                                           VRECALEN           .EQU                5
                                           VREBG              .EQU                4
                                           VREOE              .EQU                3
                                           P18OE              .EQU                2
                                           VREEN              .EQU                1
                                           LPREN              .EQU                0
                                           _VRESEL1           .EQU                7
                                           _VRESEL0           .EQU                6
                                           _VRECALEN          .EQU                5
                                           _VREBG             .EQU                4
                                           _VREOE             .EQU                3
                                           _P18OE             .EQU                2
                                           _VREEN             .EQU                1
                                           _LPREN             .EQU                0
                                           
                                           ;EIE1 Bits------------------------------------
                                           EEIE               .EQU                7
                                           ADIE               .EQU                6
                                           INT2IE             .EQU                5
                                           INT1IE             .EQU                4
                                           C1IE               .EQU                3
                                           PWM2IE             .EQU                2
                                           T2IE               .EQU                1
                                           T1IE               .EQU                0
                                           _EEIE              .EQU                7
                                           _ADIE              .EQU                6
                                           _INT2IE            .EQU                5
                                           _INT1IE            .EQU                4
                                           _C1IE              .EQU                3
                                           _PWM2IE            .EQU                2
                                           _T2IE              .EQU                1
                                           _T1IE              .EQU                0
                                           
                                           ;EIE2 Bits------------------------------------
                                           RCIE               .EQU                5
                                           TXIE               .EQU                4
                                           CCPIE              .EQU                2
                                           BCLIE              .EQU                1
                                           SSCIIE             .EQU                0
                                           _RCIE              .EQU                5
                                           _TXIE              .EQU                4
                                           _CCPIE             .EQU                2
                                           _BCLIE             .EQU                1
                                           _SSCIIE            .EQU                0
                                           
                                           ;PCTL Bits------------------------------------
                                           SLVREN             .EQU                4
                                           IPEN               .EQU                3
                                           SWDTEN             .EQU                2
                                           POR                .EQU                1
                                           LVR                .EQU                0
                                           _SLVREN            .EQU                4
                                           _IPEN              .EQU                3
                                           _SWDTEN            .EQU                2
                                           _POR               .EQU                1
                                           _LVR               .EQU                0
                                           
                                           ;OSCCTL Bits----------------------------------
                                           CLKOE              .EQU                7
                                           IRCS2              .EQU                6
                                           IRCS1              .EQU                5
                                           IRCS0              .EQU                4
                                           SCS1               .EQU                3
                                           SCS0               .EQU                2
                                           IESO               .EQU                1
                                           FSCM               .EQU                0
                                           _CLKOE             .EQU                7
                                           _IRCS2             .EQU                6
                                           _IRCS1             .EQU                5
                                           _IRCS0             .EQU                4
                                           _SCS1              .EQU                3
                                           _SCS0              .EQU                2
                                           _IESO              .EQU                1
                                           _FSCM              .EQU                0
                                           
                                           ;ANSEL Bits-----------------------------------
                                           ANS7               .EQU                7
                                           ANS6               .EQU                6
                                           ANS5               .EQU                5
                                           ANS4               .EQU                4
                                           ANS3               .EQU                3
                                           ANS2               .EQU                2
                                           ANS1               .EQU                1
                                           ANS0               .EQU                0
                                           _ANS7              .EQU                7
                                           _ANS6              .EQU                6
                                           _ANS5              .EQU                5
                                           _ANS4              .EQU                4
                                           _ANS3              .EQU                3
                                           _ANS2              .EQU                2
                                           _ANS1              .EQU                1
                                           _ANS0              .EQU                0
                                           
                                           ;PUR0 Bits------------------------------------
                                           PUR05              .EQU                5
                                           PUR04              .EQU                4
                                           PUR03              .EQU                3
                                           PUR01              .EQU                1
                                           PUR00              .EQU                0
                                           _PUR05             .EQU                5
                                           _PUR04             .EQU                4
                                           _PUR03             .EQU                3
                                           _PUR01             .EQU                1
                                           _PUR00             .EQU                0
                                           
                                           ;IOCL Bits------------------------------------
                                           IOCL5              .EQU                5
                                           IOCL4              .EQU                4
                                           IOCL3              .EQU                3
                                           IOCL2              .EQU                2
                                           IOCL1              .EQU                1
                                           IOCL0              .EQU                0
                                           _IOCL5             .EQU                5
                                           _IOCL4             .EQU                4
                                           _IOCL3             .EQU                3
                                           _IOCL2             .EQU                2
                                           _IOCL1             .EQU                1
                                           _IOCL0             .EQU                0
                                           
                                           ;ADCCTL1 Bits---------------------------------
                                           ADCALEN            .EQU                7
                                           ADCS2              .EQU                6
                                           ADCS1              .EQU                5
                                           ADCS0              .EQU                4
                                           VCFG1              .EQU                3
                                           VCFG0              .EQU                2
                                           ADCIM              .EQU                0
                                           _ADCALEN           .EQU                7
                                           _ADCS2             .EQU                6
                                           _ADCS1             .EQU                5
                                           _ADCS0             .EQU                4
                                           _VCFG1             .EQU                3
                                           _VCFG0             .EQU                2
                                           _ADCIM             .EQU                0
                                           
                                           ;P0LR Bits------------------------------------
                                           P0LR5              .EQU                5
                                           P0LR4              .EQU                4
                                           P0LR3              .EQU                3
                                           P0LR1              .EQU                1
                                           P0LR0              .EQU                0
                                           _P0LR5             .EQU                5
                                           _P0LR4             .EQU                4
                                           _P0LR3             .EQU                3
                                           _P0LR1             .EQU                1
                                           _P0LR0             .EQU                0
                                           
                                           ;P2LR Bits------------------------------------
                                           P2LR7              .EQU                7
                                           P2LR6              .EQU                6
                                           P2LR5              .EQU                5
                                           P2LR4              .EQU                4
                                           P2LR3              .EQU                3
                                           P2LR2              .EQU                2
                                           P2LR1              .EQU                1
                                           P2LR0              .EQU                0
                                           _P2LR7             .EQU                7
                                           _P2LR6             .EQU                6
                                           _P2LR5             .EQU                5
                                           _P2LR4             .EQU                4
                                           _P2LR3             .EQU                3
                                           _P2LR2             .EQU                2
                                           _P2LR1             .EQU                1
                                           _P2LR0             .EQU                0
                                           
                                           ;P1LR Bits------------------------------------
                                           P1LR7              .EQU                7
                                           P1LR6              .EQU                6
                                           P1LR5              .EQU                5
                                           P1LR4              .EQU                4
                                           P1LR3              .EQU                3
                                           P1LR2              .EQU                2
                                           P1LR1              .EQU                1
                                           P1LR0              .EQU                0
                                           _P1LR7             .EQU                7
                                           _P1LR6             .EQU                6
                                           _P1LR5             .EQU                5
                                           _P1LR4             .EQU                4
                                           _P1LR3             .EQU                3
                                           _P1LR2             .EQU                2
                                           _P1LR1             .EQU                1
                                           _P1LR0             .EQU                0
                                           
                                           ;P3LR Bits------------------------------------
                                           P3LR7              .EQU                7
                                           P3LR6              .EQU                6
                                           P3LR5              .EQU                5
                                           P3LR4              .EQU                4
                                           P3LR3              .EQU                3
                                           P3LR2              .EQU                2
                                           P3LR1              .EQU                1
                                           P3LR0              .EQU                0
                                           _P3LR7             .EQU                7
                                           _P3LR6             .EQU                6
                                           _P3LR5             .EQU                5
                                           _P3LR4             .EQU                4
                                           _P3LR3             .EQU                3
                                           _P3LR2             .EQU                2
                                           _P3LR1             .EQU                1
                                           _P3LR0             .EQU                0
                                           
                                           ;TR3 Bits-------------------------------------
                                           TR37               .EQU                7
                                           TR36               .EQU                6
                                           TR35               .EQU                5
                                           TR34               .EQU                4
                                           TR33               .EQU                3
                                           TR32               .EQU                2
                                           TR31               .EQU                1
                                           TR30               .EQU                0
                                           _TR37              .EQU                7
                                           _TR36              .EQU                6
                                           _TR35              .EQU                5
                                           _TR34              .EQU                4
                                           _TR33              .EQU                3
                                           _TR32              .EQU                2
                                           _TR31              .EQU                1
                                           _TR30              .EQU                0
                                           
                                           ;EIE3 Bits------------------------------------
                                           T4IE               .EQU                7
                                           OSCFAILIE          .EQU                5
                                           _T4IE              .EQU                7
                                           _OSCFAILIE         .EQU                5
                                           
                                           ;EIF3 Bits------------------------------------
                                           T4IF               .EQU                7
                                           OSCFAILIF          .EQU                5
                                           _T4IF              .EQU                7
                                           _OSCFAILIF         .EQU                5
                                           
                                           ;PWM5CTL0 Bits--------------------------------
                                           P5CH1MOD1          .EQU                7
                                           P5CH1MOD0          .EQU                6
                                           P5MOD3             .EQU                3
                                           P5MOD2             .EQU                2
                                           P5MOD1             .EQU                1
                                           P5MOD0             .EQU                0
                                           _P5CH1MOD1         .EQU                7
                                           _P5CH1MOD0         .EQU                6
                                           _P5MOD3            .EQU                3
                                           _P5MOD2            .EQU                2
                                           _P5MOD1            .EQU                1
                                           _P5MOD0            .EQU                0
                                           
                                           ;ADCINTCTL Bits-------------------------------
                                           INTCTL1            .EQU                1
                                           INTCTL0            .EQU                0
                                           _INTCTL1           .EQU                1
                                           _INTCTL0           .EQU                0
                                           
                                           ;PWM5CTL1 Bits--------------------------------
                                           P5RSEN             .EQU                7
                                           P5DC6              .EQU                6
                                           P5DC5              .EQU                5
                                           P5DC4              .EQU                4
                                           P5DC3              .EQU                3
                                           P5DC2              .EQU                2
                                           P5DC1              .EQU                1
                                           P5DC0              .EQU                0
                                           _P5RSEN            .EQU                7
                                           _P5DC6             .EQU                6
                                           _P5DC5             .EQU                5
                                           _P5DC4             .EQU                4
                                           _P5DC3             .EQU                3
                                           _P5DC2             .EQU                2
                                           _P5DC1             .EQU                1
                                           _P5DC0             .EQU                0
                                           
                                           ;P5ASCTL Bits---------------------------------
                                           P5ASE              .EQU                7
                                           P5ASS2             .EQU                6
                                           P5ASS1             .EQU                5
                                           P5ASS0             .EQU                4
                                           P5SSAC1            .EQU                3
                                           P5SSAC0            .EQU                2
                                           P5SSBD1            .EQU                1
                                           P5SSBD0            .EQU                0
                                           _P5ASE             .EQU                7
                                           _P5ASS2            .EQU                6
                                           _P5ASS1            .EQU                5
                                           _P5ASS0            .EQU                4
                                           _P5SSAC1           .EQU                3
                                           _P5SSAC0           .EQU                2
                                           _P5SSBD1           .EQU                1
                                           _P5SSBD0           .EQU                0
                                           
                                           ;PSTRCTL Bits---------------------------------
                                           STRSYNC            .EQU                4
                                           STREND             .EQU                3
                                           STRENC             .EQU                2
                                           STRENB             .EQU                1
                                           STRENA             .EQU                0
                                           _STRSYNC           .EQU                4
                                           _STREND            .EQU                3
                                           _STRENC            .EQU                2
                                           _STRENB            .EQU                1
                                           _STRENA            .EQU                0
                                           
                                           ;PUR1 Bits------------------------------------
                                           PUR17              .EQU                7
                                           PUR16              .EQU                6
                                           PUR15              .EQU                5
                                           PUR14              .EQU                4
                                           PUR13              .EQU                3
                                           PUR12              .EQU                2
                                           PUR11              .EQU                1
                                           PUR10              .EQU                0
                                           _PUR17             .EQU                7
                                           _PUR16             .EQU                6
                                           _PUR15             .EQU                5
                                           _PUR14             .EQU                4
                                           _PUR13             .EQU                3
                                           _PUR12             .EQU                2
                                           _PUR11             .EQU                1
                                           _PUR10             .EQU                0
                                           
                                           ;PUR2 Bits------------------------------------
                                           PUR27              .EQU                7
                                           PUR26              .EQU                6
                                           PUR25              .EQU                5
                                           PUR24              .EQU                4
                                           PUR23              .EQU                3
                                           PUR22              .EQU                2
                                           PUR21              .EQU                1
                                           PUR20              .EQU                0
                                           _PUR27             .EQU                7
                                           _PUR26             .EQU                6
                                           _PUR25             .EQU                5
                                           _PUR24             .EQU                4
                                           _PUR23             .EQU                3
                                           _PUR22             .EQU                2
                                           _PUR21             .EQU                1
                                           _PUR20             .EQU                0
                                           
                                           ;INTEDGCTL Bits-------------------------------
                                           INT2SE             .EQU                7
                                           INT1SE             .EQU                6
                                           T1CLKEN            .EQU                0
                                           _INT2SE            .EQU                7
                                           _INT1SE            .EQU                6
                                           _T1CLKEN           .EQU                0
                                           
                                           ;VBIASCTL Bits--------------------------------
                                           VBIASEN            .EQU                7
                                           VBSEL              .EQU                6
                                           ISEL3              .EQU                4
                                           ISEL2              .EQU                3
                                           ISEL1              .EQU                2
                                           ISEL0              .EQU                1
                                           _VBIASEN           .EQU                7
                                           _VBSEL             .EQU                6
                                           _ISEL3             .EQU                4
                                           _ISEL2             .EQU                3
                                           _ISEL1             .EQU                2
                                           _ISEL0             .EQU                1
                                           
                                           ;VBIAS1EN Bits--------------------------------
                                           VBS17EN            .EQU                7
                                           VBS16EN            .EQU                6
                                           VBS15EN            .EQU                5
                                           VBS14EN            .EQU                4
                                           VBS13EN            .EQU                3
                                           VBS12EN            .EQU                2
                                           VBS11EN            .EQU                1
                                           VBS10EN            .EQU                0
                                           _VBS17EN           .EQU                7
                                           _VBS16EN           .EQU                6
                                           _VBS15EN           .EQU                5
                                           _VBS14EN           .EQU                4
                                           _VBS13EN           .EQU                3
                                           _VBS12EN           .EQU                2
                                           _VBS11EN           .EQU                1
                                           _VBS10EN           .EQU                0
                                           
                                           ;VBIAS2EN Bits--------------------------------
                                           VBS27EN            .EQU                7
                                           VBS26EN            .EQU                6
                                           VBS25EN            .EQU                5
                                           VBS24EN            .EQU                4
                                           VBS23EN            .EQU                3
                                           VBS22EN            .EQU                2
                                           VBS21EN            .EQU                1
                                           VBS20EN            .EQU                0
                                           _VBS27EN           .EQU                7
                                           _VBS26EN           .EQU                6
                                           _VBS25EN           .EQU                5
                                           _VBS24EN           .EQU                4
                                           _VBS23EN           .EQU                3
                                           _VBS22EN           .EQU                2
                                           _VBS21EN           .EQU                1
                                           _VBS20EN           .EQU                0
                                           
                                           ;PWM5OC Bits----------------------------------
                                           OCA                .EQU                1
                                           OCB                .EQU                0
                                           _OCA               .EQU                1
                                           _OCB               .EQU                0
                                           
                                           ;T2CTL1 Bits----------------------------------
                                           T2MOD1             .EQU                7
                                           T2MOD0             .EQU                6
                                           T2OFS1             .EQU                5
                                           T2OFS0             .EQU                4
                                           T2TRIGEN           .EQU                3
                                           T2DIR              .EQU                0
                                           _T2MOD1            .EQU                7
                                           _T2MOD0            .EQU                6
                                           _T2OFS1            .EQU                5
                                           _T2OFS0            .EQU                4
                                           _T2TRIGEN          .EQU                3
                                           _T2DIR             .EQU                0
                                           
                                           ;VDAC Bits------------------------------------
                                           VDAC3              .EQU                7
                                           VDAC2              .EQU                6
                                           VDAC1              .EQU                5
                                           VDAC0              .EQU                4
                                           _VDAC3             .EQU                7
                                           _VDAC2             .EQU                6
                                           _VDAC1             .EQU                5
                                           _VDAC0             .EQU                4
                                           
                                           ;PWM5CTL2 Bits--------------------------------
                                           PFUSES             .EQU                5
                                           UDEVT1             .EQU                2
                                           UDEVT0             .EQU                1
                                           UDEN               .EQU                0
                                           _PFUSES            .EQU                5
                                           _UDEVT1            .EQU                2
                                           _UDEVT0            .EQU                1
                                           _UDEN              .EQU                0
                                           
                                           ;PWMPC Bits-----------------------------------
                                           PCA                .EQU                1
                                           PCB                .EQU                0
                                           _PCA               .EQU                1
                                           _PCB               .EQU                0
                                           
                                           ;RSCTL Bits-----------------------------------
                                           SPEN               .EQU                7
                                           RX9                .EQU                6
                                           SRXEN              .EQU                5
                                           CRXEN              .EQU                4
                                           ADREN              .EQU                3
                                           FRER               .EQU                2
                                           OVFER              .EQU                1
                                           RX9D               .EQU                0
                                           _SPEN              .EQU                7
                                           _RX9               .EQU                6
                                           _SRXEN             .EQU                5
                                           _CRXEN             .EQU                4
                                           _ADREN             .EQU                3
                                           _FRER              .EQU                2
                                           _OVFER             .EQU                1
                                           _RX9D              .EQU                0
                                           
                                           ;BRCTL Bits-----------------------------------
                                           ABRDOVF            .EQU                7
                                           RCIDLF             .EQU                6
                                           SCKPS              .EQU                5
                                           BRG16              .EQU                4
                                           WUEN               .EQU                1
                                           ABRDEN             .EQU                0
                                           _ABRDOVF           .EQU                7
                                           _RCIDLF            .EQU                6
                                           _SCKPS             .EQU                5
                                           _BRG16             .EQU                4
                                           _WUEN              .EQU                1
                                           _ABRDEN            .EQU                0
                                           
                                           ;TSCTL Bits-----------------------------------
                                           CSRS               .EQU                7
                                           TX9                .EQU                6
                                           TXEN               .EQU                5
                                           SYNC               .EQU                4
                                           SENDB              .EQU                3
                                           HBRG               .EQU                2
                                           TXSRS              .EQU                1
                                           TX9D               .EQU                0
                                           _CSRS              .EQU                7
                                           _TX9               .EQU                6
                                           _TXEN              .EQU                5
                                           _SYNC              .EQU                4
                                           _SENDB             .EQU                3
                                           _HBRG              .EQU                2
                                           _TXSRS             .EQU                1
                                           _TX9D              .EQU                0
                                           
                                           ;SSCICTL0 Bits--------------------------------
                                           SSCIWCFL           .EQU                7
                                           SSCIOV             .EQU                6
                                           SSCIEN             .EQU                5
                                           SSCICKP            .EQU                4
                                           SSCIMOD3           .EQU                3
                                           SSCIMOD2           .EQU                2
                                           SSCIMOD1           .EQU                1
                                           SSCIMOD0           .EQU                0
                                           _SSCIWCFL          .EQU                7
                                           _SSCIOV            .EQU                6
                                           _SSCIEN            .EQU                5
                                           _SSCICKP           .EQU                4
                                           _SSCIMOD3          .EQU                3
                                           _SSCIMOD2          .EQU                2
                                           _SSCIMOD1          .EQU                1
                                           _SSCIMOD0          .EQU                0
                                           
                                           ;SSCICTL1 Bits--------------------------------
                                           SSCICALLEN         .EQU                7
                                           SSCIACKSTA         .EQU                6
                                           SSCIACKDAT         .EQU                5
                                           SSCIACKEN          .EQU                4
                                           SSCIRCEN           .EQU                3
                                           STOPEN             .EQU                2
                                           RESTARTEN          .EQU                1
                                           STARTEN            .EQU                0
                                           _SSCICALLEN        .EQU                7
                                           _SSCIACKSTA        .EQU                6
                                           _SSCIACKDAT        .EQU                5
                                           _SSCIACKEN         .EQU                4
                                           _SSCIRCEN          .EQU                3
                                           _STOPEN            .EQU                2
                                           _RESTARTEN         .EQU                1
                                           _STARTEN           .EQU                0
                                           
                                           ;SSCISTA Bits---------------------------------
                                           SAMPLE             .EQU                7
                                           CKEGE              .EQU                6
                                           SSCIDA             .EQU                5
                                           SSCISTOP           .EQU                4
                                           SSCISTART          .EQU                3
                                           SSCIRW             .EQU                2
                                           SSCIUA             .EQU                1
                                           SSCIBUF            .EQU                0
                                           _SAMPLE            .EQU                7
                                           _CKEGE             .EQU                6
                                           _SSCIDA            .EQU                5
                                           _SSCISTOP          .EQU                4
                                           _SSCISTART         .EQU                3
                                           _SSCIRW            .EQU                2
                                           _SSCIUA            .EQU                1
                                           _SSCIBUF           .EQU                0
                                           
                                           ;SSCIMSK Bits---------------------------------
                                           SSCIMSK7           .EQU                7
                                           SSCIMSK6           .EQU                6
                                           SSCIMSK5           .EQU                5
                                           SSCIMSK4           .EQU                4
                                           SSCIMSK3           .EQU                3
                                           SSCIMSK2           .EQU                2
                                           SSCIMSK1           .EQU                1
                                           SSCIMSK0           .EQU                0
                                           _SSCIMSK7          .EQU                7
                                           _SSCIMSK6          .EQU                6
                                           _SSCIMSK5          .EQU                5
                                           _SSCIMSK4          .EQU                4
                                           _SSCIMSK3          .EQU                3
                                           _SSCIMSK2          .EQU                2
                                           _SSCIMSK1          .EQU                1
                                           _SSCIMSK0          .EQU                0
                                           
                                           ;WDTPS Bits-----------------------------------
                                           WDTPS3             .EQU                3
                                           WDTPS2             .EQU                2
                                           WDTPS1             .EQU                1
                                           WDTPS0             .EQU                0
                                           _WDTPS3            .EQU                3
                                           _WDTPS2            .EQU                2
                                           _WDTPS1            .EQU                1
                                           _WDTPS0            .EQU                0
                                           
                                           ;MULCTL Bits----------------------------------
                                           MULEN              .EQU                1
                                           MULIF              .EQU                0
                                           _MULEN             .EQU                1
                                           _MULIF             .EQU                0
                                           
                                           ;DIVCTL Bits----------------------------------
                                           DIVOEN             .EQU                1
                                           DIVEN              .EQU                0
                                           _DIVOEN            .EQU                1
                                           _DIVEN             .EQU                0
                                           
                                           ;LEDCTL Bits----------------------------------
                                           LEDEN              .EQU                7
                                           DIGEN2             .EQU                4
                                           DIGEN1             .EQU                3
                                           DIGEN0             .EQU                2
                                           PNS1               .EQU                1
                                           PNS0               .EQU                0
                                           _LEDEN             .EQU                7
                                           _DIGEN2            .EQU                4
                                           _DIGEN1            .EQU                3
                                           _DIGEN0            .EQU                2
                                           _PNS1              .EQU                1
                                           _PNS0              .EQU                0
                                           
                                           ;LEDPRE Bits----------------------------------
                                           LEDCKS13           .EQU                7
                                           LEDCKS12           .EQU                6
                                           LEDCKS11           .EQU                5
                                           LEDCKS10           .EQU                4
                                           LEDCKS03           .EQU                3
                                           LEDCKS02           .EQU                2
                                           LEDCKS01           .EQU                1
                                           LEDCKS00           .EQU                0
                                           _LEDCKS13          .EQU                7
                                           _LEDCKS12          .EQU                6
                                           _LEDCKS11          .EQU                5
                                           _LEDCKS10          .EQU                4
                                           _LEDCKS03          .EQU                3
                                           _LEDCKS02          .EQU                2
                                           _LEDCKS01          .EQU                1
                                           _LEDCKS00          .EQU                0
                                           
                                           ;LEDDATA0 Bits--------------------------------
                                           DAT07              .EQU                7
                                           DAT06              .EQU                6
                                           DAT05              .EQU                5
                                           DAT04              .EQU                4
                                           DAT03              .EQU                3
                                           DAT02              .EQU                2
                                           DAT01              .EQU                1
                                           DAT00              .EQU                0
                                           _DAT07             .EQU                7
                                           _DAT06             .EQU                6
                                           _DAT05             .EQU                5
                                           _DAT04             .EQU                4
                                           _DAT03             .EQU                3
                                           _DAT02             .EQU                2
                                           _DAT01             .EQU                1
                                           _DAT00             .EQU                0
                                           
                                           ;LEDDATA1 Bits--------------------------------
                                           DAT17              .EQU                7
                                           DAT16              .EQU                6
                                           DAT15              .EQU                5
                                           DAT14              .EQU                4
                                           DAT13              .EQU                3
                                           DAT12              .EQU                2
                                           DAT11              .EQU                1
                                           DAT10              .EQU                0
                                           _DAT17             .EQU                7
                                           _DAT16             .EQU                6
                                           _DAT15             .EQU                5
                                           _DAT14             .EQU                4
                                           _DAT13             .EQU                3
                                           _DAT12             .EQU                2
                                           _DAT11             .EQU                1
                                           _DAT10             .EQU                0
                                           
                                           ;LEDDATA2 Bits--------------------------------
                                           DAT27              .EQU                7
                                           DAT26              .EQU                6
                                           DAT25              .EQU                5
                                           DAT24              .EQU                4
                                           DAT23              .EQU                3
                                           DAT22              .EQU                2
                                           DAT21              .EQU                1
                                           DAT20              .EQU                0
                                           _DAT27             .EQU                7
                                           _DAT26             .EQU                6
                                           _DAT25             .EQU                5
                                           _DAT24             .EQU                4
                                           _DAT23             .EQU                3
                                           _DAT22             .EQU                2
                                           _DAT21             .EQU                1
                                           _DAT20             .EQU                0
                                           
                                           ;LEDDATA3 Bits--------------------------------
                                           DAT37              .EQU                7
                                           DAT36              .EQU                6
                                           DAT35              .EQU                5
                                           DAT34              .EQU                4
                                           DAT33              .EQU                3
                                           DAT32              .EQU                2
                                           DAT31              .EQU                1
                                           DAT30              .EQU                0
                                           _DAT37             .EQU                7
                                           _DAT36             .EQU                6
                                           _DAT35             .EQU                5
                                           _DAT34             .EQU                4
                                           _DAT33             .EQU                3
                                           _DAT32             .EQU                2
                                           _DAT31             .EQU                1
                                           _DAT30             .EQU                0
                                           
                                           ;LEDDATA4 Bits--------------------------------
                                           DAT47              .EQU                7
                                           DAT46              .EQU                6
                                           DAT45              .EQU                5
                                           DAT44              .EQU                4
                                           DAT43              .EQU                3
                                           DAT42              .EQU                2
                                           DAT41              .EQU                1
                                           DAT40              .EQU                0
                                           _DAT47             .EQU                7
                                           _DAT46             .EQU                6
                                           _DAT45             .EQU                5
                                           _DAT44             .EQU                4
                                           _DAT43             .EQU                3
                                           _DAT42             .EQU                2
                                           _DAT41             .EQU                1
                                           _DAT40             .EQU                0
                                           
                                           ;LEDDATA5 Bits--------------------------------
                                           DAT57              .EQU                7
                                           DAT56              .EQU                6
                                           DAT55              .EQU                5
                                           DAT54              .EQU                4
                                           DAT53              .EQU                3
                                           DAT52              .EQU                2
                                           DAT51              .EQU                1
                                           DAT50              .EQU                0
                                           _DAT57             .EQU                7
                                           _DAT56             .EQU                6
                                           _DAT55             .EQU                5
                                           _DAT54             .EQU                4
                                           _DAT53             .EQU                3
                                           _DAT52             .EQU                2
                                           _DAT51             .EQU                1
                                           _DAT50             .EQU                0
                                           
                                           ;LEDDATA6 Bits--------------------------------
                                           DAT67              .EQU                7
                                           DAT66              .EQU                6
                                           DAT65              .EQU                5
                                           DAT64              .EQU                4
                                           DAT63              .EQU                3
                                           DAT62              .EQU                2
                                           DAT61              .EQU                1
                                           DAT60              .EQU                0
                                           _DAT67             .EQU                7
                                           _DAT66             .EQU                6
                                           _DAT65             .EQU                5
                                           _DAT64             .EQU                4
                                           _DAT63             .EQU                3
                                           _DAT62             .EQU                2
                                           _DAT61             .EQU                1
                                           _DAT60             .EQU                0
                                           
                                           ;LEDDATA7 Bits--------------------------------
                                           DAT77              .EQU                7
                                           DAT76              .EQU                6
                                           DAT75              .EQU                5
                                           DAT74              .EQU                4
                                           DAT73              .EQU                3
                                           DAT72              .EQU                2
                                           DAT71              .EQU                1
                                           DAT70              .EQU                0
                                           _DAT77             .EQU                7
                                           _DAT76             .EQU                6
                                           _DAT75             .EQU                5
                                           _DAT74             .EQU                4
                                           _DAT73             .EQU                3
                                           _DAT72             .EQU                2
                                           _DAT71             .EQU                1
                                           _DAT70             .EQU                0
                                           
                                           ;C1FILTCTL Bits-------------------------------
                                           INV1               .EQU                7
                                           WEN1               .EQU                6
                                           FEN1               .EQU                5
                                           F1CNT2             .EQU                2
                                           F1CNT1             .EQU                1
                                           F1CNT0             .EQU                0
                                           _INV1              .EQU                7
                                           _WEN1              .EQU                6
                                           _FEN1              .EQU                5
                                           _F1CNT2            .EQU                2
                                           _F1CNT1            .EQU                1
                                           _F1CNT0            .EQU                0
                                           
                                           ;C1FILTPRE Bits-------------------------------
                                           FP17               .EQU                7
                                           FP16               .EQU                6
                                           FP15               .EQU                5
                                           FP14               .EQU                4
                                           FP13               .EQU                3
                                           FP12               .EQU                2
                                           FP11               .EQU                1
                                           FP10               .EQU                0
                                           _FP17              .EQU                7
                                           _FP16              .EQU                6
                                           _FP15              .EQU                5
                                           _FP14              .EQU                4
                                           _FP13              .EQU                3
                                           _FP12              .EQU                2
                                           _FP11              .EQU                1
                                           _FP10              .EQU                0
                                           
                                           ;LEDOMS1 Bits---------------------------------
                                           LEDOM17            .EQU                7
                                           LEDOM16            .EQU                6
                                           LEDOM15            .EQU                5
                                           LEDOM14            .EQU                4
                                           LEDOM13            .EQU                3
                                           LEDOM12            .EQU                2
                                           LEDOM11            .EQU                1
                                           LEDOM10            .EQU                0
                                           _LEDOM17           .EQU                7
                                           _LEDOM16           .EQU                6
                                           _LEDOM15           .EQU                5
                                           _LEDOM14           .EQU                4
                                           _LEDOM13           .EQU                3
                                           _LEDOM12           .EQU                2
                                           _LEDOM11           .EQU                1
                                           _LEDOM10           .EQU                0
                                           
                                           ;LEDODS0 Bits---------------------------------
                                           LEDOD07            .EQU                7
                                           LEDOD06            .EQU                6
                                           LEDOD05            .EQU                5
                                           LEDOD04            .EQU                4
                                           LEDOD03            .EQU                3
                                           LEDOD02            .EQU                2
                                           LEDOD01            .EQU                1
                                           LEDOD00            .EQU                0
                                           _LEDOD07           .EQU                7
                                           _LEDOD06           .EQU                6
                                           _LEDOD05           .EQU                5
                                           _LEDOD04           .EQU                4
                                           _LEDOD03           .EQU                3
                                           _LEDOD02           .EQU                2
                                           _LEDOD01           .EQU                1
                                           _LEDOD00           .EQU                0
                                           
                                           ;LEDOMS0 Bits---------------------------------
                                           LEDOM07            .EQU                7
                                           LEDOM06            .EQU                6
                                           LEDOM05            .EQU                5
                                           LEDOM04            .EQU                4
                                           LEDOM03            .EQU                3
                                           LEDOM02            .EQU                2
                                           LEDOM01            .EQU                1
                                           LEDOM00            .EQU                0
                                           _LEDOM07           .EQU                7
                                           _LEDOM06           .EQU                6
                                           _LEDOM05           .EQU                5
                                           _LEDOM04           .EQU                4
                                           _LEDOM03           .EQU                3
                                           _LEDOM02           .EQU                2
                                           _LEDOM01           .EQU                1
                                           _LEDOM00           .EQU                0
                                           
                                           ;LEDODS1 Bits---------------------------------
                                           LEDOD17            .EQU                7
                                           LEDOD16            .EQU                6
                                           LEDOD15            .EQU                5
                                           LEDOD14            .EQU                4
                                           LEDOD13            .EQU                3
                                           LEDOD12            .EQU                2
                                           LEDOD11            .EQU                1
                                           LEDOD10            .EQU                0
                                           _LEDOD17           .EQU                7
                                           _LEDOD16           .EQU                6
                                           _LEDOD15           .EQU                5
                                           _LEDOD14           .EQU                4
                                           _LEDOD13           .EQU                3
                                           _LEDOD12           .EQU                2
                                           _LEDOD11           .EQU                1
                                           _LEDOD10           .EQU                0
                                           
                                           ;LEDLUM Bits----------------------------------
                                           LEDBR              .EQU                7
                                           FRAMEF             .EQU                3
                                           LUM2               .EQU                2
                                           LUM1               .EQU                1
                                           LUM0               .EQU                0
                                           _LEDBR             .EQU                7
                                           _FRAMEF            .EQU                3
                                           _LUM2              .EQU                2
                                           _LUM1              .EQU                1
                                           _LUM0              .EQU                0
                                           
                                           ;PWM5FC Bits----------------------------------
                                           FCA                .EQU                1
                                           FCB                .EQU                0
                                           _FCA               .EQU                1
                                           _FCB               .EQU                0
                                           
                                           ;T4CTL Bits-----------------------------------
                                           T4REN              .EQU                7
                                           HSPEN              .EQU                6
                                           T4CKS1             .EQU                5
                                           T4CKS0             .EQU                4
                                           LSPEN              .EQU                3
                                           T4CS1              .EQU                2
                                           T4CS0              .EQU                1
                                           T4ON               .EQU                0
                                           _T4REN             .EQU                7
                                           _HSPEN             .EQU                6
                                           _T4CKS1            .EQU                5
                                           _T4CKS0            .EQU                4
                                           _LSPEN             .EQU                3
                                           _T4CS1             .EQU                2
                                           _T4CS0             .EQU                1
                                           _T4ON              .EQU                0
                                            
                                            
                                           ;--------------------------------------------------------
                                           ; external declarations
                                           ;--------------------------------------------------------
                                           	.extern	_PSW_bits
                                           	.extern	_P0_bits
                                           	.extern	_P2_bits
                                           	.extern	_P1_bits
                                           	.extern	_P3_bits
                                           	.extern	_INTCTL_bits
                                           	.extern	_EIF1_bits
                                           	.extern	_EIF2_bits
                                           	.extern	_T1CTL_bits
                                           	.extern	_T2CTL0_bits
                                           	.extern	_PWMCTL_bits
                                           	.extern	_BANK_bits
                                           	.extern	_ADSCANCTL_bits
                                           	.extern	_C1CTL_bits
                                           	.extern	_VDACS_bits
                                           	.extern	_AMPCTL_bits
                                           	.extern	_ANSEH_bits
                                           	.extern	_ADCCTL0_bits
                                           	.extern	_AMPDT_bits
                                           	.extern	_OPTR_bits
                                           	.extern	_IP0_bits
                                           	.extern	_IP1_bits
                                           	.extern	_IP2_bits
                                           	.extern	_TR0_bits
                                           	.extern	_TR2_bits
                                           	.extern	_TR1_bits
                                           	.extern	_OSCSTA_bits
                                           	.extern	_IP3_bits
                                           	.extern	_VRECTL_bits
                                           	.extern	_EIE1_bits
                                           	.extern	_EIE2_bits
                                           	.extern	_PCTL_bits
                                           	.extern	_OSCCTL_bits
                                           	.extern	_ANSEL_bits
                                           	.extern	_PUR0_bits
                                           	.extern	_IOCL_bits
                                           	.extern	_ADCCTL1_bits
                                           	.extern	_P0LR_bits
                                           	.extern	_P2LR_bits
                                           	.extern	_P1LR_bits
                                           	.extern	_P3LR_bits
                                           	.extern	_TR3_bits
                                           	.extern	_EIE3_bits
                                           	.extern	_EIF3_bits
                                           	.extern	_PWM5CTL0_bits
                                           	.extern	_ADCINTCTL_bits
                                           	.extern	_PWM5CTL1_bits
                                           	.extern	_P5ASCTL_bits
                                           	.extern	_PSTRCTL_bits
                                           	.extern	_PUR1_bits
                                           	.extern	_PUR2_bits
                                           	.extern	_INTEDGCTL_bits
                                           	.extern	_VBIASCTL_bits
                                           	.extern	_VBIAS1EN_bits
                                           	.extern	_VBIAS2EN_bits
                                           	.extern	_PWM5OC_bits
                                           	.extern	_T2CTL1_bits
                                           	.extern	_VDAC_bits
                                           	.extern	_PWM5CTL2_bits
                                           	.extern	_PWMPC_bits
                                           	.extern	_RSCTL_bits
                                           	.extern	_BRCTL_bits
                                           	.extern	_TSCTL_bits
                                           	.extern	_SSCICTL0_bits
                                           	.extern	_SSCICTL1_bits
                                           	.extern	_SSCISTA_bits
                                           	.extern	_SSCIMSK_bits
                                           	.extern	_WDTPS_bits
                                           	.extern	_MULCTL_bits
                                           	.extern	_DIVCTL_bits
                                           	.extern	_LEDCTL_bits
                                           	.extern	_LEDPRE_bits
                                           	.extern	_LEDDATA0_bits
                                           	.extern	_LEDDATA1_bits
                                           	.extern	_LEDDATA2_bits
                                           	.extern	_LEDDATA3_bits
                                           	.extern	_LEDDATA4_bits
                                           	.extern	_LEDDATA5_bits
                                           	.extern	_LEDDATA6_bits
                                           	.extern	_LEDDATA7_bits
                                           	.extern	_C1FILTCTL_bits
                                           	.extern	_C1FILTPRE_bits
                                           	.extern	_LEDOMS1_bits
                                           	.extern	_LEDODS0_bits
                                           	.extern	_LEDOMS0_bits
                                           	.extern	_LEDODS1_bits
                                           	.extern	_LEDLUM_bits
                                           	.extern	_PWM5FC_bits
                                           	.extern	_T4CTL_bits
                                           	.extern	_T0
                                           	.extern	_PCL
                                           	.extern	_PSW
                                           	.extern	_P0
                                           	.extern	_P2
                                           	.extern	_P1
                                           	.extern	_P3
                                           	.extern	_PCH
                                           	.extern	_INTCTL
                                           	.extern	_EIF1
                                           	.extern	_EIF2
                                           	.extern	_T1L
                                           	.extern	_T1H
                                           	.extern	_T1CTL
                                           	.extern	_T2L
                                           	.extern	_T2CTL0
                                           	.extern	_PWM1L
                                           	.extern	_PWM1H
                                           	.extern	_PWMCTL
                                           	.extern	_PP1
                                           	.extern	_BANK
                                           	.extern	_ADSCANCTL
                                           	.extern	_C1CTL
                                           	.extern	_VDACS
                                           	.extern	_AMPCTL
                                           	.extern	_ANSEH
                                           	.extern	_ADCDATA0H
                                           	.extern	_ADCCTL0
                                           	.extern	_AMPDT
                                           	.extern	_OPTR
                                           	.extern	_IP0
                                           	.extern	_IP1
                                           	.extern	_IP2
                                           	.extern	_TR0
                                           	.extern	_TR2
                                           	.extern	_TR1
                                           	.extern	_OSCSTA
                                           	.extern	_IP3
                                           	.extern	_VRECAL1
                                           	.extern	_VRECTL
                                           	.extern	_EIE1
                                           	.extern	_EIE2
                                           	.extern	_PCTL
                                           	.extern	_OSCCTL
                                           	.extern	_OSCCAL0
                                           	.extern	_ANSEL
                                           	.extern	_PP2
                                           	.extern	_PWM2L
                                           	.extern	_PWM2H
                                           	.extern	_PUR0
                                           	.extern	_IOCL
                                           	.extern	_OSCCAL1
                                           	.extern	_NVMDATAH
                                           	.extern	_NVMDATAL
                                           	.extern	_NVMADDRH
                                           	.extern	_NVMADDRL
                                           	.extern	_NVMCTL0
                                           	.extern	_NVMCTL1
                                           	.extern	_ADCDATA0L
                                           	.extern	_ADCCTL1
                                           	.extern	_T2CCRH
                                           	.extern	_T2H
                                           	.extern	_PP5H
                                           	.extern	_PWM5H0
                                           	.extern	_PWM5H1
                                           	.extern	_P0LR
                                           	.extern	_P2LR
                                           	.extern	_P1LR
                                           	.extern	_P3LR
                                           	.extern	_TR3
                                           	.extern	_EIE3
                                           	.extern	_EIF3
                                           	.extern	_OSCCAL2
                                           	.extern	_OSCCAL3
                                           	.extern	_ADCDATA1H
                                           	.extern	_ADCDATA1L
                                           	.extern	_PP5L
                                           	.extern	_T2CCRL
                                           	.extern	_PWM5L0
                                           	.extern	_PWM5L1
                                           	.extern	_PWM5CTL0
                                           	.extern	_ADCINTCTL
                                           	.extern	_ADCDATA2H
                                           	.extern	_ADCDATA2L
                                           	.extern	_PWM5CTL1
                                           	.extern	_P5ASCTL
                                           	.extern	_PSTRCTL
                                           	.extern	_ADCDATA3H
                                           	.extern	_PUR1
                                           	.extern	_PUR2
                                           	.extern	_INTEDGCTL
                                           	.extern	_ADCDATA3L
                                           	.extern	_VBIASCTL
                                           	.extern	_VBIAS1EN
                                           	.extern	_VBIAS2EN
                                           	.extern	_PWM5OC
                                           	.extern	_T2CTL1
                                           	.extern	_VDAC
                                           	.extern	_PWM5CTL2
                                           	.extern	_PWMPC
                                           	.extern	_RSCTL
                                           	.extern	_TXSDR
                                           	.extern	_RXSDR
                                           	.extern	_BRCTL
                                           	.extern	_TSCTL
                                           	.extern	_EUBRGL
                                           	.extern	_EUBRGH
                                           	.extern	_SSCICTL0
                                           	.extern	_SSCICTL1
                                           	.extern	_SSCISTA
                                           	.extern	_SSCIBUFR
                                           	.extern	_SSCIMSK
                                           	.extern	_WDTPS
                                           	.extern	_MULAH
                                           	.extern	_MULAL
                                           	.extern	_MULBH
                                           	.extern	_MULBL
                                           	.extern	_MULCTL
                                           	.extern	_MULRES3
                                           	.extern	_MULRES2
                                           	.extern	_MULRES1
                                           	.extern	_MULRES0
                                           	.extern	_DIVCTL
                                           	.extern	_DIVAH
                                           	.extern	_DIVAL
                                           	.extern	_DIVB
                                           	.extern	_DIVQH
                                           	.extern	_DIVQL
                                           	.extern	_DIVR
                                           	.extern	_LEDCTL
                                           	.extern	_LEDPRE
                                           	.extern	_LEDDATA0
                                           	.extern	_LEDDATA1
                                           	.extern	_LEDDATA2
                                           	.extern	_LEDDATA3
                                           	.extern	_LEDDATA4
                                           	.extern	_LEDDATA5
                                           	.extern	_LEDDATA6
                                           	.extern	_LEDDATA7
                                           	.extern	_C1FILTCTL
                                           	.extern	_C1FILTPRE
                                           	.extern	_LEDOMS1
                                           	.extern	_LEDODS0
                                           	.extern	_LEDOMS0
                                           	.extern	_LEDODS1
                                           	.extern	_VRECAL2
                                           	.extern	_VRECAL3
                                           	.extern	_LEDLUM
                                           	.extern	_PWM5FC
                                           	.extern	_T4L
                                           	.extern	_T4H
                                           	.extern	_T4REL
                                           	.extern	_T4REH
                                           	.extern	_T4CTL
                                           	.extern	_RC32KCAL
                                           	.extern	_startup
                                           	.extern	__sdcc_gsinit_startup
                                           ;--------------------------------------------------------
                                           ; global declarations
                                           ;--------------------------------------------------------
                                           	.global	_Delay_ms
                                           	.global	_init_mcu
                                           	.global	_init_pwm
                                           	.global	_T0TimeTurnOnFun
                                           	.global	_pwm_function
                                           	.global	_main
                                           	.global	_int_fun0
                                           	.global	_int_fun1
                                           	.global	_TimeCnt
                                           	.global	_PSTRCTLTEMP
                                           	.global	_PWM5CTL0TEMP
                                           
                                           	.global I0R1
                                           	.global I0PSW
                                           	.global I0PCH
                                           	.global I1R1
                                           	.global I1PSW
                                           	.global I1PCH
                                           	.global STK11
                                           	.global STK10
                                           	.global STK09
                                           	.global STK08
                                           	.global STK07
                                           	.global STK06
                                           	.global STK05
                                           	.global STK04
                                           	.global STK03
                                           	.global STK02
                                           	.global STK01
                                           	.global STK00
                                           
                                           sharebank .udata 0x0080
                                           I0R1		.res 1
                                           I0PSW		.res 1
                                           I0PCH		.res 1
                                           I1R1		.res 1
                                           I1PSW		.res 1
                                           I1PCH		.res 1
                                           STK11	.res 1
                                           	.type STK11, 108
                                           STK10	.res 1
                                           	.type STK10, 108
                                           STK09	.res 1
                                           	.type STK09, 108
                                           STK08	.res 1
                                           	.type STK08, 108
                                           STK07	.res 1
                                           	.type STK07, 108
                                           STK06	.res 1
                                           	.type STK06, 108
                                           STK05	.res 1
                                           	.type STK05, 108
                                           STK04	.res 1
                                           	.type STK04, 108
                                           STK03	.res 1
                                           	.type STK03, 108
                                           STK02	.res 1
                                           	.type STK02, 108
                                           STK01	.res 1
                                           	.type STK01, 108
                                           STK00	.res 1
                                           	.type STK00, 108
                                           
                                           ;--------------------------------------------------------
                                           ; global definitions
                                           ;--------------------------------------------------------
                                           UD_main_0	.udata
                                           _TimeCnt	.res	1
                                           
                                           UD_main_1	.udata
                                           _PSTRCTLTEMP	.res	1
                                           
                                           UD_main_2	.udata
                                           _PWM5CTL0TEMP	.res	1
                                           
                                           ;--------------------------------------------------------
                                           ; absolute symbol definitions
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; compiler-defined variables
                                           ;--------------------------------------------------------
                                           UDL_main_0	.udata
                                           r0x1004	.res	1
                                           UDL_main_1	.udata
                                           r0x1003	.res	1
                                           UDL_main_2	.udata
                                           r0x1005	.res	1
                                           UDL_main_3	.udata
                                           r0x1006	.res	1
                                           ;--------------------------------------------------------
                                           ; initialized data
                                           ;--------------------------------------------------------
                                           ;--------------------------------------------------------
                                           ; overlayable items in internal ram 
                                           ;--------------------------------------------------------
                                           ;	.udata_ovr
                                           ;--------------------------------------------------------
                                           ; reset vector 
                                           ;--------------------------------------------------------
                                           STARTUP	.code 0x0000
000000   0000     NOP                      	NOP
000001   e000     MOVP	0                   	PAGESEL	init_imp
000002   c0c9     JMP	#0xc9                	JMP		init_imp
                                           
                                           	.global	init_imp
                                           INIT_IMP	.code
                                           init_imp
0000c9   e000     MOVP	0                   	PAGESEL	_startup
0000ca   d00f     CALL	#0xf                	CALL	_startup
0000cb   e000     MOVP	0                   	PAGESEL	__sdcc_gsinit_startup
0000cc   d0cf     CALL	#0xcf               	CALL	__sdcc_gsinit_startup
0000cd   e000     MOVP	0                   	PAGESEL	_main
0000ce   c068     JMP	#0x68                	JMP		_main
                                           ;--------------------------------------------------------
                                           ; interrupt and initialization code
                                           ;--------------------------------------------------------
                                           interrupt_0x04	.code	0x4
000004   f8c2     MOV	R2, R0               	MOV		R2,R0
000005   5617     MOV	R3, 0x17             	MOV		R3,BANK
000006   5003     MOV	R0, 0x3              	MOV		R0,PSW
000007   e100     MOVB	0                   	BANKSEL	I0PSW
000008   5181     MOV	0x81, R0             	MOV		I0PSW,R0
000009   500a     MOV	R0, 0xa              	MOV		R0,PCH
00000a   e100     MOVB	0                   	BANKSEL	I0PCH
00000b   5182     MOV	0x82, R0             	MOV		I0PCH,R0
00000c   5380     MOV	0x80, R1             	MOV		I0R1,R1
00000d   e000     MOVP	0                   	PAGESEL	interrupt_service_routine_0x04
00000e   c0a3     JMP	#0xa3                	JMP		interrupt_service_routine_0x04
                                           
                                           
                                           
                                           func._int_fun0	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun0	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun0	;Function start
                                           ; 0 exit points
                                           ;	op : GET_VALUE_AT_ADDRESS
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x04
                                           ;	.line	157; "../main.c"	if(T0IF)				//¶¨Ê±ÖÐ¶Ï   1ms
0000a3   e100     MOVB	0                   	BANKSEL	_INTCTL_bits
0000a4   7a0b     JB	0xb, 2                	JB	_INTCTL_bits, 2
0000a5   c0aa     JMP	#0xaa                	JMP	_00034_DS_
                                           ;	op : =
                                           ;	.line	159; "../main.c"	T0IF = 0;
                                           	BANKSEL	_INTCTL_bits
0000a6   620b     CLR	0xb, 2               	CLR	_INTCTL_bits, 2
                                           ;	op : =
                                           ;	.line	160; "../main.c"	T0=	240;
0000a7   98f0     MOV	R0, #0xf0            	MOV	R0,# 0xf0
                                           	BANKSEL	_T0
0000a8   5101     MOV	0x1, R0              	MOV	_T0, R0
                                           ;	op : +
                                           ;	.line	161; "../main.c"	TimeCnt++;
                                           	BANKSEL	_TimeCnt
0000a9   0b92     INC	0x92                 	INC	_TimeCnt
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00034_DS_
                                           	BANKSEL	I0R1
0000aa   5280     MOV	R1, 0x80             	MOV	R1, I0R1
                                           	BANKSEL	I0PCH
0000ab   5082     MOV	R0, 0x82             	MOV	R0, I0PCH
0000ac   510a     MOV	0xa, R0              	MOV	PCH, R0
                                           	BANKSEL	I0PSW
0000ad   5081     MOV	R0, 0x81             	MOV	R0, I0PSW
0000ae   5103     MOV	0x3, R0              	MOV	PSW, R0
0000af   5717     MOV	0x17, R3             	MOV	BANK, R3
0000b0   f8d0     MOV	R0, R2               	MOV	R0, R2
0000b1   0009     IRET                     	IRET	
                                           
                                           
                                           
                                           func._int_fun1	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = I
                                           ;***
                                           ;entry:  _int_fun1	;Function start
                                           ; 0 exit points
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _int_fun1	;Function start
                                           ; 0 exit points
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           ; R3 resprent for wsave,R4 resprent for ssave, R5 resprent for psave
                                           interrupt_service_routine_0x14
                                           _00037_DS_
                                           ;	.line	170; "../main.c"	}
                                           	IRET	
                                           
                                           
                                           
                                           func._main	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = M
                                           ;***
                                           ;entry:  _main	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;functions called:
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _T0TimeTurnOnFun
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;   _init_mcu
                                           ;   _init_pwm
                                           ;   _T0TimeTurnOnFun
                                           ;   _Delay_ms
                                           ;   _pwm_function
                                           ;1 compiler assigned register :
                                           ;   STK00
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _main	;Function start
                                           ; 2 exit points
                                           ;	op : CALL
                                           ;	.line	143; "../main.c"	init_mcu();
000068   e000     MOVP	0                   	PAGESEL	_init_mcu
000069   d092     CALL	#0x92               	CALL	_init_mcu
00006a   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	144; "../main.c"	init_pwm();
00006b   e000     MOVP	0                   	PAGESEL	_init_pwm
00006c   d07d     CALL	#0x7d               	CALL	_init_pwm
00006d   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : CALL
                                           ;	.line	145; "../main.c"	T0TimeTurnOnFun();
00006e   e000     MOVP	0                   	PAGESEL	_T0TimeTurnOnFun
00006f   d0be     CALL	#0xbe               	CALL	_T0TimeTurnOnFun
000070   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : SEND
                                           ;	op : CALL
                                           ;	.line	146; "../main.c"	Delay_ms(10);
000071   980a     MOV	R0, #0xa             	MOV	R0,# 0x0a
000072   e100     MOVB	0                   	BANKSEL	STK00
000073   5191     MOV	0x91, R0             	MOV	STK00, R0
000074   9800     MOV	R0, #0               	MOV	R0,# 0x00
000075   e000     MOVP	0                   	PAGESEL	_Delay_ms
000076   d033     CALL	#0x33               	CALL	_Delay_ms
000077   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : LABEL
                                           ;	op : CALL
                                           _00027_DS_
                                           ;	.line	150; "../main.c"	pwm_function();
000078   e000     MOVP	0                   	PAGESEL	_pwm_function
000079   d04f     CALL	#0x4f               	CALL	_pwm_function
00007a   e000     MOVP	0                   	PAGESEL	$
                                           ;	op : GOTO
00007b   c078     JMP	#0x78                	JMP	_00027_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
00007c   0008     CRET                     	CRET	
                                           ; exit point of _main
                                           
                                           
                                           
                                           func._pwm_function	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _pwm_function	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _pwm_function	;Function start
                                           ; 2 exit points
                                           ;	op : >
                                           ;swapping arguments (AOP_TYPEs 1/3)
                                           ;unsigned compare: left >= lit(0x1A=26), size=1
                                           ;	.line	117; "../main.c"	if(TimeCnt>25)			//25ms±ä»¯Ò»´Î    ÖÜÆÚÎª50HZ
00004f   981a     MOV	R0, #0x1a            	MOV	R0,# 0x1a
000050   e100     MOVB	0                   	BANKSEL	_TimeCnt
000051   3892     SUB	R0, 0x92             	SUB	R0, _TimeCnt
                                           ;comparing bytes at offset 0
000052   7803     JB	0x3, 0                	JB	PSW, 0
000053   c067     JMP	#0x67                	JMP	_00022_DS_
                                           ;	op : =
                                           ;	.line	119; "../main.c"	TimeCnt = 0 ;
                                           	BANKSEL	_TimeCnt
000054   0392     CLR	0x92                 	CLR	_TimeCnt
                                           ;	op : =
                                           ;	.line	120; "../main.c"	PSTRCTLTEMP = PSTRCTL;
                                           	BANKSEL	_PSTRCTL
000055   0e5d     MOVZ	R0, 0x5d            	MOVZ	R0, _PSTRCTL
                                           	BANKSEL	_PSTRCTLTEMP
000056   5193     MOV	0x93, R0             	MOV	_PSTRCTLTEMP, R0
                                           ;	op : ^
                                           ;	.line	121; "../main.c"	PSTRCTLTEMP ^= 0b00001111;			//È¡·´È«ÇÅÄ£Ê½£¬ÕýÏòºÍ·´ÏòÇÐ»»
000057   980f     MOV	R0, #0xf             	MOV	R0,# 0x0f
                                           	BANKSEL	_PSTRCTLTEMP
000058   1993     XOR	0x93, R0             	XOR	_PSTRCTLTEMP, R0
                                           ;	op : =
                                           ;	.line	122; "../main.c"	PWM5CTL0TEMP = PWM5CTL0;
                                           	BANKSEL	_PWM5CTL0
000059   0e57     MOVZ	R0, 0x57            	MOVZ	R0, _PWM5CTL0
                                           	BANKSEL	_PWM5CTL0TEMP
00005a   5194     MOV	0x94, R0             	MOV	_PWM5CTL0TEMP, R0
                                           ;	op : ^
                                           ;	.line	123; "../main.c"	PWM5CTL0TEMP ^= 0b10000000;
00005b   9880     MOV	R0, #0x80            	MOV	R0,# 0x80
                                           	BANKSEL	_PWM5CTL0TEMP
00005c   1994     XOR	0x94, R0             	XOR	_PWM5CTL0TEMP, R0
                                           ;	op : =
                                           ;	.line	124; "../main.c"	PSTRCTL	 = 0;
                                           	BANKSEL	_PSTRCTL
00005d   035d     CLR	0x5d                 	CLR	_PSTRCTL
                                           ;	op : =
                                           ;	.line	125; "../main.c"	PWM5CTL0    =0;
                                           	BANKSEL	_PWM5CTL0
00005e   0357     CLR	0x57                 	CLR	_PWM5CTL0
                                           ;	op : INLINEASM
00005f   0000     NOP                      	NOP 
                                           ;	op : INLINEASM
000060   0000     NOP                      	NOP 
                                           ;	op : INLINEASM
000061   0000     NOP                      	NOP 
                                           ;	op : INLINEASM
000062   0000     NOP                      	NOP 
                                           ;	op : =
                                           ;	.line	130; "../main.c"	PSTRCTL = PSTRCTLTEMP;
                                           	BANKSEL	_PSTRCTLTEMP
000063   0e93     MOVZ	R0, 0x93            	MOVZ	R0, _PSTRCTLTEMP
                                           	BANKSEL	_PSTRCTL
000064   515d     MOV	0x5d, R0             	MOV	_PSTRCTL, R0
                                           ;	op : =
                                           ;	.line	131; "../main.c"	PWM5CTL0 = PWM5CTL0TEMP;
                                           	BANKSEL	_PWM5CTL0TEMP
000065   0e94     MOVZ	R0, 0x94            	MOVZ	R0, _PWM5CTL0TEMP
                                           	BANKSEL	_PWM5CTL0
000066   5157     MOV	0x57, R0             	MOV	_PWM5CTL0, R0
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00022_DS_
000067   0008     CRET                     	CRET	
                                           ; exit point of _pwm_function
                                           
                                           
                                           
                                           func._T0TimeTurnOnFun	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _T0TimeTurnOnFun	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _T0TimeTurnOnFun	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	99; "../main.c"	T0CS = 0;
0000be   e100     MOVB	0                   	BANKSEL	_OPTR_bits
0000bf   6521     CLR	0x21, 5              	CLR	_OPTR_bits, 5
                                           ;	op : =
                                           ;	.line	100; "../main.c"	PSA = 0;
                                           	BANKSEL	_OPTR_bits
0000c0   6321     CLR	0x21, 3              	CLR	_OPTR_bits, 3
                                           ;	op : =
                                           ;	.line	101; "../main.c"	PS2 = 1;
                                           	BANKSEL	_OPTR_bits
0000c1   6a21     SET	0x21, 2              	SET	_OPTR_bits, 2
                                           ;	op : =
                                           ;	.line	102; "../main.c"	PS1 = 1;
                                           	BANKSEL	_OPTR_bits
0000c2   6921     SET	0x21, 1              	SET	_OPTR_bits, 1
                                           ;	op : =
                                           ;	.line	103; "../main.c"	PS0 = 1;
                                           	BANKSEL	_OPTR_bits
0000c3   6821     SET	0x21, 0              	SET	_OPTR_bits, 0
                                           ;	op : =
                                           ;	.line	104; "../main.c"	T0=	240;
0000c4   98f0     MOV	R0, #0xf0            	MOV	R0,# 0xf0
                                           	BANKSEL	_T0
0000c5   5101     MOV	0x1, R0              	MOV	_T0, R0
                                           ;	op : =
                                           ;	.line	105; "../main.c"	T0IE = 1;
                                           	BANKSEL	_INTCTL_bits
0000c6   6d0b     SET	0xb, 5               	SET	_INTCTL_bits, 5
                                           ;	op : =
                                           ;	.line	106; "../main.c"	AIE = 1;
                                           	BANKSEL	_INTCTL_bits
0000c7   6f0b     SET	0xb, 7               	SET	_INTCTL_bits, 7
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
0000c8   0008     CRET                     	CRET	
                                           ; exit point of _T0TimeTurnOnFun
                                           
                                           
                                           
                                           func._init_pwm	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_pwm	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_pwm	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	76; "../main.c"	P5ASCTL		= 0b00000000;			//ÉèÖÃPWM5¹Ø±ÕÊ±ºòPWM¿ÚÊä³öµçÆ½		ÕâÀïÎªÄ¬ÈÏÉèÖÃ£¬¹Ø±ÕPWMÊ±ºò¶¼Êä³ö0
00007d   e100     MOVB	0                   	BANKSEL	_P5ASCTL
00007e   035c     CLR	0x5c                 	CLR	_P5ASCTL
                                           ;	op : =
                                           ;	.line	77; "../main.c"	PWM5CTL2	= 0b00000001;			//PWMÖÜÆÚ×Ô¶¯Ìî³ä¸üÐÂ
00007f   9801     MOV	R0, #0x1             	MOV	R0,# 0x01
000080   e101     MOVB	0x1                 	BANKSEL	_PWM5CTL2
000081   511c     MOV	0x1c, R0             	MOV	_PWM5CTL2, R0
                                           ;	op : =
                                           ;	.line	78; "../main.c"	PWM5CTL0	= 0b01001100; 			//³õÊ¼»¯ÏÈÏÈÕýÏòÈ«ÇÅÊä³ö
000082   984c     MOV	R0, #0x4c            	MOV	R0,# 0x4c
000083   e100     MOVB	0                   	BANKSEL	_PWM5CTL0
000084   5157     MOV	0x57, R0             	MOV	_PWM5CTL0, R0
                                           ;	op : =
                                           ;	.line	79; "../main.c"	PSTRCTL		= 0b00011001;			//PWMµ¥ÏîÊä³öÊ±ºò£¬ºÍÈ«ÇÅÊä³öÊ±ºò£¬PWMÐÅºÅ¿ØÖÆÊÇ·ñÊä³öµ½ÏàÓ¦IOÉÏ£¬ PSTRCTL£¨3:0£©·Ö±ðÎªP5D P5C P5B P5A
000085   9819     MOV	R0, #0x19            	MOV	R0,# 0x19
                                           	BANKSEL	_PSTRCTL
000086   515d     MOV	0x5d, R0             	MOV	_PSTRCTL, R0
                                           ;	op : =
                                           ;	.line	80; "../main.c"	PP5H		= 0;					//¸ßÎ»
                                           	BANKSEL	_PP5H
000087   0342     CLR	0x42                 	CLR	_PP5H
                                           ;	op : =
                                           ;	.line	81; "../main.c"	PP5L		= 40;					//µÍÎ»			ÉèÖÃPWMÖÜÆÚ  ÖÜÆÚÊ±¼äÎªPP5+1½øÐÐ¼ÆËã
000088   9828     MOV	R0, #0x28            	MOV	R0,# 0x28
                                           	BANKSEL	_PP5L
000089   5152     MOV	0x52, R0             	MOV	_PP5L, R0
                                           ;	op : =
                                           ;	.line	82; "../main.c"	PWM5L1		= 0;					//¸ßÎ»
                                           	BANKSEL	_PWM5L1
00008a   0356     CLR	0x56                 	CLR	_PWM5L1
                                           ;	op : =
                                           ;	.line	83; "../main.c"	PWM5L0		= 20;					//  µØÎ»    ÉèÖÃPWMÕ¼¿Õ±È
00008b   9814     MOV	R0, #0x14            	MOV	R0,# 0x14
                                           	BANKSEL	_PWM5L0
00008c   5155     MOV	0x55, R0             	MOV	_PWM5L0, R0
                                           ;	op : =
                                           ;	.line	84; "../main.c"	T2H			= 0;
                                           	BANKSEL	_T2H
00008d   0341     CLR	0x41                 	CLR	_T2H
                                           ;	op : =
                                           ;	.line	85; "../main.c"	T2L			= 0;					//PWMÊ±ÖÓÔ´ T2Ïà¹ØÉèÖÃ
                                           	BANKSEL	_T2L
00008e   0311     CLR	0x11                 	CLR	_T2L
                                           ;	op : =
                                           ;	.line	86; "../main.c"	T2CTL0		= 0b00000000;
                                           	BANKSEL	_T2CTL0
00008f   0312     CLR	0x12                 	CLR	_T2CTL0
                                           ;	op : =
                                           ;	.line	87; "../main.c"	T2ON		= 1;
                                           	BANKSEL	_T2CTL0_bits
000090   6a12     SET	0x12, 2              	SET	_T2CTL0_bits, 2
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
000091   0008     CRET                     	CRET	
                                           ; exit point of _init_pwm
                                           
                                           
                                           
                                           func._init_mcu	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _init_mcu	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _init_mcu	;Function start
                                           ; 2 exit points
                                           ;	op : =
                                           ;	.line	49; "../main.c"	OSCCTL = 0x70;          //ÉèÖÃÎª16M
000092   9870     MOV	R0, #0x70            	MOV	R0,# 0x70
000093   e100     MOVB	0                   	BANKSEL	_OSCCTL
000094   512f     MOV	0x2f, R0             	MOV	_OSCCTL, R0
                                           ;	op : =
                                           ;	.line	52; "../main.c"	TR0 = 0x08;				//ÉèÖÃP03¶Ë¿ÚÎªÊäÈë£¬P0ÆäËûI/O¿ÚÎªÊä³ö
000095   9808     MOV	R0, #0x8             	MOV	R0,# 0x08
                                           	BANKSEL	_TR0
000096   5125     MOV	0x25, R0             	MOV	_TR0, R0
                                           ;	op : =
                                           ;	.line	53; "../main.c"	TR1 = 0x00;				//ÉèÖÃP1¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR1
000097   0327     CLR	0x27                 	CLR	_TR1
                                           ;	op : =
                                           ;	.line	54; "../main.c"	TR2 = 0x00;				//ÉèÖÃP2¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR2
000098   0326     CLR	0x26                 	CLR	_TR2
                                           ;	op : =
                                           ;	.line	55; "../main.c"	TR3 = 0x00;				//ÉèÖÃP3¶Ë¿ÚÎªÊä³ö
                                           	BANKSEL	_TR3
000099   0349     CLR	0x49                 	CLR	_TR3
                                           ;	op : =
                                           ;	.line	56; "../main.c"	P0 = 0;
                                           	BANKSEL	_P0
00009a   0305     CLR	0x5                  	CLR	_P0
                                           ;	op : =
                                           ;	.line	57; "../main.c"	P1 = 0;
                                           	BANKSEL	_P1
00009b   0307     CLR	0x7                  	CLR	_P1
                                           ;	op : =
                                           ;	.line	58; "../main.c"	P2 = 0;
                                           	BANKSEL	_P2
00009c   0306     CLR	0x6                  	CLR	_P2
                                           ;	op : =
                                           ;	.line	59; "../main.c"	P3 = 0;
                                           	BANKSEL	_P3
00009d   0308     CLR	0x8                  	CLR	_P3
                                           ;	op : =
                                           ;	.line	60; "../main.c"	P0LR = 0;				//P0¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P0LR
00009e   0345     CLR	0x45                 	CLR	_P0LR
                                           ;	op : =
                                           ;	.line	61; "../main.c"	P1LR = 0;				//P1¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P1LR
00009f   0347     CLR	0x47                 	CLR	_P1LR
                                           ;	op : =
                                           ;	.line	62; "../main.c"	P2LR = 0;				//P2¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P2LR
0000a0   0346     CLR	0x46                 	CLR	_P2LR
                                           ;	op : =
                                           ;	.line	63; "../main.c"	P3LR = 0;				//P3¿ÚÊä³öµÍµçÆ½
                                           	BANKSEL	_P3LR
0000a1   0348     CLR	0x48                 	CLR	_P3LR
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
0000a2   0008     CRET                     	CRET	
                                           ; exit point of _init_mcu
                                           
                                           
                                           
                                           func._Delay_ms	.code
                                           ;***
                                           ;  PostBlock Stats: dbName = C
                                           ;***
                                           ;entry:  _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;has an exit
                                           ;5 compiler assigned registers:
                                           ;   r0x1003
                                           ;   STK00
                                           ;   r0x1004
                                           ;   r0x1005
                                           ;   r0x1006
                                           ;; Starting PostCode block
                                           ;	op : LABEL
                                           ;	op : FUNCTION
                                           _Delay_ms	;Function start
                                           ; 2 exit points
                                           ;	op : RECEIVE
                                           ;	.line	30; "../main.c"	void Delay_ms(uint ms_data)
000033   e100     MOVB	0                   	BANKSEL	r0x1003
000034   5196     MOV	0x96, R0             	MOV	r0x1003, R0
                                           	BANKSEL	STK00
000035   0e91     MOVZ	R0, 0x91            	MOVZ	R0, STK00
                                           	BANKSEL	r0x1004
000036   5195     MOV	0x95, R0             	MOV	r0x1004, R0
                                           ;	op : =
                                           ;	op : LABEL
                                           ;	op : =
                                           _00004_DS_
                                           ;	.line	33; "../main.c"	while(ms_data--)
                                           	BANKSEL	r0x1004
000037   0e95     MOVZ	R0, 0x95            	MOVZ	R0, r0x1004
                                           	BANKSEL	r0x1005
000038   5197     MOV	0x97, R0             	MOV	r0x1005, R0
                                           	BANKSEL	r0x1003
000039   0e96     MOVZ	R0, 0x96            	MOVZ	R0, r0x1003
                                           	BANKSEL	r0x1006
00003a   5198     MOV	0x98, R0             	MOV	r0x1006, R0
                                           ;	op : -
00003b   98ff     MOV	R0, #0xff            	MOV	R0,# 0xff
                                           	BANKSEL	r0x1004
00003c   2195     ADD	0x95, R0             	ADD	r0x1004, R0
00003d   7003     JNB	0x3, 0               	JNB	PSW, 0
00003e   c040     JMP	#0x40                	JMP	_00039_DS_
                                           	BANKSEL	r0x1003
00003f   0796     DEC	0x96                 	DEC	r0x1003
                                           ;	op : IFX
                                           _00039_DS_
                                           	BANKSEL	r0x1005
000040   0e97     MOVZ	R0, 0x97            	MOVZ	R0, r0x1005
                                           	BANKSEL	r0x1006
000041   3098     ORL	R0, 0x98             	ORL	R0, r0x1006
000042   7203     JNB	0x3, 2               	JNB	PSW, 2
000043   c04e     JMP	#0x4e                	JMP	_00007_DS_
                                           ;	op : =
                                           ;	.line	36; "../main.c"	while(i--);
000044   987c     MOV	R0, #0x7c            	MOV	R0,# 0x7c
                                           	BANKSEL	r0x1005
000045   5197     MOV	0x97, R0             	MOV	r0x1005, R0
                                           ;	op : LABEL
                                           ;	op : =
                                           _00001_DS_
                                           	BANKSEL	r0x1005
000046   0e97     MOVZ	R0, 0x97            	MOVZ	R0, r0x1005
                                           	BANKSEL	r0x1006
000047   5198     MOV	0x98, R0             	MOV	r0x1006, R0
                                           ;	op : -
                                           	BANKSEL	r0x1005
000048   0797     DEC	0x97                 	DEC	r0x1005
                                           ;	op : IFX
000049   9800     MOV	R0, #0               	MOV	R0,# 0x00
                                           	BANKSEL	r0x1006
00004a   3098     ORL	R0, 0x98             	ORL	R0, r0x1006
00004b   7203     JNB	0x3, 2               	JNB	PSW, 2
00004c   c037     JMP	#0x37                	JMP	_00004_DS_
                                           ;	op : GOTO
00004d   c046     JMP	#0x46                	JMP	_00001_DS_
                                           ;	op : LABEL
                                           ;	op : ENDFUNCTION
                                           _00007_DS_
00004e   0008     CRET                     	CRET	
                                           ; exit point of _Delay_ms
                                           
                                           
                                           ;	code size estimation:
                                           ;	  126+   71 =   197 instructions (  536 byte)
                                           
                                           
                                           	.end
                                           .config
002007   3f94     SUB	0x94, R3            
002008   ffff     NOPZ                    
                                           func.__sdcc_gsinit_startup
0000cf   e000     MOVP	0                  
0000d0   d0b2     CALL	#0xb2              
0000d1   e000     MOVP	0                  
0000d2   0008     CRET                    
                                           .code
00000f   e01f     MOVP	0x1f               
000010   e100     MOVB	0                  
000011   dfff     CALL	#0xfff             
000012   5130     MOV	0x30, R0            
000013   ffff     NOPZ                    
000014   ffff     NOPZ                    
000015   dffe     CALL	#0xffe             
000016   5137     MOV	0x37, R0            
000017   ffff     NOPZ                    
000018   ffff     NOPZ                    
000019   dffd     CALL	#0xffd             
00001a   514c     MOV	0x4c, R0            
00001b   ffff     NOPZ                    
00001c   ffff     NOPZ                    
00001d   dffc     CALL	#0xffc             
00001e   514d     MOV	0x4d, R0            
00001f   ffff     NOPZ                    
000020   ffff     NOPZ                    
000021   dffb     CALL	#0xffb             
000022   512a     MOV	0x2a, R0            
000023   ffff     NOPZ                    
000024   ffff     NOPZ                    
000025   e101     MOVB	0x1                
000026   dffa     CALL	#0xffa             
000027   5159     MOV	0x59, R0            
000028   ffff     NOPZ                    
000029   ffff     NOPZ                    
00002a   dff9     CALL	#0xff9             
00002b   515a     MOV	0x5a, R0            
00002c   ffff     NOPZ                    
00002d   ffff     NOPZ                    
00002e   dff8     CALL	#0xff8             
00002f   5165     MOV	0x65, R0            
000030   ffff     NOPZ                    
000031   ffff     NOPZ                    
000032   0008     CRET                    
                                           .cinit
0000b2   e100     MOVB	0                  
0000b3   9880     MOV	R0, #0x80           
0000b4   9919     MOV	R1, #0x19           
0000b5   e000     MOVP	0                  
0000b6   d0b8     CALL	#0xb8              
0000b7   0008     CRET                    
0000b8   020a     CLR	R2                  
0000b9   f750     ST	[R0], R2             
0000ba   ff10     INC	R0                  
0000bb   ff59     DECJZ	R1                
0000bc   c0b9     JMP	#0xb9               
0000bd   0008     CRET                    
